Sender : superbill999@yahoo.com
SpeedFan version : SpeedFan 4.32
Motherboard model : ????? - DELL INSPIRON 2200

*****************************

BIOS CopyRight : DELL   - 27d50413Phoenix ROM BIOS PLUS Version 1.10 A04
BIOS Date : 04/19/05
BIOS Extended Info : 
BIOS Name : AT/AT COMPATIBLE

Windows NT Uniprocessor Free version 5.1.2600

1 processor(s)
Intel Corporation Intel(R) Pentium(R) M processor 1.60GHz family 6 model 13 stepping 6 brand 22 598 MHz (64.0 Kb level 1 - 0 bytes level 2 - 0 bytes level 3)
Running at 598 MHz
I Agree to receive beta versions : ON

*****************************

DELL on ISA at $3E8 CPU : 38.0   min=35.0   max=59.0   mean=38.0
DELL on ISA at $3E8 GPU : 36.0   min=28.0   max=40.0   mean=36.0
DELL on ISA at $3E8 DIMM : 40.0   min=28.0   max=41.0   mean=40.4
DELL on ISA at $3E8 Fan1 : 0   min=0   max=3152   mean=0
DELL on ISA at $3E8 Fan2 : 922   min=922   max=922   mean=922
DELL on ISA at $3E8 Fan3 : 922   min=922   max=922   mean=922
DELL on ISA at $3E8 Pwm1 : 0%   min=0%   max=0%   mean=0%
HD0 (60.0GB) on SMART at $0 HD0 : 40.0   min=27.0   max=42.0   mean=39.0
Hitachi HTS541060G9AT00 (drive 0) : fitness=95%   performance=95%
ACPI on ISA at $0 Temp1 : 37.5   min=37.5   max=37.5   mean=37.5

*****************************

HD0 --> active=ON  chip=1  index=1 wanted=40  warning=50  offset=0  InTray=ON Used pwms=
Temp1 --> active=ON  chip=2  index=1 wanted=40  warning=50  offset=0  InTray=OFF Used pwms=1 
DIMM --> active=ON  chip=0  index=3 wanted=40  warning=50  offset=0  InTray=OFF Used pwms=1 
CPU --> active=ON  chip=0  index=1 wanted=40  warning=50  offset=0  InTray=ON Used pwms=1 
GPU --> active=ON  chip=0  index=2 wanted=40  warning=50  offset=0  InTray=OFF Used pwms=1 
Fan1 --> active=ON  chip=0  index=1
Fan2 --> active=ON  chip=0  index=2
Fan3 --> active=ON  chip=0  index=3
Speed01 --> active=ON  chip=0  index=1  min=0  max=100  variate=OFF
Set Fans to 100% on exit : OFF
Debug Mode : ON
Use ISA : ON
Use SMB : ON
Scan PCI : ON
Scan SMB : ON
Slow SMB detection : OFF
Detect SuperIO : ON
ASUS Card Detect : ON
DELL Support : ON
Command line : "C:\Program Files\SpeedFan\speedfan.exe" 
Delta Fan Speed : 10

*****************************

Chipset : Intel 82801FB ICH6
SMBus Base Address : $10C0
SMBus Revision : 00000003
SMBus I/O Enabled : ON

*****************************

Bus : 00 Device: 00 Function : 00 --> 25908086 Vendor : 8086 Device : 2590 (rev 03) - <Unknown device>
00: 8086 2590 0006 2090 0003 0600 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 1028 01A4 0000 0000 00E0 0000 0000 0000 0000 0000
40: 5000 F000 0000 F000 0000 E000 4000 F000 0000 0030 0019 B800 0000 0000 0000 0000
60: 6001 F000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0000 0000 0000 0000 0000 0000 0000 0000 1110 0011 0000 0000 0000 0000 0A20 00F8
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0019 0000
E0: 0009 3109 E823 E28B 000A 0000 0000 0000 0000 0000 0000 0000 0000 0005 0010 0000

Bus : 00 Device: 02 Function : 00 --> 25928086 Vendor : 8086 Device : 2592 (rev 03) - <Unknown device>
00: 8086 2592 0007 0090 0003 0300 0000 0080 0000 DFF0 EC39 0000 0008 C000 0000 DFEC
20: 0000 0000 0000 0000 0000 0000 1028 01A4 0000 0000 00D0 0000 0000 0000 0110 0000
40: 0000 0000 00E0 0000 0009 3109 E823 E28B 000A 0030 0019 B800 0000 0000 0000 1F80
60: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0001 0022 0000 0000 0000 0000 0000 0000
E0: 0528 0000 0000 0000 0000 0000 0000 0000 0000 3464 0000 0000 0000 0005 0000 0000

Bus : 00 Device: 02 Function : 01 --> 27928086 Vendor : 8086 Device : 2792 (rev 03) - <Unknown device>
00: 8086 2792 0007 0090 0003 0380 0000 0080 0000 DFF8 0000 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 1028 01A4 0000 0000 00D0 0000 0000 0000 0000 0000
40: 0000 0000 00E0 0000 0009 3109 E823 E28B 000A 0030 0019 B800 0000 0000 0000 1F80
60: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0001 0022 0000 0000 0000 0000 0000 0000
E0: 0528 0000 0000 0000 0000 0000 0000 0000 0000 3464 0000 0000 0000 0005 0000 0000

Bus : 00 Device: 29 Function : 00 --> 26588086 Vendor : 8086 Device : 2658 (rev 03) - Intel Corporation 82801FB/FR/FW/FRW USB UHCI Controller #1
00: 8086 2658 0005 0280 0003 0C03 0000 0080 0000 0000 0000 0000 0000 0000 0000 0000
20: BF81 0000 0000 0000 0000 0000 1028 01A4 0000 0000 0000 0000 0000 0000 0110 0000
40: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
60: 0010 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 2F00 0000 0003 0000 0000 0001 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0F80 0004 0000 0000

Bus : 00 Device: 29 Function : 01 --> 26598086 Vendor : 8086 Device : 2659 (rev 03) - Intel Corporation 82801FB/FR/FW/FRW USB UHCI Controller #2
00: 8086 2659 0005 0280 0003 0C03 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
20: BF61 0000 0000 0000 0000 0000 1028 01A4 0000 0000 0000 0000 0000 0000 0211 0000
40: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
60: 0010 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 2F00 0000 0003 0000 0000 0001 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0F80 0004 0000 0000

Bus : 00 Device: 29 Function : 02 --> 265A8086 Vendor : 8086 Device : 265A (rev 03) - Intel Corporation 82801FB/FR/FW/FRW USB UHCI Controller #3
00: 8086 265A 0005 0280 0003 0C03 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
20: BF41 0000 0000 0000 0000 0000 1028 01A4 0000 0000 0000 0000 0000 0000 0312 0000
40: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
60: 0010 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 2F00 0000 0003 0000 0000 0001 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0F80 0004 0000 0000

Bus : 00 Device: 29 Function : 03 --> 265B8086 Vendor : 8086 Device : 265B (rev 03) - Intel Corporation 82801FB/FR/FW/FRW USB UHCI Controller #4
00: 8086 265B 0005 0280 0003 0C03 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
20: BF21 0000 0000 0000 0000 0000 1028 01A4 0000 0000 0000 0000 0000 0000 0413 0000
40: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
60: 0010 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 2F00 0000 0000 0000 0000 0001 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0F80 0004 0000 0000

Bus : 00 Device: 29 Function : 07 --> 265C8086 Vendor : 8086 Device : 265C (rev 03) - Intel Corporation 82801FB/FR/FW/FRW USB 2.0 EHCI Controller
00: 8086 265C 0106 0290 2003 0C03 0000 0000 0800 FFA8 0000 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 1028 01A4 0000 0000 0050 0000 0000 0000 0110 0000
40: 0000 0000 0000 0000 0000 0000 0000 0000 5801 C9C2 0000 0000 000A 20A0 0000 0000
60: 2020 01FF 0000 0000 0001 0000 0000 C000 0000 3FFF 0000 0000 0000 0000 0000 0000
80: 0000 0000 0001 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 AA00 00FF 5555 00FF 0020 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 8000 0900 8C88 0040 0F80 0004 1700 0000

Bus : 00 Device: 30 Function : 00 --> 24488086 Vendor : 8086 Device : 2448 (rev D3) - Intel Corporation 82801BAM/CAM/DBM Hub Interface to PCI Bridge
00: 8086 2448 0107 0010 01D3 0604 0000 0081 0000 0000 0000 0000 0200 2003 D0D0 2280
20: DFD0 DFD0 FFF1 0001 0000 0000 0000 0000 0000 0000 0050 0000 0000 0000 00FF 0002
40: 0000 0000 0000 0000 0000 0000 0000 0000 000D 0000 1028 01A4 0000 0000 0000 0000
60: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0F80 0004 0000 0000

Bus : 00 Device: 30 Function : 02 --> 266E8086 Vendor : 8086 Device : 266E (rev 03) - Intel Corporation 82801FB/FR/FW/FRW AC '97 Audio Controller/ Sigmatel
00: 8086 266E 0007 0290 0003 0401 0000 0000 ED01 0000 EC41 0000 FE00 DFEB FD00 DFEB
20: 0000 0000 0000 0000 0000 0000 1028 01A4 0000 0000 0050 0000 0000 0000 0110 0000
40: 0109 0000 0000 0000 0000 0000 0000 0000 0001 C9C2 0000 0000 0000 0000 0000 0000
60: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0F80 0004 0000 0000

Bus : 00 Device: 30 Function : 03 --> 266D8086 Vendor : 8086 Device : 266D (rev 03) - Intel Corporation 82801 db (m)ich4(-m) - AC '97 audio Controller
00: 8086 266D 0005 0290 0003 0703 0000 0000 EE01 0000 EC81 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 14F1 5423 0000 0000 0050 0000 0000 0000 0211 0000
40: 0000 0000 0000 0000 0000 0000 0000 0000 0001 C9C2 0000 0000 0000 0000 0000 0000
60: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0F80 0004 0000 0000

Bus : 00 Device: 31 Function : 00 --> 26418086 Vendor : 8086 Device : 2641 (rev 03) - Intel Corporation 82801FBM LPC Interface Bridge (ICH6-M)
00: 8086 2641 0107 0200 0003 0601 0000 0080 0000 0000 0000 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 1028 01A4 0000 0000 0000 0000 0000 0000 0000 0000
40: 1001 0000 0080 0000 1081 0000 0010 0000 0000 0000 0000 0000 0000 0000 0000 0000
60: 8080 8080 0091 0000 8080 8080 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0010 1C00 0901 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 06A0 0000 0000 0000 1C00 6000 0300 0000 0000 0000 0000 0000 0000 0801 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 C0C0 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 8001 F000 0000 0000 0F80 0004 0000 0000

Bus : 00 Device: 31 Function : 01 --> 266F8086 Vendor : 8086 Device : 266F (rev 03) - Intel Corporation 82801FB/FBM Ultra ATA Storage Controllers - 266F
00: 8086 266F 0005 0280 8A03 0101 0000 0000 01F1 0000 03F5 0000 0171 0000 0375 0000
20: BFA1 0000 0000 0000 0000 0000 1028 01A4 0000 0000 0000 0000 0000 0000 010B 0000
40: E337 0000 000B 0000 0003 0021 0000 0000 0000 0000 10F0 0000 0000 0000 0000 0000
60: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0003 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0F80 0004 0000 0000

Bus : 00 Device: 31 Function : 03 --> 266A8086 Vendor : 8086 Device : 266A (rev 03) - Intel Corporation 82801BA/CA SMBus Controller
00: 8086 266A 0001 0280 0003 0C05 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
20: 10C1 0000 0000 0000 0000 0000 1028 01A4 0000 0000 0000 0000 0000 0000 0200 0000
40: 0001 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
60: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0F80 0004 0000 0000

Bus : 02 Device: 01 Function : 00 --> AC56104C Vendor : 104C Device : AC56 (rev 00) - Texas Instruments PCI1510 PCCard CardBus Controller
00: 104C AC56 0007 0210 0000 0607 4010 0002 F000 FFAF 00A0 0200 0302 2003 E000 FFAF
20: E000 FFAF 0000 FAC0 F000 FEBF FE00 0000 FEFC 0000 FD00 0000 FDFC 0000 0110 04C0
40: 1028 01A4 0001 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
60: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 5061 0840 0000 0000 0000 0000 1002 0000 A2C0 6064 0000 0000 0000 0000 0000 0000
A0: 0001 FE12 0000 00C0 0003 0000 0017 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000

Bus : 02 Device: 03 Function : 00 --> 431914E4 Vendor : 14E4 Device : 4319 (rev 02) - <Unknown device>
00: 14E4 4319 0000 0000 0002 0280 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 1028 0005 0000 0000 0000 0000 0000 0000 0100 0000
40: 0001 07C2 4000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
60: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 1000 1800 0000 0000 0000 0000 0003 0000 0000 0000 0200 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000

Bus : 02 Device: 08 Function : 00 --> 10688086 Vendor : 8086 Device : 1068 (rev 03) - <Unknown device>
00: 8086 1068 0117 0290 0003 0200 4010 0000 D000 DFDF DF41 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 1028 01A4 0000 0000 00DC 0000 0000 0000 0114 3808
40: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
60: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0001 FE22
E0: 4000 3A00 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0F66 0004 0000 0000

*****************************

ISA Dump from address $290 --> <Unknown> (ISA at $0290) (No error)
 --> all bytes have the same value ($FF)

*****************************

SMB Dump from address $51 --> <RAM> (SMBus at $10C0) (No error)
00: 80 08 07 0D 09 02 40 00 04 60 70 00 82 10 00 01   ......@..`p.....
10: 0E 04 0C 01 02 20 00 75 70 00 00 48 30 48 2A 20   ..... .up..H0H*
20: 75 75 45 45 00 00 00 00 00 3C 48 30 2D 60 00 00   uuEE.....<H0-`..
30: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 33   ...............3
40: 40 00 00 00 00 00 00 00 02 56 38 32 36 36 33 32   @........V826632
50: 42 32 34 53 41 54 47 2D 43 30 00 00 00 05 1C 4A   B24SATG-C0.....J
60: 6F 13 09 00 00 00 00 00 00 00 00 00 00 00 00 00   o...............
70: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
80: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
90: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
A0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
B0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
C0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
D0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
E0: 38 49 50 45 31 30 30 30 2D 38 30 00 00 00 00 00   8IPE1000-80.....
F0: AA 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
SMB Device at address $69 --> (SMBus at $10C0) (No error)

*****************************

Retry attempts info for SMBus at $10C0
  [ -1]=301
  [  1]=301

*****************************

Pause stats for SMBusIntel@$10C0: min=48151 max=49999 avg=49829(2976) touts=0 count=2976

*****************************

Scanning SMBus at $10C0...
Decoding DIMM #1
 Memory type is DDR
 Module Rows : 2
 Levels : 2.5V
 Parity : NO PARITY
 Refresh Rate : 7.8us
 Total Size : 256MB

*****************************

Scanning SMBus at $10C0...
 - device found at $08
 - device found at $51
 - device found at $69

*****************************

Can change fan speeds : DON'T KNOW
Can smoothly change fan speeds : DON'T KNOW
Can stop fans : DON'T KNOW

*****************************

WMI interface is registered : ON
MB manufacturer: Dell Inc.
MB model: 0U6962
MB version:    
ACPI temp: 37.5
ACPI active trip point: 0.0
ACPI passive trip point: -273.2
ACPI critical trip point: 102.0
WMI quick analysis results -->
EXPLORING : root\CIMV2\Win32_BaseBoard
  -> Object Start
  Caption = Base Board
  CreationClassName = Win32_BaseBoard
  Description = Base Board
  HostingBoard = True
  Manufacturer = Dell Inc.
  Name = Base Board
  PoweredOn = True
  Product = 0U6962
  SerialNumber = .HJZ2581.CN4864357F4914.
  Tag = Base Board
  Version =    
  Method -> IsCompatible(ElementToCheck)
EXPLORING : root\WMI\msacpi_thermalzonetemperature
  -> Object Start
  Active = True
  ActiveTripPoint =  0 0 0 0 0 0 0 0 0 (0.0C)
  ActiveTripPointCount = 0
  CriticalTripPoint = 3752 (102.0C)
  CurrentTemperature = 3107 (37.5C)
  InstanceName = ACPI\ThermalZone\THM__0
  PassiveTripPoint = 0 (-273.2C)
  Reserved = 0
  SamplingPeriod = 0
  ThermalConstant1 = 0
  ThermalConstant2 = 0
  ThermalStamp = 6
EXPLORING : root\CIMV2\CIM_AssociatedSensor
EXPLORING : root\CIMV2\CIM_CoolingDevice
  -> Object Start
  ActiveCooling = True
  Availability = 3
  Caption = Cooling Device
  CreationClassName = Win32_Fan
  Description = Cooling Device
  DeviceID = root\cimv2 0
  Name = Cooling Device
  Status = OK
  StatusInfo = 2
  SystemCreationClassName = Win32_ComputerSystem
  SystemName = SUPERBILL-3
  Method -> SetPowerState(PowerState,Time)
  Method -> Reset
  Method -> SetSpeed(DesiredSpeed)
EXPLORING : root\CIMV2\CIM_Fan
  -> Object Start
  ActiveCooling = True
  Availability = 3
  Caption = Cooling Device
  CreationClassName = Win32_Fan
  Description = Cooling Device
  DeviceID = root\cimv2 0
  Name = Cooling Device
  Status = OK
  StatusInfo = 2
  SystemCreationClassName = Win32_ComputerSystem
  SystemName = SUPERBILL-3
  Method -> SetPowerState(PowerState,Time)
  Method -> Reset
  Method -> SetSpeed(DesiredSpeed)
EXPLORING : root\CIMV2\CIM_HeatPipe
EXPLORING : root\CIMV2\CIM_ManagementController
EXPLORING : root\CIMV2\CIM_NumericSensor
  -> Object Start
  Accuracy = 32768
  Caption = Numeric Sensor
  CreationClassName = Win32_TemperatureProbe
  Description = CPU Internal Temperature
  DeviceID = root\cimv2 0
  MaxReadable = 1270
  MinReadable = 0
  Name = Numeric Sensor
  Resolution = 1000
  Status = OK
  SystemCreationClassName = Win32_ComputerSystem
  SystemName = SUPERBILL-3
  Tolerance = 5
  Method -> SetPowerState(PowerState,Time)
  Method -> Reset
EXPLORING : root\CIMV2\CIM_PackageAlarm
EXPLORING : root\CIMV2\CIM_PackageCooling
EXPLORING : root\CIMV2\CIM_Refrigeration
EXPLORING : root\CIMV2\CIM_Sensor
  -> Object Start
  Accuracy = 32768
  Caption = Numeric Sensor
  CreationClassName = Win32_TemperatureProbe
  Description = CPU Internal Temperature
  DeviceID = root\cimv2 0
  MaxReadable = 1270
  MinReadable = 0
  Name = Numeric Sensor
  Resolution = 1000
  Status = OK
  SystemCreationClassName = Win32_ComputerSystem
  SystemName = SUPERBILL-3
  Tolerance = 5
  Method -> SetPowerState(PowerState,Time)
  Method -> Reset
EXPLORING : root\CIMV2\CIM_Tachometer
EXPLORING : root\CIMV2\CIM_TemperatureSensor
  -> Object Start
  Accuracy = 32768
  Caption = Numeric Sensor
  CreationClassName = Win32_TemperatureProbe
  Description = CPU Internal Temperature
  DeviceID = root\cimv2 0
  MaxReadable = 1270
  MinReadable = 0
  Name = Numeric Sensor
  Resolution = 1000
  Status = OK
  SystemCreationClassName = Win32_ComputerSystem
  SystemName = SUPERBILL-3
  Tolerance = 5
  Method -> SetPowerState(PowerState,Time)
  Method -> Reset
EXPLORING : root\CIMV2\CIM_VoltageSensor
EXPLORING : root\CIMV2\Win32_CurrentProbe
EXPLORING : root\CIMV2\Win32_Fan
  -> Object Start
  ActiveCooling = True
  Availability = 3
  Caption = Cooling Device
  CreationClassName = Win32_Fan
  Description = Cooling Device
  DeviceID = root\cimv2 0
  Name = Cooling Device
  Status = OK
  StatusInfo = 2
  SystemCreationClassName = Win32_ComputerSystem
  SystemName = SUPERBILL-3
  Method -> SetPowerState(PowerState,Time)
  Method -> Reset
  Method -> SetSpeed(DesiredSpeed)
EXPLORING : root\CIMV2\Win32_HeatPipe
EXPLORING : root\CIMV2\Win32_Refrigeration
EXPLORING : root\CIMV2\Win32_TemperatureProbe
  -> Object Start
  Accuracy = 32768
  Caption = Numeric Sensor
  CreationClassName = Win32_TemperatureProbe
  Description = CPU Internal Temperature
  DeviceID = root\cimv2 0
  MaxReadable = 1270
  MinReadable = 0
  Name = Numeric Sensor
  Resolution = 1000
  Status = OK
  SystemCreationClassName = Win32_ComputerSystem
  SystemName = SUPERBILL-3
  Tolerance = 5
  Method -> SetPowerState(PowerState,Time)
  Method -> Reset
EXPLORING : root\CIMV2\Win32_VoltageProbe
EXPLORING : SMBIOS
  -> Object Start
Structure  27 - 1B00 - fixed len is 12 bytes -> Cooling device
  -> FF FF 63 00 00 DD 00 00
Structure  28 - 1C00 - fixed len is 20 bytes -> Temperature probe
  -> 01 63 F6 04 00 00 E8 03 05 00 00 80 00 DC 00 00
  -> <CPU Internal Temperature>
Structure 176 - B000 - fixed len is 5 bytes -> Unknown (176)
  -> 00
Structure 177 - B100 - fixed len is 12 bytes -> Unknown (177)
  -> 00 00 00 00 00 00 00 00
Structure 208 - D000 - fixed len is 10 bytes -> Unknown (208)
  -> 01 04 FE 00 A4 01
Structure 216 - D800 - fixed len is 9 bytes -> Unknown (216)
  -> 01 03 01 F0 03
  -> <Intel Corp.         >
  -> < >
  -> <1219  >
Structure 217 - D900 - fixed len is 8 bytes -> Unknown (217)
  -> 01 02 01 03
  -> <US-101>
  -> <Proprietary>
Structure 219 - DB00 - fixed len is 9 bytes -> Unknown (219)
  -> 03 01 02 03 FF
  -> <System Device Bay>
  -> <Floppy, Battery, CD-ROM, CD-RW, DVD, DVD+RW, DVD+/-RW, Hard Disk>
  -> <CDRW+DVD  >
Structure 220 - DC00 - fixed len is 22 bytes -> Unknown (220)
  -> 01 F0 00 00 02 F0 00 00 00 00 03 F0 04 F0 00 00 00 00
Structure 221 - DD00 - fixed len is 19 bytes -> Unknown (221)
  -> 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
Structure 212 - D400 - fixed len is 147 bytes -> Unknown (212)
  -> 70 00 71 00 00 10 2D 2E 5C 00 78 BF 40 5D 00 78 BF 00 65 00 21 F7 00 66 00 21 F7 08 5E 00 23 FE 01 5F 00 23 FE 00 F1 00 21 FC 00 F2 00 21 FC 01 F3 00 21 FC 02 28 00 23 F3 00 29 00 23 F3 04 2A 00 23 F3 08 2B 00 58 00 00 2C 00 59 00 00 E7 00 1D F3 04 E6 00 1D F3 00 0E 01 23 FD 02 0F 01 23 FD 00 9B 00 23 EF 10 9C 00 23 EF 00 E8 00 23 DF 20 E9 00 23 DF 00 12 01 34 FB 04 13 01 34 FB 00 08 00 1D DF 00 03 00 1D DF 00 FF FF 00 00 00
Structure 212 - D401 - fixed len is 127 bytes -> Unknown (212)
  -> 70 00 71 00 03 40 49 4A 42 00 48 7F 80 43 00 48 7F 00 55 00 47 BF 00 6D 00 47 BF 40 0C 01 46 FB 04 0D 01 46 FB 00 14 01 46 E7 00 15 01 46 E7 08 16 01 46 E7 10 0A 01 48 EF 10 0B 01 48 EF 00 2D 00 48 DF 20 2E 00 48 DF 00 11 01 48 BF 00 10 01 48 BF 40 F0 00 46 DF 20 ED 00 46 DF 00 41 01 46 FE 01 40 01 46 FE 00 EA 00 67 F3 00 EB 00 67 F3 04 EC 00 67 F3 08 FF FF 00 00 00
Structure 222 - DE00 - fixed len is 13 bytes -> Unknown (222)
  -> 01 02 FF FF 00 00 00 00 00
<-- End of WMI quick analysis results

*****************************

DMI structures from SMBIOS ver. 2.3
MBManufacturer : Dell Inc.
MBModel : 0U6962
MBVersion : 
BIOSVendor : Dell Inc.
BIOSVersion : A04
Structure 218 - DA00 - fixed len is 61 bytes -> Unknown (218)
  -> B2 00 0D 5F 0F 37 40 7D 00 00 00 00 00 7E 00 02 00 00 00 40 00 04 00 01 00 41 00 04 00 00 00 01 F0 01 F0 00 00 02 F0 02 F0 00 00 03 F0 03 F0 00 00 04 F0 04 F0 00 00 FF FF 00 00 00 00
Structure   0 - 0000 - fixed len is 16 bytes -> BIOS information
  -> 01 02 00 F0 03 08 90 9B 01 7D 00 00 17 00 87 03
  -> 'Dell Inc.'
  -> 'A04'
  -> '04/19/2005'
Structure   1 - 0100 - fixed len is 21 bytes -> System information
  -> 01 02 00 03 44 45 4C 4C 4A 00 10 5A 80 32 C8 C0 4F 35 38 31 06
  -> 'Dell Inc.'
  -> 'Inspiron 2200                   '
  -> 'HJZ2581'
  -> ' '
Structure   2 - 0200 - fixed len is 5 bytes -> Base board (or module) information
  -> 01 02 03 04 05
  -> 'Dell Inc.'
  -> '0U6962'
  -> '   '
  -> '.HJZ2581.CN4864357F4914.'
  -> '          '
Structure   3 - 0300 - fixed len is 9 bytes -> System enclosure or chassis
  -> 01 08 00 03 00 03 03 03 03
  -> 'Dell Inc.'
  -> '          '
  -> 'HJZ2581'
  -> ' '
Structure  27 - 1B00 - fixed len is 8 bytes -> Cooling device
  -> FF FF 63 00 00 DD 00 00
Structure  28 - 1C00 - fixed len is 16 bytes -> Temperature probe
  -> 01 63 F6 04 00 00 E8 03 05 00 00 80 00 DC 00 00
  -> 'CPU Internal Temperature'
Structure 176 - B000 - fixed len is 1 bytes -> Unknown (176)
  -> 00
Structure 177 - B100 - fixed len is 8 bytes -> Unknown (177)
  -> 00 00 00 00 00 00 00 00
Structure 208 - D000 - fixed len is 6 bytes -> Unknown (208)
  -> 01 04 FE 00 A4 01
Structure 216 - D800 - fixed len is 5 bytes -> Unknown (216)
  -> 01 03 01 F0 03
  -> 'Intel Corp.         '
  -> ' '
  -> '1219  '
Structure 217 - D900 - fixed len is 4 bytes -> Unknown (217)
  -> 01 02 01 03
  -> 'US-101'
  -> 'Proprietary'
Structure 219 - DB00 - fixed len is 5 bytes -> Unknown (219)
  -> 03 01 02 03 FF
  -> 'System Device Bay'
  -> 'Floppy, Battery, CD-ROM, CD-RW, DVD, DVD+RW, DVD+/-RW, Hard Disk'
  -> 'CDRW+DVD  '
Structure 220 - DC00 - fixed len is 18 bytes -> Unknown (220)
  -> 01 F0 00 00 02 F0 00 00 00 00 03 F0 04 F0 00 00 00 00
Structure 221 - DD00 - fixed len is 15 bytes -> Unknown (221)
  -> 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
Structure 212 - D400 - fixed len is 143 bytes -> Unknown (212)
  -> 70 00 71 00 00 10 2D 2E 5C 00 78 BF 40 5D 00 78 BF 00 65 00 21 F7 00 66 00 21 F7 08 5E 00 23 FE 01 5F 00 23 FE 00 F1 00 21 FC 00 F2 00 21 FC 01 F3 00 21 FC 02 28 00 23 F3 00 29 00 23 F3 04 2A 00 23 F3 08 2B 00 58 00 00 2C 00 59 00 00 E7 00 1D F3 04 E6 00 1D F3 00 0E 01 23 FD 02 0F 01 23 FD 00 9B 00 23 EF 10 9C 00 23 EF 00 E8 00 23 DF 20 E9 00 23 DF 00 12 01 34 FB 04 13 01 34 FB 00 08 00 1D DF 00 03 00 1D DF 00 FF FF 00 00 00
Structure 212 - D401 - fixed len is 123 bytes -> Unknown (212)
  -> 70 00 71 00 03 40 49 4A 42 00 48 7F 80 43 00 48 7F 00 55 00 47 BF 00 6D 00 47 BF 40 0C 01 46 FB 04 0D 01 46 FB 00 14 01 46 E7 00 15 01 46 E7 08 16 01 46 E7 10 0A 01 48 EF 10 0B 01 48 EF 00 2D 00 48 DF 20 2E 00 48 DF 00 11 01 48 BF 00 10 01 48 BF 40 F0 00 46 DF 20 ED 00 46 DF 00 41 01 46 FE 01 40 01 46 FE 00 EA 00 67 F3 00 EB 00 67 F3 04 EC 00 67 F3 08 FF FF 00 00 00
Structure 222 - DE00 - fixed len is 9 bytes -> Unknown (222)
  -> 01 02 FF FF 00 00 00 00 00

*****************************

0 events defined

*****************************

Tray icon size : 16x16
UPTIME : 0 days 18:56:12

*****************************

Win9x:NO  64Bit:NO  GiveIO:YES  SpeedFan:YES
I/O properly initialized
Linked ISA BUS at $0290
Linked Intel 82801FB ICH6 SMBUS at $10C0
Scanning ISA BUS at $0290...
none at $3E8 msg : DELL Sensor constructor starting...
none at $3E8 msg : DFC : c=0000 d=0100 s1=0000 s2=0000
none at $3E8 msg : Fan 0 properly set through SMBIOS
none at $3E8 msg : DFC : c=FFFF d=0101 s1=0000 s2=0000
none at $3E8 msg : info1 : CMD=$002C   DATA=$4B80   S1=$0000   S2=$0000
none at $3E8 msg : info1 : CMD=$0027   DATA=$3280   S1=$0000   S2=$0000
none at $3E8 msg : info1 : CMD=$0028   DATA=$3280   S1=$0000   S2=$0000
none at $3E8 msg : ERROR info1 : CMD=$FFFF   DATA=$0003   S1=$0000   S2=$0000
none at $3E8 msg : ERROR info1 : CMD=$FFFF   DATA=$0004   S1=$0000   S2=$0000
none at $3E8 msg : info fan0 : CMD=$0788   DATA=$0000   S1=$0000   S2=$0000
none at $3E8 msg : info fan1 : CMD=$039A   DATA=$0001   S1=$0000   S2=$0000
none at $3E8 msg : info fan2 : CMD=$039A   DATA=$0002   S1=$0000   S2=$0000
Scanning Intel SMBus at $10C0...
SMART Enabled for drive 0
Found Hitachi HTS541060G9AT00 (60.0GB)
Found ACPI temperature (37.5C)
End of detection
Loaded 0 events
QUERYSUSPEND message received
Preparing for suspend...
I/O properly closed
Ready for suspend!
SUSPEND message received
Preparing for suspend...
Ready for suspend!
APMRESUME message received
Resuming from suspend...
Win9x:NO  64Bit:NO  GiveIO:YES  SpeedFan:YES
I/O properly initialized
Loaded 0 events
Resumed from suspend!
APMRESUME message received
Resuming from suspend...
Loaded 0 events
Resumed from suspend!
AC is ONLINE Battery Charge HIGH
Battery Life Percentage 100%
AC is ONLINE Battery Charge HIGH
Battery Life Percentage 100%

*****************************

Win9x:NO  64Bit:NO  GiveIO:YES  SpeedFan:YES
SpeedFan.sys ver. 1.002
  -> Can read memory
  -> Can read MSR
About to do a test on INTEL MSRs...
Found <Intel(R) Pentium(R) M processor 1.60GHz>
CURRENT AFFINITY=0001
CPU#00
  AFFINITY=0001
CPUID[1].EBX=00000816
  TSC=$000002B6F7BF60B3
  MSR[$1B]=$00000000FEE00900
CPU#00 MSR[$1B]=$00000000FEE00900
End of INTEL MSR test
I/O properly initialized
Linked ISA BUS at $0290
Linked PCI
Starting PCI scan...
RCBA=$F0008001
  FuncDis=$000F0015
Command Register : $0101
I/O Space Enabled
Host Configuration Register : $01
SMBus Host Enabled
Linked Intel 82801FB ICH6 SMBUS at $10C0
HST_CNT=$08
PCI scan done!
Scanning ISA BUS at $0290...
About to check DELL support
PCI scanning is enabled
Intel SouthBridge found
DELL sensors
none at $3E8 msg : DELL Sensor constructor starting...
none at $3E8 msg : DFC : c=0000 d=0100 s1=0000 s2=0000
none at $3E8 msg : Fan 0 properly set through SMBIOS
none at $3E8 msg : DFC : c=FFFF d=0101 s1=0000 s2=0000
none at $3E8 msg : info1 : CMD=$002C   DATA=$4B80   S1=$0000   S2=$0000
none at $3E8 msg : info1 : CMD=$0027   DATA=$3280   S1=$0000   S2=$0000
none at $3E8 msg : info1 : CMD=$0028   DATA=$3280   S1=$0000   S2=$0000
none at $3E8 msg : ERROR info1 : CMD=$FFFF   DATA=$0003   S1=$0000   S2=$0000
none at $3E8 msg : ERROR info1 : CMD=$FFFF   DATA=$0004   S1=$0000   S2=$0000
none at $3E8 msg : info fan0 : CMD=$0788   DATA=$0000   S1=$0000   S2=$0000
none at $3E8 msg : info fan1 : CMD=$039A   DATA=$0001   S1=$0000   S2=$0000
none at $3E8 msg : info fan2 : CMD=$039A   DATA=$0002   S1=$0000   S2=$0000
 -> Temperature 1 offset : 0
 -> Temperature 2 offset : 0
 -> Temperature 3 offset : 0
 -> FAN1 mult : 1
 -> FAN1 div : 1
 -> FAN2 mult : 1
 -> FAN2 div : 1
 -> FAN3 mult : 1
 -> FAN3 div : 1
 -> Reverse PWM01 logic : OFF
End of DELL support check
INFO: ISA seems to be unused
Second pass...
SMSC (1) r[$0D]=$00 r[$0E]=$00 r[$20]=$1D r[$21]=$01 r[$07]=$0B 
SMSC (2) r[$0D]=$00 r[$0E]=$00 r[$20]=$1D r[$21]=$01 r[$07]=$0B 
ITE r[$20]=$1D r[$21]=$01 r[$22]=$00 r[$07]=$0B 
Checking $0370 for SMSC (2)...
Checking $0370 for SMSC (1)...
Checking $03F0 for SMSC (2)...
Checking $03F0 for SMSC (1)...
Checking $002E for SMSC (1)...
Registers [$002E] : $1D $01 $00 $00
Checking $004E for SMSC (1)...
Checking $002E for WINBOND...
Checking $004E for WINBOND...
Checking $0250 for WINBOND...
Checking $0370 for WINBOND...
Checking $03F0 for WINBOND...
Checking $002E for NS...
Checking $004E for NS...
Checking $002E for ITE (1)...
Registers [$002E] : $1D $01 $00
Scanning Intel SMBus at $10C0...
About to probe TOSHIBA SUPPORT...
End of TOSHIBA SUPPORT probing
Version 1.1 21 00000007
SMART Enabled for drive 0
 --> S.M.A.R.T. attributes properly read
 --> S.M.A.R.T. thresholds properly read
Start of DEBUG DATA for drive 0
--> cylinders : 7296
--> tracks per cilinder : 255
--> sectors per track : 63
--> bytes per sector : 512
--> disk size : 60.0
End of DEBUG DATA for drive 0
Found Hitachi HTS541060G9AT00 (60.0GB)
Found Hitachi HTS541060G9AT00 Firmware revision <MB3OA61A> (60.0GB) Serial <MPB3PAX5H0JM1G>
 --> ATA device
 --> Fixed Drive
 --> S.M.A.R.T. Supported (enabled)
 --> Power Management Supported (enabled)
 --> Advanced Power Management Supported (Current:$4080)
 --> Automatic Acoustic Management Supported (Current:$80  Reccomended:$80)
 --> 48-bit Addressing ($7C80 $06FC $0000 $0000)
 --> UDMA Mode 0 Supported
 --> UDMA Mode 1 Supported
 --> UDMA Mode 2 Supported
 --> UDMA Mode 3 Supported
 --> UDMA Mode 4 Supported
 --> UDMA Mode 5 Supported
 --> UDMA Mode 5 Active
SMART Structure Revision : $0010
ID=$01  NAME=Raw Read Error Rate  VALUE=$64  WORST=$64  RAW=$000000000000  THRSHLD=$3E  FLAGS=$000B
ID=$02  NAME=Throughput Performance  VALUE=$64  WORST=$64  RAW=$0000000000E4  THRSHLD=$00  FLAGS=$0004
ID=$03  NAME=Spin Up Time  VALUE=$9F  WORST=$9F  RAW=$000F00000001  THRSHLD=$21  FLAGS=$0007
ID=$04  NAME=Start/Stop Count  VALUE=$63  WORST=$63  RAW=$0000000007BF  THRSHLD=$00  FLAGS=$0012
ID=$05  NAME=Reallocated Sector Count  VALUE=$64  WORST=$64  RAW=$000000000000  THRSHLD=$05  FLAGS=$0033
ID=$07  NAME=Seek Error Rate  VALUE=$64  WORST=$64  RAW=$000000000000  THRSHLD=$00  FLAGS=$000A
ID=$08  NAME=Seek Time Performance  VALUE=$64  WORST=$64  RAW=$000000000000  THRSHLD=$00  FLAGS=$0004
ID=$09  NAME=Power On Hours Count  VALUE=$55  WORST=$55  RAW=$000000001AE5  THRSHLD=$00  FLAGS=$0012
ID=$0A  NAME=Spin Retry Count  VALUE=$64  WORST=$64  RAW=$000000000000  THRSHLD=$00  FLAGS=$0012
ID=$0C  NAME=Power Cycle Count  VALUE=$63  WORST=$63  RAW=$000000000794  THRSHLD=$00  FLAGS=$0032
ID=$BF  NAME=GSense Error Rate  VALUE=$64  WORST=$64  RAW=$000000000001  THRSHLD=$00  FLAGS=$000A
ID=$C0  NAME=Power Off Retract Count  VALUE=$64  WORST=$64  RAW=$00000000006D  THRSHLD=$00  FLAGS=$0032
ID=$C1  NAME=Load Cycle Count  VALUE=$59  WORST=$59  RAW=$00000001B2EE  THRSHLD=$00  FLAGS=$0012
ID=$C2  NAME=Temperature  VALUE=$98  WORST=$98  RAW=$003100050024  THRSHLD=$00  FLAGS=$0002
Current HD temperature is 36C
ID=$C4  NAME=Reallocated Event Count  VALUE=$64  WORST=$64  RAW=$000000000000  THRSHLD=$00  FLAGS=$0032
ID=$C5  NAME=Current Pending Sector  VALUE=$64  WORST=$64  RAW=$000000000000  THRSHLD=$00  FLAGS=$0022
ID=$C6  NAME=Offline Correctable  VALUE=$64  WORST=$64  RAW=$000000000000  THRSHLD=$00  FLAGS=$0008
ID=$C7  NAME=UltraATA CRC Error Rate  VALUE=$C8  WORST=$C8  RAW=$000000000000  THRSHLD=$00  FLAGS=$000A
Linked S.M.A.R.T.
 -> Temperature 1 offset : 0
About to probe SCSI...
End of SCSI probing
About to probe UGURU support...
Motherboard is Dell Inc. 0U6962
End of UGURU support probing
About to probe ACPI temperatures...
Found ACPI temperature (37.5C)
 -> Temperature 1 offset : 0
End of ACPI temperatures probing
About to probe AMD Internal Sensors...
End of AMD Internal Sensors probing
About to probe INTEL Internal Sensors...
End of INTEL Internal Sensors probing
End of detection
Reading Cfg Version 2.01
Old sensor properly detected -->
  DELL on ISA @ $3E8
Old sensor properly detected -->
  HD0 (60.0GB) on SMART @ $0
Old sensor properly detected -->
  ACPI on ISA @ $0
PWM from DELL@$3E8(onISA@$290) -->
  Speed01 0 100
  properly added
Temperature from Hitachi HTS541060G9AT00MPB3PAX5H0JM1G -->
  HD0 40 50 0
  properly added
Temperature from ACPI -->
  Temp1 40 50 0
  PWM 1 from 0
  properly added
Temperature from DELL@$3E8(onISA@$290) -->
  DIMM 40 50 0
  PWM 1 from 0
  properly added
Temperature from DELL@$3E8(onISA@$290) -->
  CPU 40 50 0
  PWM 1 from 0
  properly added
Temperature from DELL@$3E8(onISA@$290) -->
  GPU 40 50 0
  PWM 1 from 0
  properly added
Fan from DELL@$3E8(onISA@$290) -->
  Fan1
  properly added
Fan from DELL@$3E8(onISA@$290) -->
  Fan2
  properly added
Fan from DELL@$3E8(onISA@$290) -->
  Fan3
  properly added
Loaded 0 events
QUERYSUSPEND message received
Preparing for suspend...
I/O properly closed
Ready for suspend!
SUSPEND message received
Preparing for suspend...
Ready for suspend!
APMRESUME message received
Resuming from suspend...
Win9x:NO  64Bit:NO  GiveIO:YES  SpeedFan:YES
SpeedFan.sys ver. 1.002
  -> Can read memory
  -> Can read MSR
About to do a test on INTEL MSRs...
Found <Intel(R) Pentium(R) M processor 1.60GHz>
CURRENT AFFINITY=0001
CPU#00
  AFFINITY=0001
CPUID[1].EBX=00000816
  TSC=$0000000191C70A8A
  MSR[$1B]=$00000000FEE00900
CPU#00 MSR[$1B]=$00000000FEE00900
End of INTEL MSR test
I/O properly initialized
Reading Cfg Version 2.01
Old sensor properly detected -->
  DELL on ISA @ $3E8
Old sensor properly detected -->
  HD0 (60.0GB) on SMART @ $0
Old sensor properly detected -->
  ACPI on ISA @ $0
Loaded 0 events
Resumed from suspend!
APMRESUME message received
Resuming from suspend...
Reading Cfg Version 2.01
Old sensor properly detected -->
  DELL on ISA @ $3E8
Old sensor properly detected -->
  HD0 (60.0GB) on SMART @ $0
Old sensor properly detected -->
  ACPI on ISA @ $0
Loaded 0 events
Resumed from suspend!
AC is ONLINE Battery Charge HIGH
Battery Life Percentage 100%
AC is ONLINE Battery Charge HIGH
Battery Life Percentage 100%
HTTP state=not connected
HTTP state=dns lookup
HTTP state=dns lookup done
HTTP state=connected
HTTP state=waiting header
HTTP state=waiting body
HTTP state=unknown
HTTP state=ready
Preparing report...