Sender : 
SpeedFan version : SpeedFan 4.41 beta 11
Motherboard model : Emachines E627-5279

***************************** BIOS INFO

BIOS CopyRight : ACRSYS - 3InsydeH2O Version V1.10
BIOS Date : 11/30/09
BIOS Extended Info : 
BIOS Name : AT/AT COMPATIBLE

Windows NT Uniprocessor Free version 5.1.2600 (Windows XP)

1 processor(s)
Advanced Micro Devices AMD Athlon(tm) Processor TF-20 family 15 model 12 stepping 2 brand 0 1596 MHz
Running at 1596 MHz
I Agree to receive beta versions : ON

***************************** CPUID INFO

CPU Name : AMD Athlon(tm) Processor TF-20
 - Identified CPU Name : !!!AMD Processor model unknown
 - Vendor : AuthenticAMD
 - Family : 15
 - Model : 124
 - Stepping : 2
 - L1 Data Cache : 64 KB 2-way
 - L1 Instruction Cache : 64 KB 2-way
 - L2 Cache : 512 KB 16-way
 - Die Revision : DH-G2 
 - Socket Type : Socket S1g1
 - Manufacturing Technology : Unknown
 - Max cpu speed : 1600 MHz
 - Core Multi-processing Legacy Mode : no
 - Cores : 1
 - CPUs in system : 1
 - Secure Virtual Machine Feature : yes
 - Temperature Sensor : yes
 - Frequency ID Control : yes
 - Voltage ID Control : yes
 - Hardware P-State Control : no
 - Hardware Thermal Control : yes
 - Software Thermal Control : yes
 - THERMTRIP : yes
 - TDP : 0.0 W
 - Execute Disable : yes
 - Hyper-Threading Technology : no
$00000000 - $00000001 $68747541 $444D4163 $69746E65 - .... Auth cAMD enti
$80000000 - $80000018 $68747541 $444D4163 $69746E65 - .... Auth cAMD enti
$00000001 - $00070FC2 $00000800 $00002001 $078BFBFF - .... .... . .. ....
$80000001 - $00070FC2 $00000C85 $0000011D $EBD3FBFF - .... .... .... ....
$80000002 - $20444D41 $6C687441 $74286E6F $5020296D - AMD  Athl on(t m) P
$80000003 - $65636F72 $726F7373 $2D465420 $00003032 - roce ssor  TF- 20..
$80000004 - $00000000 $00000000 $00000000 $00000000 - .... .... .... ....
$80000005 - $FF08FF08 $FF20FF20 $40020140 $40020140 - ....  . . @..@ @..@
$80000006 - $00000000 $42004200 $02008140 $00000000 - .... .B.B @... ....
$80000007 - $00000000 $00000000 $00000000 $0000007F - .... .... .... ...
$80000008 - $00003028 $00000000 $00000000 $00000000 - (0.. .... .... ....
 - DEBUG : MSRC0010015=$0000000000000000  MSRC0010042=$3014161614080008  MSRC0010071=$FFFFFFFFFFFFFFFF
 -         AnalyzeFamilyF: BrandId=$0C85 BaseModel=$0C PwrLmt=$04 BTI=$06 NN=$05 Socket=$00 CmpCap=$00 TDP=0
 -         !!!DeriveAmdAdditionalData didn' find this PwrLmt
 -         AnalyzeFamilyF: CurrFID=8.0 StartFID=4.0 MaxFID=8.0 - CurrVID=1.0000 StartVID=1.0000 MaxVID=1.0500
 -         !!!DeriveAmdAdditionalData table needs refining

***************************** SENSORS' READINGS

HD0 (160.0GB) on AdvSMART at $0 HD0 : 44.0   min=42.0   max=44.0   mean=44.0
Hitachi HTS545016B9A300 (drive 0) : fitness=97%   performance=98%
ACPI on ISA at $0 Temp1 : 38.0   min=38.0   max=38.0   mean=38.0
AMD K8 on PCI at $0 Core : -49.0   min=-49.0   max=-49.0   mean=-49.0

***************************** SENSORS' ASSOCIATIONS AND GENERAL CONFIG OPTIONS

HD0 --> active=ON  chip=0  index=1 wanted=40  warning=50  offset=0  InTray=ON Used pwms=
Temp1 --> active=ON  chip=1  index=1 wanted=40  warning=50  offset=0  InTray=OFF Used pwms=
Core --> active=ON  chip=2  index=1 wanted=40  warning=50  offset=0  InTray=OFF Used pwms=
Set Fans to 100% on exit : OFF
Debug Mode : ON
Use ISA : ON
Use SMB : ON
Scan PCI : ON
Scan SMB : ON
Slow SMB detection : OFF
Detect SuperIO : ON
ASUS Card Detect : ON
DELL Support : OFF
Summary Log Scan : ON
Command line : "E:\Program Files\SpeedFan\speedfan.exe" 
Delta Fan Speed : 10

***************************** CHIPSET SMBUS

Chipset : ATI SBx00
SMBus Base Address : $0B00
SMBus Revision : 0000003C
SMBus I/O Enabled : ON

***************************** PCI SCAN

Bus : 00 Device: 00 Function : 00 --> 96001022 Vendor : 1022 Device : 9600 (rev 00) - <Unknown device>
00: 1022 9600 0006 2230 0000 0600 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 1025 028D 0000 0000 00C4 0000 0000 0000 0000 0000
40: 9C08 C000 00C0 0000 0000 0000 2042 0005 1025 028D 4008 9000 1008 0005 0000 0000
60: 007F 0000 0000 0000 0200 0020 800D 818E 0000 0000 0000 0000 42AA 6E83 0000 2000
80: 0000 0000 0010 0304 2A20 0000 2613 1000 0000 8000 007F 0000 0000 0000 F808 D07C
A0: 003A 0074 0000 0500 0000 0000 0171 0280 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 8000 5408 0181 2020 1111 00D0 0000 0560 1C75 0002 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0202 0000 0200 8023 0000 0000 8000 0080 0008 E000 0000 0000

Bus : 00 Device: 01 Function : 00 --> 96021022 Vendor : 1022 Device : 9602 (rev 00) - <Unknown device>
00: 1022 9602 0007 0230 0000 0604 0000 0001 0000 0000 0000 0000 0100 0001 7171 0220
20: 9210 9220 8001 8FF1 0000 0000 0000 0000 0000 0000 0044 0000 0000 0000 00FF 0008
40: 0000 0000 B008 A803 0000 0000 1022 9602 0000 0000 0000 0000 0000 0000 0000 0000
60: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 000D 0000 1022 9602 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000

Bus : 00 Device: 04 Function : 00 --> 96041022 Vendor : 1022 Device : 9604 (rev 00) - <Unknown device>
00: 1022 9604 0007 0010 0000 0604 0010 0001 0000 0000 0000 0000 0200 0007 6131 2000
20: 9110 9200 9001 90F1 0000 0000 0000 0000 0000 0000 0050 0000 0000 0000 0110 0004
40: 0000 0000 0000 0000 0000 0000 0000 0000 5801 C803 0000 0000 A010 0142 8020 0000
60: 0810 0000 0C12 0130 0042 7011 0CE0 0024 0000 0148 0000 0001 0000 0000 0000 0000
80: 0000 0000 0000 0000 0001 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: B005 0000 0000 0000 0000 0000 0000 0000 B80D 0000 1025 028D 0008 A803 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 FFFF FFFF 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000

Bus : 00 Device: 05 Function : 00 --> 96051022 Vendor : 1022 Device : 9605 (rev 00) - <Unknown device>
00: 1022 9605 0007 0010 0000 0604 0010 0001 0000 0000 0000 0000 0800 0008 2121 2000
20: 9100 9100 FFF1 0001 0000 0000 0000 0000 0000 0000 0050 0000 0000 0000 0111 0004
40: 0000 0000 0000 0000 0000 0000 0000 0000 5801 C803 0000 0000 A010 0142 8020 0000
60: 0810 0000 0C12 0230 0042 7011 0C80 002C 0000 0148 0000 0001 0000 0000 0000 0000
80: 0000 0000 0000 0000 0001 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: B005 0000 0000 0000 0000 0000 0000 0000 B80D 0000 1025 028D 0008 A803 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 FFFF FFFF 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000

Bus : 00 Device: 17 Function : 00 --> 43901002 Vendor : 1002 Device : 4390 (rev 00) - <Unknown device>
00: 1002 4390 0007 0230 8F00 0101 4010 0000 8039 0000 804D 0000 8031 0000 8049 0000
20: 8011 0000 6000 9230 0000 0000 1025 028D 0000 0000 0050 0000 0000 0000 0116 0000
40: 0010 003A 0003 0010 BFC0 0000 0000 0000 7005 0084 0000 0000 0000 0000 0000 0000
60: 5001 0022 0000 0000 0000 0000 0000 0000 0012 0010 000F 0000 0000 0000 0000 0000
80: 0000 0000 0006 2C00 8014 01B4 A0B8 01B4 A036 01B4 A0F8 01B4 8016 01B4 8016 01B4
A0: A098 A0FC A07A A07A A07A A07A 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 2000 0000
E0: 0080 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000

Bus : 00 Device: 18 Function : 00 --> 43971002 Vendor : 1002 Device : 4397 (rev 00) - <Unknown device>
00: 1002 4397 0007 02A0 1000 0C03 0010 0080 5000 9230 0000 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 1025 028D 0000 0000 0000 0000 0000 0000 0110 0000
40: 0380 0000 0011 0000 0000 0000 0000 0000 1340 F603 0000 0000 FFFF FFFF 0000 0000
60: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 00FF 8000 0000 0000 0000 0000
80: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000

Bus : 00 Device: 18 Function : 01 --> 43981002 Vendor : 1002 Device : 4398 (rev 00) - <Unknown device>
00: 1002 4398 0017 02A0 1000 0C03 0010 0000 4000 9230 0000 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 1025 028D 0000 0000 0000 0000 0000 0000 0110 0000
40: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
60: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000

Bus : 00 Device: 18 Function : 02 --> 43961002 Vendor : 1002 Device : 4396 (rev 00) - <Unknown device>
00: 1002 4396 0017 02B0 2000 0C03 0010 0000 6400 9230 0000 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 1025 028D 0000 0000 00C0 0000 0000 0000 0211 0000
40: 0000 0000 0000 0000 0000 0000 0000 0000 01D8 809E 0000 0000 0000 0000 0000 0000
60: 2020 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0001 0100 2000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: E401 7E02 0000 0040 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 000A 20E0 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000

Bus : 00 Device: 20 Function : 00 --> 43851002 Vendor : 1002 Device : 4385 (rev 3C) - <Unknown device>
00: 1002 4385 0403 D230 003C 0C05 0000 0080 0000 0000 0000 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 1025 028D 0000 0000 00B0 0000 0000 0000 0000 0000
40: E944 FD00 0000 0000 FF0F 0000 0000 C000 0978 0FF0 0EE0 0FF0 0B21 5EA4 0000 0000
60: 0001 2024 ECBF 03DE 900F 0000 0020 0000 0000 0000 0008 FEC0 6EFF 0000 0000 06F0
80: 0AF0 0FF0 0000 0000 0000 0000 0000 0000 0B01 0000 CEF9 00FF 0000 0000 0000 0000
A0: 0000 FFFF FF7F 09F0 FF00 0208 4306 1820 0008 A802 0000 FED0 0000 0000 CB38 1A08
C0: FFFF FFFF 0000 0000 0000 0000 0000 0000 0000 0001 0000 0000 0000 0000 0000 0000
E0: B920 0000 0000 0000 0000 0000 0000 0000 0CD8 0000 087F 0044 0000 0000 00AA 0030

Bus : 00 Device: 20 Function : 01 --> 439C1002 Vendor : 1002 Device : 439C (rev 00) - <Unknown device>
00: 1002 439C 0015 0230 8A00 0101 0010 0000 0001 0000 0001 0000 0001 0000 0001 0000
20: 8001 0000 0000 0000 0000 0000 1025 028D 0000 0000 0070 0000 0000 0000 0104 0000
40: 9999 9999 FFFF FFFF 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
60: 0000 2240 2C10 0701 0001 0000 FFFF 000F 0005 0000 0000 0000 0000 0000 0000 0000
80: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000

Bus : 00 Device: 20 Function : 02 --> 43831002 Vendor : 1002 Device : 4383 (rev 00) - <Unknown device>
00: 1002 4383 0006 0410 0000 0403 0010 0000 0004 9230 0000 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 1025 028D 0000 0000 0050 0000 0000 0000 0110 0000
40: 0000 0000 0001 0000 0000 0000 0001 0000 0001 C842 0000 0000 0000 0000 0000 0000
60: 0005 0080 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000

Bus : 00 Device: 20 Function : 03 --> 439D1002 Vendor : 1002 Device : 439D (rev 00) - <Unknown device>
00: 1002 439D 000F 0220 0000 0601 0000 0080 0000 0000 0000 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 1025 028D 0000 0000 0000 0000 0000 0000 0000 0000
40: 0004 0000 FFD5 FF03 FF07 00E2 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
60: 0000 0000 0068 0000 000E 000F FFBC FFFF 4567 0023 0001 0000 001C 0000 0A05 0000
80: 0008 A803 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0400 0001 0000
A0: 0002 FED0 002F 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 E900 FFF2 0000
C0: 0000 0000 0000 0008 FFF7 FFFF 0000 7800 FF00 00FF 0000 FF00 FFFF 00FF 0000 0C00
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000

Bus : 00 Device: 20 Function : 04 --> 43841002 Vendor : 1002 Device : 4384 (rev 00) - <Unknown device>
00: 1002 4384 0007 02A0 0100 0604 4000 0081 0000 0000 0000 0000 0900 4009 00F0 2280
20: FFF0 0000 FFF0 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
40: 0026 FF00 0000 0000 0F0C D13C 0000 0000 0001 0000 0008 A803 0000 0000 0085 FFFF
60: 0ECA 0017 D9BA 0010 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0001 0602
E0: 0000 0080 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000

Bus : 00 Device: 24 Function : 00 --> 11001022 Vendor : 1022 Device : 1100 (rev 00) - Advanced Micro Devices Athlon 64 / Opteron HyperTransport Technology Configuration
00: 1022 1100 0000 0010 0000 0600 0000 0080 0000 0000 0000 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0080 0000 0000 0000 0000 0000
40: 0101 0001 0101 0001 0101 0001 0101 0001 0101 0001 0101 0001 0101 0001 0101 0001
60: 0000 0000 00E4 0000 CC0F 0F2E 021C 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0008 2101 A820 1111 0522 8035 0002 0000 0169 0170 0000 000F 0007 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000

Bus : 00 Device: 24 Function : 01 --> 11011022 Vendor : 1022 Device : 1101 (rev 00) - Advanced Micro Devices Athlon 64 / Opteron Address Map
00: 1022 1101 0000 0000 0000 0600 0000 0080 0000 0000 0000 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
40: 0003 0000 0000 007F 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
60: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0000 0000 0000 0000 0A03 0000 0B00 0000 0003 0080 FF80 008F 0003 0090 0F00 0092
A0: 1003 0092 2F80 0092 3003 0092 FF00 00F6 0003 00F7 FF80 00F7 0003 00F8 FF00 00FF
C0: 0013 0000 F000 00FF 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0003 0F00 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000

Bus : 00 Device: 24 Function : 02 --> 11021022 Vendor : 1022 Device : 1102 (rev 00) - Advanced Micro Devices Athlon 64 / Opteron DRAM Controller
00: 1022 1102 0000 0000 0000 0600 0000 0080 0000 0000 0000 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
40: 0001 0000 0201 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
60: 3DE0 0078 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0046 0000 0000 0000
80: 0004 0000 0000 0000 CA24 5DA9 1320 0022 0820 0001 006A A700 0010 8000 002D 0000
A0: 06EF 5D00 0000 0000 0000 0000 0000 0000 46C0 AE14 009E 0000 238A 003A 137D 1E32
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0E15 109C 818C 6A2F 0F87 C8E1 1006 105C
E0: 1612 10CC 4586 72E5 19E4 A844 200A 8010 0000 0000 0000 0000 0000 0000 0000 0000

Bus : 00 Device: 24 Function : 03 --> 11031022 Vendor : 1022 Device : 1103 (rev 00) - Advanced Micro Devices Athlon 64 / Opteron Miscellaneous Control
00: 1022 1103 0000 0010 0000 0600 0000 0080 0000 0000 0000 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 00F0 0000 0000 0000 0000 0000
40: 3BFF 0004 0040 0210 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 30C0 2BFE
60: 0040 0000 0000 0000 00C0 0000 0000 0000 0111 5122 4021 5040 2A00 0800 212B 0000
80: 3731 3307 3113 3113 0000 0000 0000 0000 0000 0000 2C00 0000 ECF0 140F 0000 0000
A0: 0096 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 A701 000D 0000 0D40 0025 0000
E0: 0000 0000 0E32 0000 0701 0000 0000 0000 000F 0010 0000 0000 0000 0000 0FC2 0007

Bus : 01 Device: 05 Function : 00 --> 96121002 Vendor : 1002 Device : 9612 (rev 00) - <Unknown device>
00: 1002 9612 0007 0010 0000 0300 0010 0080 0008 8000 7001 0000 0000 9220 0000 0000
20: 0000 0000 0000 9210 0000 0000 1025 028D 0000 0000 0050 0000 0000 0000 0112 0000
40: 0000 0000 0000 0000 0000 0000 1025 028D A001 0603 0000 0000 A010 0012 8FA0 0000
60: 0810 000A 0D01 0000 0000 1101 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0000 0000 0000 0000 0001 0001 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0005 0080 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000

Bus : 02 Device: 00 Function : 00 --> 002B168C Vendor : 168C Device : 002B (rev 01) - <Unknown device>
00: 168C 002B 0147 0010 0001 0280 0010 0000 0004 9110 0000 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 105B E016 0000 0000 0040 0000 0000 0000 0110 0000
40: 5001 5BC3 0000 0000 0000 0000 0000 0000 6005 0000 0000 0000 0000 0000 0000 0000
60: 0010 0012 8CC0 0064 2010 0009 3C11 0003 0042 1011 0000 0000 0000 0000 0000 0000
80: 0000 0000 0010 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000

Bus : 08 Device: 00 Function : 00 --> 10621969 Vendor : 1969 Device : 1062 (rev C0) - <Unknown device>
00: 1969 1062 0007 0010 00C0 0200 0010 0000 0004 9100 0000 0000 2001 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 1025 028D 0000 0000 0040 0000 0000 0000 0111 0000
40: 4801 F9C3 0008 0000 5805 0080 0000 0000 0000 0000 0000 0000 6C10 0001 FF85 0064
60: 2000 001B FC11 0007 0042 1011 0003 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0000 0000 1969 1062 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000

***************************** ISA SCAN

ISA Dump from address $290 --> <Unknown> (ISA at $0290) (No error)
 --> all bytes have the same value ($FF)

***************************** SMBUS SCAN

SMB Dump from address $30 --> <Unknown> (SMBus at $0B00) (No error)
 --> all bytes have the same value ($FF)
SMB Dump from address $31 --> <Unknown> (SMBus at $0B00) (No error)
 --> all bytes have the same value ($FF)
SMB Dump from address $50 --> <RAM> (SMBus at $0B00) (No error)
00: 80 08 08 0D 0A 61 40 00 05 30 45 00 82 10 00 00   .....a@..0E.....
10: 0C 08 38 01 04 00 07 3D 50 50 60 3C 28 3C 2D 80   ..8....=PP`<(<-.
20: 20 27 10 17 3C 1E 1E 00 06 3C 7F 80 18 22 00 00    '..<....<..."..
30: 00 03 00 00 00 00 00 00 00 00 00 00 00 00 12 AC   ................
40: CE 00 00 00 00 00 00 00 02 4D 34 20 37 30 54 32   .........M4 70T2
50: 38 36 34 51 5A 33 2D 43 45 36 20 33 51 09 44 76   864QZ3-CE6 3Q.Dv
60: DF C1 69 00 53 45 48 31 4F 33 38 00 00 00 00 00   ..i.SEH1O38.....
70: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
80: 00 63 43 39 41 30 35 55 FE E0 54 45 00 04 07 00   .cC9A05U..TE....
90: 00 63 43 39 41 30 35 55 FE E0 54 45 00 09 08 00   .cC9A05U..TE....
A0: 00 63 43 39 41 30 35 55 FE E0 54 45 00 04 04 00   .cC9A05U..TE....
B0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
C0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
D0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
E0: 31 2F FF FF FF FF FF FF FF FF FF FF FF FF FF FF   1/..............
F0: 01 FF FF FF FF FF FF FF FF FF FF FF FF FF FF 06   ................
SMB Dump from address $51 --> <RAM> (SMBus at $0B00) (No error)
00: 80 08 08 0D 0A 61 40 00 05 30 45 00 82 10 00 00   .....a@..0E.....
10: 0C 08 38 01 04 00 07 3D 50 50 60 3C 28 3C 2D 80   ..8....=PP`<(<-.
20: 20 27 10 17 3C 1E 1E 00 06 3C 7F 80 18 22 00 00    '..<....<..."..
30: 00 03 00 00 00 00 00 00 00 00 00 00 00 00 12 AC   ................
40: CE 00 00 00 00 00 00 00 02 4D 34 20 37 30 54 32   .........M4 70T2
50: 38 36 34 51 5A 33 2D 43 45 36 20 33 51 09 44 76   864QZ3-CE6 3Q.Dv
60: DF C1 6A 00 53 45 48 31 4F 33 38 00 00 00 00 00   ..j.SEH1O38.....
70: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
80: 00 63 43 39 41 10 35 55 FE E0 54 45 00 04 07 00   .cC9A.5U..TE....
90: 00 63 43 39 41 10 35 55 FE E0 54 45 00 09 08 00   .cC9A.5U..TE....
A0: 00 63 43 39 41 10 35 55 FE E0 54 45 00 04 04 00   .cC9A.5U..TE....
B0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
C0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
D0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
E0: 31 2F FF FF FF FF FF FF FF FF FF FF FF FF FF FF   1/..............
F0: 01 FF FF FF FF FF FF FF FF FF FF FF FF FF FF 07   ................
SMB Device at address $69 --> (SMBus at $0B00) (No error)

***************************** SMBUS RETRIES

Retry attempts info for SMBus at $0B00
  [ -1]=176
  [  1]=176

***************************** SMBUS PAUSES

Pause stats for SMBusAtiIgp@$B00: min=49999 max=49999 avg=49999(4161) touts=0 count=4161

***************************** DIMM INFO

***************************** SMBUS DEVICE SCAN RESULTS

***************************** FAN SPEED CONTROL

Can change fan speeds : NO
Can smoothly change fan speeds : NO
Can stop fans : NO

***************************** WMI SCAN

WMI interface is registered : ON
MB manufacturer: eMachines 
MB model: eMachines E627  
MB version: V1.10
ACPI temp: 38.0
ACPI active trip point: 0.0
ACPI passive trip point: 90.0
ACPI critical trip point: 200.0
WMI quick analysis results -->
EXPLORING : root\CIMV2\Win32_BaseBoard
  -> Object Start
  Caption = Base Board
  ConfigOptions =  String2 for Type12 Equipment Manufacturer String3 for Type12 Equipment Manufacturer String4 for Type12 Equipment Manufacturer
  CreationClassName = Win32_BaseBoard
  Description = Base Board
  HostingBoard = True
  Manufacturer = eMachines 
  Name = Base Board
  PoweredOn = True
  Product = eMachines E627  
  SerialNumber = LXN6402008946055631601
  Tag = Base Board
  Version = V1.10
  Method -> IsCompatible(ElementToCheck)
EXPLORING : root\WMI\msacpi_thermalzonetemperature
  -> Object Start
  Active = True
  ActiveTripPoint =  0 0 0 0 0 0 0 0 0 (0.0C)
  ActiveTripPointCount = 1
  CriticalTripPoint = 4732 (200.0C)
  CurrentTemperature = 3112 (38.0C)
  InstanceName = ACPI\ThermalZone\THRM_0
  PassiveTripPoint = 3632 (90.0C)
  Reserved = 1
  SamplingPeriod = 300
  ThermalConstant1 = 2
  ThermalConstant2 = 5
  ThermalStamp = 6
EXPLORING : root\CIMV2\CIM_AssociatedSensor
EXPLORING : root\CIMV2\CIM_CoolingDevice
EXPLORING : root\CIMV2\CIM_Fan
EXPLORING : root\CIMV2\CIM_HeatPipe
EXPLORING : root\CIMV2\CIM_ManagementController
EXPLORING : root\CIMV2\CIM_NumericSensor
EXPLORING : root\CIMV2\CIM_PackageAlarm
EXPLORING : root\CIMV2\CIM_PackageCooling
EXPLORING : root\CIMV2\CIM_Refrigeration
EXPLORING : root\CIMV2\CIM_Sensor
EXPLORING : root\CIMV2\CIM_Tachometer
EXPLORING : root\CIMV2\CIM_TemperatureSensor
EXPLORING : root\CIMV2\CIM_VoltageSensor
EXPLORING : root\CIMV2\Win32_CurrentProbe
EXPLORING : root\CIMV2\Win32_Fan
EXPLORING : root\CIMV2\Win32_HeatPipe
EXPLORING : root\CIMV2\Win32_Refrigeration
EXPLORING : root\CIMV2\Win32_TemperatureProbe
EXPLORING : root\CIMV2\Win32_VoltageProbe
EXPLORING : SMBIOS
  -> Object Start
Structure 129 - 000D - fixed len is 5 bytes -> Intel_ASF
  -> 4F
  -> <em Test 1>
  -> <Oem Test 2>
Structure  40 - 001E - fixed len is 18 bytes -> Additional information
  -> 02 06 04 00 05 01 AA 07 00 00 05 02 78 05
  -> <PCIExpressx16>
  -> <Compiler Version: VC 8.0>
Structure  41 - 001F - fixed len is 11 bytes -> Onboard devices extended information
  -> 01 85 01 00 00 00 01
  -> <82567LM Gigabit Network Connection>
<-- End of WMI quick analysis results

***************************** DMI SCAN

DMI structures from SMBIOS ver. 2.6
MBManufacturer : eMachines
MBModel : eMachines E627
MBVersion : V1.10
BIOSVendor : eMachines
BIOSVersion : V1.10
SysManufacturer : eMachines
SysProductName : eMachines E627
SysVersion : V1.10
SysSerialNumber : LXN6402008946055631601
Structure   0 - 0000 - fixed len is 20 bytes -> BIOS information
  -> 01 02 00 00 03 0F 80 98 FB 4B 00 00 00 00 03 04 0A F0 FF FF
  -> 'eMachines '
  -> 'V1.10'
  -> '11/30/2009'
Structure   1 - 0001 - fixed len is 23 bytes -> System information
  -> 01 02 03 04 66 62 30 39 63 30 36 35 64 66 00 26 22 7E F2 10 06 05 06
  -> 'eMachines '
  -> 'eMachines E627  '
  -> 'V1.10'
  -> 'LXN6402008946055631601'
  -> '123456789'
  -> 'Type1Family'
Structure   2 - 0002 - fixed len is 12 bytes -> Base board (or module) information
  -> 01 02 03 04 05 09 06 03 00 0A 00 00
  -> 'eMachines '
  -> 'eMachines E627  '
  -> 'V1.10'
  -> 'LXN6402008946055631601'
  -> '                 '
  -> 'Base Board Chassis Location'
Structure   3 - 0003 - fixed len is 18 bytes -> System enclosure or chassis
  -> 01 0A 02 03 04 03 03 03 03 00 00 00 00 00 01 00 00 00
  -> 'eMachines '
  -> 'V1.10'
  -> 'LXN6402008946055631601'
  -> '                 '
Structure   9 - 0004 - fixed len is 13 bytes -> System slots
  -> 01 AA 0D 03 04 01 00 04 03 00 00 00 10
  -> 'J6C1'
Structure   9 - 0005 - fixed len is 13 bytes -> System slots
  -> 01 A6 08 03 03 02 00 04 03 00 00 00 20
  -> 'J8C1'
Structure   9 - 0006 - fixed len is 13 bytes -> System slots
  -> 01 A6 08 03 03 03 00 04 03 00 00 00 28
  -> 'J7C1'
Structure   9 - 0007 - fixed len is 13 bytes -> System slots
  -> 01 A6 08 03 03 04 00 04 03 00 00 00 30
  -> 'J8D1'
Structure   9 - 0008 - fixed len is 13 bytes -> System slots
  -> 01 06 05 03 04 05 00 A6 05 00 00 00 A4
  -> 'J8B1'
Structure  11 - 0009 - fixed len is 1 bytes -> OEM strings
  -> 05
  -> 'String1 for Original Equipment Manufacturer'
  -> 'String2 for Original Equipment Manufacturer'
  -> 'String3 for Original Equipment Manufacturer'
  -> 'String4 for Original Equipment Manufacturer'
  -> 'String5 for Original Equipment Manufacturer'
Structure  12 - 000A - fixed len is 1 bytes -> System configuration options
  -> 04
  -> 'String1 for Type12 Equipment Manufacturer'
  -> 'String2 for Type12 Equipment Manufacturer'
  -> 'String3 for Type12 Equipment Manufacturer'
  -> 'String4 for Type12 Equipment Manufacturer'
Structure  21 - 000B - fixed len is 3 bytes -> Built-in pointing device
  -> 07 04 04
Structure  32 - 000C - fixed len is 16 bytes -> System boot information
  -> 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
Structure 129 - 000D - fixed len is 1 bytes -> Intel_ASF
  -> 4F
  -> 'em Test 1'
  -> 'Oem Test 2'
Structure  40 - 001E - fixed len is 14 bytes -> Additional information
  -> 02 06 04 00 05 01 AA 07 00 00 05 02 78 05
  -> 'PCIExpressx16'
  -> 'Compiler Version: VC 8.0'
Structure  41 - 001F - fixed len is 7 bytes -> Onboard devices extended information
  -> 01 85 01 00 00 00 01
  -> '82567LM Gigabit Network Connection'
Structure   4 - 0020 - fixed len is 38 bytes -> Processor information
  -> 03 03 83 02 C2 0F 07 00 FF FB 8B 07 01 8A C8 00 40 06 40 06 41 16 21 00 22 00 23 00 05 04 06 00 01 01 04 00 83 00
  -> 'AMD Athlon(tm) Processor TF-20'
  -> 'AMD processor'
  -> 'Socket S1G1'
  -> 'FFFF'
  -> 'NotSupport'
  -> 'FFFF'
Structure  16 - 0024 - fixed len is 11 bytes -> Physical memory array
  -> 03 03 03 00 00 20 00 FF FF 04 00
Structure  17 - 0025 - fixed len is 24 bytes -> Memory device
  -> 24 00 26 00 40 00 40 00 00 04 09 FF 01 02 13 80 00 4D 01 03 04 05 06 00
  -> 'DIMM0'
  -> 'BANK0'
  -> 'Samsung'
  -> 'CE0000000000000002094476DFC169'
  -> 'Unknown'
  -> 'M4 70T2864QZ3-CE6 '
Structure  18 - 0026 - fixed len is 19 bytes -> 32-bit memory error information
  -> 03 02 02 00 00 00 00 00 00 00 80 00 00 00 80 00 00 00 80
Structure   6 - 0027 - fixed len is 8 bytes -> Memory module information
  -> 01 FF 03 02 01 2B 2B 00
  -> 'DIMM0'
Structure  20 - 0028 - fixed len is 15 bytes -> Memory device mapped address
  -> 00 00 00 00 FF FF 0F 00 25 00 32 00 01 00 00
Structure  17 - 0029 - fixed len is 24 bytes -> Memory device
  -> 24 00 2A 00 40 00 40 00 00 04 09 FF 01 02 13 80 00 4D 01 03 04 05 06 00
  -> 'DIMM1'
  -> 'BANK0'
  -> 'Samsung'
  -> 'CE0000000000000002094476DFC16A'
  -> 'Unknown'
  -> 'M4 70T2864QZ3-CE6 '
Structure  18 - 002A - fixed len is 19 bytes -> 32-bit memory error information
  -> 03 02 02 00 00 00 00 00 00 00 80 00 00 00 80 00 00 00 80
Structure   6 - 002B - fixed len is 8 bytes -> Memory module information
  -> 01 FF 03 02 01 2B 2B 00
  -> 'DIMM1'
Structure  20 - 002C - fixed len is 15 bytes -> Memory device mapped address
  -> 00 00 10 00 FF FF 1F 00 29 00 32 00 01 00 00
Structure  17 - 002D - fixed len is 24 bytes -> Memory device
  -> 24 00 FE FF 00 00 00 00 00 00 09 00 01 02 13 00 00 00 00 00 00 03 00 00
  -> 'DIMM2'
  -> 'BANK0'
  -> 'Unknown'
Structure   6 - 002E - fixed len is 8 bytes -> Memory module information
  -> 01 FF 00 02 01 7F 7F 00
  -> 'DIMM2'
Structure  17 - 002F - fixed len is 24 bytes -> Memory device
  -> 24 00 FE FF 00 00 00 00 00 00 09 00 01 02 13 00 00 00 00 00 00 03 00 00
  -> 'DIMM3'
  -> 'BANK0'
  -> 'Unknown'
Structure   6 - 0030 - fixed len is 8 bytes -> Memory module information
  -> 01 FF 00 02 01 7F 7F 00
  -> 'DIMM3'
Structure  18 - 0031 - fixed len is 19 bytes -> 32-bit memory error information
  -> 03 02 02 00 00 00 00 00 00 00 80 00 00 00 80 00 00 00 80
Structure  19 - 0032 - fixed len is 11 bytes -> Memory array mapped address
  -> 00 00 00 00 FF FF 1F 00 24 00 04
Structure   5 - 0033 - fixed len is 16 bytes -> Memory controller information
  -> 03 06 03 03 0C 01 00 01 00 00 02 27 00 2B 00 04
Structure 127 - 0034 - fixed len is 0 bytes -> End of table
  -> 

***************************** EVENTS

0 events defined

***************************** EXTRA UNCATEGORIZED INFO

Tray icon size : 16x16
UPTIME : 0 days 12:32:14
SpeedFan UPTIME : 0 days 00:40:07

***************************** MAIN WINDOW INFO

Win9x:NO  64Bit:NO  GiveIO:YES  SpeedFan:YES
I/O properly initialized
Linked ISA BUS at $0290
Linked ATI SBx00 SMBUS at $0B00
Scanning ISA BUS at $0290...
Scanning AtiIgp SMBus at $0B00...
Found Hitachi HTS545016B9A300 on AdvSMART
Found ACPI temperature (38.0C)
End of detection
Loaded 0 events

***************************** DEBUG INFO

Win9x:NO  64Bit:NO  GiveIO:YES  SpeedFan:YES
SpeedFan.sys ver. 1.002
  -> Can read memory
  -> Can read MSR
  -> Can't map memory
About to do a test on INTEL MSRs...
End of INTEL MSR test
I/O properly initialized
Linked ISA BUS at $0290
Linked PCI
Starting PCI scan...
Linked ATI SBx00 SMBUS at $0B00
PCI scan done!
Scanning ISA BUS at $0290...
Second pass...
Checking $002E for ITE (1)...
ITE Registers [$002E] : $FF $FF $FF
Checking $0370 for SMSC (2)...
Checking $0370 for SMSC (1)...
Checking $03F0 for SMSC (2)...
Checking $03F0 for SMSC (1)...
Checking $002E for SMSC (1)...
Checking $004E for SMSC (1)...
Checking $002E for WINBOND...
Checking $004E for WINBOND...
Checking $0250 for WINBOND...
Checking $0370 for WINBOND...
Checking $03F0 for WINBOND...
Checking $002E for NS...
Checking $004E for NS...
INFO: ISA seems to be unused
About to check DELL support
PCI scanning is enabled
Intel SouthBridge found
End of DELL support check
Scanning AtiIgp SMBus at $0B00...
Something is at address $30
Something is at address $31
Something is at address $50
About to probe Intel QST...
End of Intel QST probing
About to probe Intel FB-DIMM support...
End of Intel FB-DIMM support probing
About to probe TOSHIBA SUPPORT...
End of TOSHIBA SUPPORT probing
About to probe Areca RAID support...
ARECA : interface properly linked
ARECA : 0 Areca RAID controller(s) found
End of Areca RAID probing
About to probe 3ware RAID support...
DLL properly linked
API version is <2.04.00.003>
3ware Controllers found : 0
End of 3ware RAID probing
About to probe SMART (Advanced Methods)...
AdvSMART debug messages start -->
WBEM Locator creation took 47 ms to execute
Server Connect took 93 ms to execute
Find USB Controllers took 452 ms to execute
DeviceID=PCI\VEN_1002&DEV_4397&SUBSYS_028D1025&REV_00\3&2411E6FE&0&90
Name=Standard OpenHCD USB Host Controller
Find USB Controllers' Associators took 140 ms to execute
  DeviceID=USB\ROOT_HUB\4&2B3AF8B0&0
  Name=USB Root Hub
DeviceID=PCI\VEN_1002&DEV_4398&SUBSYS_028D1025&REV_00\3&2411E6FE&0&91
Name=Standard OpenHCD USB Host Controller
Find USB Controllers' Associators took 46 ms to execute
  DeviceID=USB\ROOT_HUB\4&50F771C&0
  Name=USB Root Hub
DeviceID=PCI\VEN_1002&DEV_4396&SUBSYS_028D1025&REV_00\3&2411E6FE&0&92
Name=Standard Enhanced PCI to USB Host Controller
Find USB Controllers' Associators took 31 ms to execute
  DeviceID=USB\ROOT_HUB20\4&226161B2&0
  Name=USB Root Hub
  DeviceID=USB\VID_0BDA&PID_0159\20071114173400000
  Name=USB Mass Storage Device
  DeviceID=USBSTOR\DISK&VEN_GENERIC-&PROD_MULTI-CARD&REV_1.00\20071114173400000&0
    --> USB disk found
        Owner Device Id is USB\VID_0BDA&PID_0159\20071114173400000
        VID=$0BDA  PID=$0159
  Name=Generic- Multi-Card USB Device
  DeviceID=STORAGE\REMOVABLEMEDIA\7&24E8D74F&0&RM
  Name=Generic volume
USB Drive Search took 718 ms to execute
Find 1394 Controllers took 15 ms to execute
1394 Drive Search took 31 ms to execute
Find Disk Drives took 31 ms to execute
 
BytesPerSector=512
Caption=Hitachi HTS545016B9A300
DeviceID=\\.\PHYSICALDRIVE0
InterfaceType=IDE
MediaLoaded=True
Model=Hitachi HTS545016B9A300
Name=\\.\PHYSICALDRIVE0
Partitions=3
SCSIBus=0
SCSILogicalUnit=0
SCSIPort=0
SCSITargetId=0
Trying Physical access...
Using TSmartHardDiskPhysical
    Identify Sector -->
      000  5A 04 FF 3F 37 C8 10 00 00 00 00 00 3F 00 00 00 00 00 00 00 30 39 31 30 32 36 50 42 50 42 30 36 Z.ÿ?7È......?.......091026PBPB06
      020  51 43 44 35 4A 56 33 4C 03 00 50 38 04 00 50 42 42 4F 43 36 30 46 48 69 74 61 63 68 69 20 48 54 QCD5JV3L..P8..PBBOC60FHitachi HT
      040  53 35 34 35 30 31 36 42 39 41 33 30 30 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 10 80 S545016B9A300                 .€
      060  00 40 00 0F 00 40 00 02 00 02 07 00 FF 3F 10 00 3F 00 10 FC FB 00 10 01 FF FF FF 0F 00 00 07 00 .@...@......ÿ?..?..üû...ÿÿÿ.....
      080  03 00 78 00 78 00 78 00 78 00 00 00 00 00 00 00 00 00 00 00 00 00 1F 00 06 17 00 00 5E 00 40 00 ..x.x.x.x...................^.@.
      0A0  FC 01 28 00 6B 74 69 7F 63 61 69 74 49 BC 63 61 7F 40 20 00 21 00 80 40 FE FF 00 00 FE 80 00 00 ü.(.kticaitI¼ca@ .!.€@þÿ..þ€..
      0C0  00 00 00 00 00 00 00 00 B0 9E A1 12 00 00 00 00 00 00 00 00 00 00 48 88 00 50 A5 CC D0 A2 95 9C ........°ž¡...........Hˆ.P¥ÌÐ¢•œ
      0E0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 1C 40 1C 40 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ...............@.@..............
      100  29 00 0B 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 )...............................
      120  00 00 00 00 00 00 00 00 01 40 00 00 00 80 00 00 4F 42 00 00 00 00 A9 B8 E5 E5 00 00 00 00 00 00 .........@...€..OB....©¸åå......
      140  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 03 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................................
      160  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................................
      180  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 3D 00 00 00 ............................=...
      1A0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 18 15 00 00 00 00 00 00 00 00 1F 10 21 00 ..............................!.
      1C0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 01 00 C7 02 00 00 00 00 00 00 00 00 ......................Ç.........
      1E0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 A5 26 ..............................¥&
      SMART checksum is $00
      000  10 00 01 0B 00 64 64 00 00 00 00 00 00 00 02 05 00 64 64 00 00 00 00 00 00 00 03 07 00 C8 C8 01
      020  00 00 00 0F 00 00 04 12 00 64 64 A4 02 00 00 00 00 00 05 33 00 64 64 00 00 00 00 00 00 00 07 0B
      040  00 64 64 00 00 00 00 00 00 00 08 05 00 64 64 00 00 00 00 00 00 00 09 12 00 5E 5E A6 0A 00 00 00
      060  00 00 0A 13 00 64 64 00 00 00 00 00 00 00 0C 32 00 64 64 5C 02 00 00 00 00 00 BF 0A 00 62 62 03
      080  00 01 00 00 00 00 C0 32 00 64 64 0F 00 00 00 00 00 00 C1 12 00 62 62 E8 4E 00 00 00 00 00 C2 02
      0A0  00 82 82 2A 00 0C 00 32 00 00 C4 32 00 64 64 00 00 00 00 00 00 00 C5 22 00 64 64 00 00 00 00 00
      0C0  00 00 C6 08 00 64 64 00 00 00 00 00 00 00 C7 0A 00 C8 C8 00 00 00 00 00 00 00 DF 0A 00 64 64 00
      0E0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      100  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      120  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      140  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      160  00 00 00 00 00 00 00 00 00 00 00 00 85 02 01 5B 03 00 01 00 02 41 00 00 00 00 00 00 00 00 00 00
      180  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      1A0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      1C0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      1E0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 0A
    Smart Log Directory -->
      000  01 00 01 00 01 00 00 00 00 00 00 00 01 00 00 00 00 00 01 00 00 00 00 00 00 00 00 00 00 00 00 00
      020  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      040  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      060  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      080  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      0A0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      0C0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      0E0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      100  10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00
      120  10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00
      140  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      160  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      180  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      1A0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      1C0  01 00 01 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      1E0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      Smart Logging Version=$0001
      Log #$01 contains 1 pages
      Log #$02 contains 1 pages
      Log #$06 contains 1 pages
    Smart Summary Error Log -->
      000  01 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      020  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      040  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      060  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      080  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      0A0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      0C0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      0E0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      100  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      120  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      140  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      160  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      180  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      1A0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      1C0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      1E0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 FF
      Error Log Version=$0001
      Error Log Index=0
      Device Error Count=0
    Smart Self-Test Log -->
      000  01 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      020  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      040  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      060  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      080  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      0A0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      0C0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      0E0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      100  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      120  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      140  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      160  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      180  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      1A0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      1C0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      1E0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 FF
      Revision=$0001
      Self-Test Index=0
 
BytesPerSector=512
Caption=Generic- Multi-Card USB Device
DeviceID=\\.\PHYSICALDRIVE1
InterfaceType=USB
MediaLoaded=True
Model=Generic- Multi-Card USB Device
Name=\\.\PHYSICALDRIVE1
Partitions=1
\\.\PHYSICALDRIVE1 (Generic- Multi-Card USB Device) - VID=$0BDA  PID=$0159
Trying Physical access...
Using TSmartHardDiskPhysical
  Error identifying using TSmartHardDiskPhysical
  Error reading attrs using TSmartHardDiskPhysical
Freeing HD (Physical) as it reports no SMART
Looking for Guessed USB access...
Using TSmartHardDiskSatCypress
    Identify Sector -->
      SMART Revision is $0000
      Bad attributes using TSmartHardDiskSatCypress
Freeing HD (Guessed USB) as it reports no SMART
Disk Objects Creation took 655 ms to execute
AdvSMART debug messages end <--
SMART Hard disks found: 1
Found Hitachi HTS545016B9A300 on AdvSMART
  HD00 -> <\\.\PHYSICALDRIVE0> (Physical) Model: <Hitachi HTS545016B9A300> - Firmware: <PBBOC60F> - Serial: <091026PBPB06QCD5JV3L>
    AAM:supported (currently disabled)
    APM:supported (currently enabled)
    Power Management:supported (currently enabled)
    SMART:supported (currently enabled)
    48-bit Addressing:supported
    Max Queue Depth=32
    NCQ:supported
    SATA I (1.5Gb/s):unsupported
    SATA II (3.0Gb/s):supported
    UDMA0:supported (currently disabled)
    UDMA1:supported (currently disabled)
    UDMA2:supported (currently disabled)
    UDMA3:supported (currently disabled)
    UDMA4:supported (currently disabled)
    UDMA5:supported (currently disabled)
    UDMA6:supported (currently enabled)
SMART Structure Revision : $0010
ID=$01  NAME=Raw Read Error Rate  VALUE=$64  WORST=$64  RAW=$000000000000  THRSHLD=$3E  FLAGS=$000B
ID=$02  NAME=Throughput Performance  VALUE=$64  WORST=$64  RAW=$000000000000  THRSHLD=$28  FLAGS=$0005
ID=$03  NAME=Spin Up Time  VALUE=$C8  WORST=$C8  RAW=$000F00000001  THRSHLD=$21  FLAGS=$0007
ID=$04  NAME=Start/Stop Count  VALUE=$64  WORST=$64  RAW=$0000000002A4  THRSHLD=$00  FLAGS=$0012
ID=$05  NAME=Reallocated Sector Count  VALUE=$64  WORST=$64  RAW=$000000000000  THRSHLD=$05  FLAGS=$0033
ID=$07  NAME=Seek Error Rate  VALUE=$64  WORST=$64  RAW=$000000000000  THRSHLD=$43  FLAGS=$000B
ID=$08  NAME=Seek Time Performance  VALUE=$64  WORST=$64  RAW=$000000000000  THRSHLD=$28  FLAGS=$0005
ID=$09  NAME=Power On Hours Count  VALUE=$5E  WORST=$5E  RAW=$000000000AA6  THRSHLD=$00  FLAGS=$0012
ID=$0A  NAME=Spin Retry Count  VALUE=$64  WORST=$64  RAW=$000000000000  THRSHLD=$3C  FLAGS=$0013
ID=$0C  NAME=Power Cycle Count  VALUE=$64  WORST=$64  RAW=$00000000025C  THRSHLD=$00  FLAGS=$0032
ID=$BF  NAME=GSense Error Rate  VALUE=$62  WORST=$62  RAW=$000000010003  THRSHLD=$00  FLAGS=$000A
ID=$C0  NAME=Power Off Retract Count  VALUE=$64  WORST=$64  RAW=$00000000000F  THRSHLD=$00  FLAGS=$0032
ID=$C1  NAME=Load Cycle Count  VALUE=$62  WORST=$62  RAW=$000000004EE8  THRSHLD=$00  FLAGS=$0012
ID=$C2  NAME=Temperature  VALUE=$82  WORST=$82  RAW=$0032000C002A  THRSHLD=$00  FLAGS=$0002
Current HD temperature is 42C
ID=$C4  NAME=Reallocated Event Count  VALUE=$64  WORST=$64  RAW=$000000000000  THRSHLD=$00  FLAGS=$0032
ID=$C5  NAME=Current Pending Sector Count  VALUE=$64  WORST=$64  RAW=$000000000000  THRSHLD=$00  FLAGS=$0022
ID=$C6  NAME=Uncorrectable Sector Count  VALUE=$64  WORST=$64  RAW=$000000000000  THRSHLD=$00  FLAGS=$0008
ID=$C7  NAME=UltraATA CRC Error Rate  VALUE=$C8  WORST=$C8  RAW=$000000000000  THRSHLD=$00  FLAGS=$000A
ID=$DF  NAME=Load/Unload Retry Count  VALUE=$64  WORST=$64  RAW=$000000000000  THRSHLD=$00  FLAGS=$000A
Adding drive #0 (Hitachi HTS545016B9A300) found on AdvSMART
Linked AdvSMART
 -> Temperature 1 offset : 0
End of SMART (Advanced Methods) probing
Version 1.1 84 00000007
SMART Enabled for drive 0
 --> S.M.A.R.T. attributes properly read
 --> S.M.A.R.T. thresholds properly read
Start of DEBUG DATA for drive 0
--> cylinders : 19457
--> tracks per cilinder : 255
--> sectors per track : 63
--> bytes per sector : 512
--> disk size : 160.0
End of DEBUG DATA for drive 0
Found Hitachi HTS545016B9A300 Firmware revision <PBBOC60F> (160.0GB) Serial <091026PBPB06QCD5JV3L>
 --> Drive already linked
21:17:25.875 About to probe SCSI...
21:17:25.875 ProbeSCSI: before first LogSense
21:17:25.875 ProbeSCSI: before first LogSense
21:17:25.890 End of SCSI probing
About to probe UGURU support...
Motherboard is eMachines eMachines E627
End of UGURU support probing
About to probe ACPI temperatures...
Found ACPI temperature (38.0C)
 -> Temperature 1 offset : 0
End of ACPI temperatures probing
About to probe AMD Internal Sensors...
Found AMD Athlon(tm) Processor TF-20 internal sensor for K8 CPU#0 : -49C
 -> [$E4]=$00000E32
 -> TCaseMax=49
 -> Core=0
 -> Sensor=0
 -> Offset=14
 -> Temperature 1 offset : 0
End of AMD Internal Sensors probing
About to probe INTEL Internal Sensors...
End of INTEL Internal Sensors probing
About to probe NVIDIA ControlPanel Sensors...
End of NVIDIA ControlPanel Sensors probing
End of detection
Reading Cfg Version 2.01
Old sensor properly detected -->
  HD0 (160.0GB) on AdvSMART @ $0
Old sensor properly detected -->
  ACPI on ISA @ $0
Old sensor properly detected -->
  AMD K8 on PCI @ $0
Temperature from Hitachi HTS545016B9A300091026PBPB06QCD5JV3L -->
  HD0 40 50 0
  properly added
Temperature from ACPI -->
  Temp1 40 50 0
  properly added
Temperature from AMD K8@$0(onPCI@$0) -->
  Core 40 50 0
  properly added
Loaded 0 events
Preparing report...