Sender : Until_It_Sleeps-enwiki@comcast.net
SpeedFan version : SpeedFan 4.40
Motherboard model : ECS MCP61PM-GM 

***************************** BIOS INFO

BIOS CopyRight : GATEWA - 42302e31
BIOS Date : 10/29/08
BIOS Extended Info : 
BIOS Name : AT/AT COMPATIBLE

Windows NT Multiprocessor Free version 6.1.7600 (Windows 7)

2 processor(s)
Advanced Micro Devices AMD Athlon(tm) Dual Core Processor 4050e family 15 model 11 stepping 2 brand 0 2064 MHz
Running at 2109 MHz
I Agree to receive beta versions : ON

***************************** CPUID INFO

CPU Name : AMD Athlon(tm) Dual Core Processor 4050e
 - Identified CPU Name : AMD Athlon(tm) Dual Core Processor 4050e
 - Vendor : AuthenticAMD
 - Family : 15
 - Model : 107
 - Stepping : 2
 - L1 Data Cache : 128 KB (2 x 64 KB) 2-way
 - L1 Instruction Cache : 128 KB (2 x 64 KB) 2-way
 - L2 Cache : 1 MB (2 x 512 KB) 16-way
 - Core Name : Brisbane 
 - Die Revision : BH-G2 
 - Socket Type : Socket AM2
 - Manufacturing Technology : 65 nm
 - Voltage : 1.150-1.250 V
 - BUS Speed : 1 GHz
 - Max cpu speed : 2100 MHz
 - Core Multi-processing Legacy Mode : yes
 - Cores : 2
 - CPUs in system : 1
 - Secure Virtual Machine Feature : yes
 - Temperature Sensor : yes
 - Frequency ID Control : yes
 - Voltage ID Control : yes
 - Hardware P-State Control : no
 - Hardware Thermal Control : yes
 - Software Thermal Control : yes
 - THERMTRIP : yes
 - TDP : 45.0 W
 - Execute Disable : yes
 - Hyper-Threading Technology : yes
$00000000 - $00000001 $68747541 $444D4163 $69746E65 - .... Auth cAMD enti
$80000000 - $80000018 $68747541 $444D4163 $69746E65 - .... Auth cAMD enti
$00000001 - $00060FB2 $00020800 $00002001 $178BFBFF - .... .... . .. ....
$80000001 - $00060FB2 $00004E4F $0000011F $EBD3FBFF - .... ON.. .... ....
$80000002 - $20444D41 $6C687441 $74286E6F $4420296D - AMD  Athl on(t m) D
$80000003 - $206C6175 $65726F43 $6F725020 $73736563 - ual  Core  Pro cess
$80000004 - $3420726F $65303530 $00002020 $00000000 - or 4 050e   .. ....
$80000005 - $FF08FF08 $FF20FF20 $40020140 $40020140 - ....  . . @..@ @..@
$80000006 - $00000000 $42004200 $02008140 $00000000 - .... .B.B @... ....
$80000007 - $00000000 $00000000 $00000000 $0000007F - .... .... .... ...
$80000008 - $00003028 $00000000 $00000001 $00000000 - (0.. .... .... ....
 - DEBUG : MSRC0010015=$0000000002000041  MSRC0010042=$310C160E0C0D020D  MSRC0010071=$FFFFFFFFFFFFFFFF
 -         AnalyzeFamilyF: BrandId=$4E4F BaseModel=$0B PwrLmt=$03 BTI=$07 NN=$0F Socket=$03 CmpCap=$01 TDP=0
 -         AnalyzeFamilyF: CurrFID=10.5 StartFID=5.0 MaxFID=10.5 - CurrVID=1.2000 StartVID=1.0000 MaxVID=1.2500
 -         !!!STRONG CHECK (CPUSPEED) Name='4450e' sSPEC='' CpuSpeed=2.300 BusSpeed=1000 Ratio=11.5 TDP=45.00 ThermSpec=0.0 VMin=1.1500 VMax=1.2500 Socket='Socket AM2' Tech='65 nm' Core='brisbane' Revision='BH-G2'
 -         !!!STRONG CHECK (CPUSPEED) Name='4450B' sSPEC='' CpuSpeed=2.300 BusSpeed=1000 Ratio=11.5 TDP=45.00 ThermSpec=0.0 VMin=1.1500 VMax=1.2500 Socket='Socket AM2' Tech='65 nm' Core='brisbane' Revision='BH-G2'
 -         !!!STRONG CHECK (CPUSPEED) Name='4850e' sSPEC='' CpuSpeed=2.500 BusSpeed=1000 Ratio=12.5 TDP=45.00 ThermSpec=0.0 VMin=1.1500 VMax=1.2500 Socket='Socket AM2' Tech='65 nm' Core='brisbane' Revision='BH-G2'
 -         !!!STRONG CHECK (CPUTYPE) Name='4200+' sSPEC='' CpuSpeed=2.200 BusSpeed=1000 Ratio=11.0 TDP=65.00 ThermSpec=0.0 VMin=1.3250 VMax=1.3750 Socket='Socket AM2' Tech='65 nm' Core='brisbane EE' Revision='BH-G2'
 -         !!!STRONG CHECK (CPUTYPE) Name='4400+' sSPEC='' CpuSpeed=2.300 BusSpeed=1000 Ratio=11.5 TDP=65.00 ThermSpec=0.0 VMin=1.3250 VMax=1.3750 Socket='Socket AM2' Tech='65 nm' Core='brisbane EE' Revision='BH-G2'
 -         !!!STRONG CHECK (CPUTYPE) Name='4600+' sSPEC='' CpuSpeed=2.400 BusSpeed=1000 Ratio=12.0 TDP=65.00 ThermSpec=0.0 VMin=1.3250 VMax=1.3750 Socket='Socket AM2' Tech='65 nm' Core='brisbane EE' Revision='BH-G2'
 -         !!!STRONG CHECK (CPUTYPE) Name='4800+' sSPEC='' CpuSpeed=2.500 BusSpeed=1000 Ratio=12.5 TDP=65.00 ThermSpec=0.0 VMin=1.3250 VMax=1.3750 Socket='Socket AM2' Tech='65 nm' Core='brisbane EE' Revision='BH-G2'
 -         !!!STRONG CHECK (CPUTYPE) Name='5000+' sSPEC='' CpuSpeed=2.600 BusSpeed=1000 Ratio=13.0 TDP=65.00 ThermSpec=0.0 VMin=1.3250 VMax=1.3750 Socket='Socket AM2' Tech='65 nm' Core='brisbane EE' Revision='BH-G2'
 -         !!!STRONG CHECK (CPUTYPE) Name='5000+ Black Edition' sSPEC='' CpuSpeed=2.600 BusSpeed=1000 Ratio=13.0 TDP=65.00 ThermSpec=0.0 VMin=1.2500 VMax=1.3500 Socket='Socket AM2' Tech='65 nm' Core='brisbane EE' Revision='BH-G2'
 -         !!!STRONG CHECK (CPUTYPE) Name='5200+' sSPEC='' CpuSpeed=2.700 BusSpeed=1000 Ratio=13.5 TDP=65.00 ThermSpec=0.0 VMin=1.3250 VMax=1.3750 Socket='Socket AM2' Tech='65 nm' Core='brisbane EE' Revision='BH-G2'
 -         !!!STRONG CHECK (CPUTYPE) Name='5400+' sSPEC='' CpuSpeed=2.800 BusSpeed=1000 Ratio=14.0 TDP=65.00 ThermSpec=0.0 VMin=1.3250 VMax=1.3750 Socket='Socket AM2' Tech='65 nm' Core='brisbane EE' Revision='BH-G2'
 -         !!!STRONG CHECK (CPUTYPE) Name='5600+' sSPEC='' CpuSpeed=2.900 BusSpeed=1000 Ratio=14.5 TDP=65.00 ThermSpec=0.0 VMin=1.3250 VMax=1.3750 Socket='Socket AM2' Tech='65 nm' Core='brisbane EE' Revision='BH-G2'

***************************** SENSORS' READINGS

GeForce Video Card on PCI at $0 GPU : 0.0   min=0.0   max=0.0   mean=0.0
IT8712F-J on ISA at $290 Temp1 : 17.0   min=16.0   max=23.0   mean=17.1
IT8712F-J on ISA at $290 Temp2 : 34.0   min=34.0   max=34.0   mean=34.0
IT8712F-J on ISA at $290 Temp3 : 22.0   min=22.0   max=22.0   mean=22.0
IT8712F-J on ISA at $290 Fan1 : 1588   min=1577   max=1596   mean=1588
IT8712F-J on ISA at $290 Fan2 : 0   min=0   max=0   mean=0
IT8712F-J on ISA at $290 Fan3 : 0   min=0   max=0   mean=0
IT8712F-J on ISA at $290 Fan4 : 0   min=0   max=0   mean=0
IT8712F-J on ISA at $290 Fan5 : 0   min=0   max=0   mean=0
IT8712F-J on ISA at $290 Pwm1 : 30%   min=30%   max=30%   mean=30%
IT8712F-J on ISA at $290 Pwm2 : 0%   min=0%   max=0%   mean=0%
IT8712F-J on ISA at $290 Pwm3 : 0%   min=0%   max=0%   mean=0%
IT8712F-J on ISA at $290 Pwm4 : 0%   min=0%   max=0%   mean=0%
IT8712F-J on ISA at $290 Pwm5 : 0%   min=0%   max=0%   mean=0%
IT8712F-J on ISA at $290 Vcore1 : 1.20   min=1.20   max=1.22   mean=1.20
IT8712F-J on ISA at $290 Vcore2 : 2.50   min=2.50   max=2.50   mean=2.50
IT8712F-J on ISA at $290 +3.3V : 1.79   min=1.79   max=1.79   mean=1.79
IT8712F-J on ISA at $290 +5V : 5.64   min=5.62   max=5.64   mean=5.64
IT8712F-J on ISA at $290 +12V : 12.16   min=12.16   max=12.16   mean=12.16
IT8712F-J on ISA at $290 -12V : -10.96   min=-10.96   max=-10.96   mean=-10.96
IT8712F-J on ISA at $290 -5V : 0.27   min=0.22   max=0.27   mean=0.27
IT8712F-J on ISA at $290 +5V : 5.08   min=5.05   max=5.08   mean=5.08
IT8712F-J on ISA at $290 Vbat : 3.07   min=3.07   max=3.07   mean=3.07
HD0 (500.1GB) on AdvSMART at $0 HD0 : 32.0   min=32.0   max=32.0   mean=32.0
ST3500410AS (drive 0) : fitness=92%   performance=92%
HD1 (320.1GB) on AdvSMART at $1 HD1 : 35.0   min=35.0   max=35.0   mean=35.0
WDC WD3200AAJS-22L7A0 (drive 1) : fitness=94%   performance=94%
ACPI on ISA at $0 Temp1 : 40.0   min=40.0   max=40.0   mean=40.0
AMD K8 on PCI at $0 Core : 10.0   min=7.0   max=15.0   mean=9.5

***************************** SENSORS' ASSOCIATIONS AND GENERAL CONFIG OPTIONS

Temp1 --> active=ON  chip=1  index=1 wanted=40  warning=50  offset=0  InTray=OFF Used pwms=1 2 3 4 5 
Temp2 --> active=ON  chip=1  index=2 wanted=40  warning=50  offset=0  InTray=OFF Used pwms=1 2 3 4 5 
Temp3 --> active=ON  chip=1  index=3 wanted=40  warning=50  offset=0  InTray=OFF Used pwms=1 2 3 4 5 
Core --> active=ON  chip=5  index=1 wanted=40  warning=50  offset=0  InTray=OFF Used pwms=1 2 3 4 5 
HD0 --> active=ON  chip=2  index=1 wanted=40  warning=50  offset=0  InTray=OFF Used pwms=1 2 3 4 5 
HD1 --> active=ON  chip=3  index=1 wanted=40  warning=50  offset=0  InTray=OFF Used pwms=1 2 3 4 5 
Temp1 --> active=ON  chip=4  index=1 wanted=40  warning=50  offset=0  InTray=OFF Used pwms=1 2 3 4 5 
GPU --> active=ON  chip=0  index=1 wanted=40  warning=50  offset=0  InTray=ON Used pwms=1 2 3 4 5 
Fan1 --> active=ON  chip=1  index=1
Fan2 --> active=ON  chip=1  index=2
Fan3 --> active=ON  chip=1  index=3
Fan4 --> active=ON  chip=1  index=4
Fan5 --> active=ON  chip=1  index=5
Speed01 --> active=ON  chip=1  index=1  min=0  max=100  variate=OFF
Speed02 --> active=ON  chip=1  index=2  min=0  max=100  variate=OFF
Speed03 --> active=ON  chip=1  index=3  min=0  max=100  variate=OFF
Speed04 --> active=ON  chip=1  index=4  min=0  max=100  variate=OFF
Speed05 --> active=ON  chip=1  index=5  min=0  max=100  variate=OFF
Vcore1 --> active=ON  chip=1  index=1
Vcore2 --> active=ON  chip=1  index=2
+3.3V --> active=ON  chip=1  index=3
+5V --> active=ON  chip=1  index=4
+12V --> active=ON  chip=1  index=5
-12V --> active=ON  chip=1  index=6
-5V --> active=ON  chip=1  index=7
+5V --> active=ON  chip=1  index=8
Vbat --> active=ON  chip=1  index=9
Set Fans to 100% on exit : OFF
Debug Mode : OFF
Use ISA : ON
Use SMB : ON
Scan PCI : ON
Scan SMB : ON
Slow SMB detection : OFF
Detect SuperIO : ON
ASUS Card Detect : ON
DELL Support : OFF
Command line : "C:\Program Files (x86)\SpeedFan\speedfan.exe" 
Delta Fan Speed : 10

***************************** CHIPSET SMBUS

Chipset : nVidia MCP61
SMBus Base Address : $F400
SMBus Revision : A2
SMBus I/O Enabled : ON

***************************** PCI SCAN

Bus : 00 Device: 00 Function : 00 --> 03EA10DE Vendor : 10DE Device : 03EA (rev A1) - <Unknown device>
00: 10DE 03EA 0006 00B0 00A1 0500 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 1019 2606 0000 0000 0044 0000 0000 0000 00FF 0000
40: 1019 2606 DC08 0220 0020 1111 00D0 0000 0623 007F 0003 0000 0000 0003 0000 0000
60: 0000 0000 0000 0000 0000 0000 3606 0000 4444 0044 09D0 0000 0011 0000 1111 0088
80: 9923 0088 00FA 0D64 0003 0000 007F 0000 0078 A000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0101 0101 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0080 0000 0000 0000 0000 0000 0000 0000 0000 0000 0008 A801
E0: 0000 FEE0 0000 0000 0007 0000 1020 0000 FFF0 FFFF 0000 0000 0000 0000 0000 0000

Bus : 00 Device: 01 Function : 00 --> 03E010DE Vendor : 10DE Device : 03E0 (rev A2) - <Unknown device>
00: 10DE 03E0 000F 00A0 00A2 0601 0000 0080 0000 0000 0000 0000 1D01 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 1019 2606 0000 0000 0000 0000 0000 0000 00FF 0000
40: 1019 2606 0000 FEFF 3EFA 00FF 3EFA 00FF 3EFA 00FF 5A00 0262 0000 0500 002F FFFC
60: 0000 0000 0000 0000 0000 0000 0000 0000 0010 FFFF 80C5 0000 2000 1945 0040 0000
80: D009 1100 2D02 0080 00C0 0140 00FF 0000 7FFF 0000 0000 0000 6521 7408 0CB9 D000
A0: 0001 C010 0000 0000 0000 0000 0000 0000 0290 02EF 0800 085F 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 4150 FE00 01FD B000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0010 0000 0000 0000

Bus : 00 Device: 01 Function : 01 --> 03EB10DE Vendor : 10DE Device : 03EB (rev A2) - <Unknown device>
00: 10DE 03EB 0001 00B0 00A2 0C05 0000 0080 FC01 0000 0000 0000 0000 0000 0000 0000
20: 1C01 0000 F401 0000 0000 0000 1019 2606 0000 0000 0044 0000 0000 0000 010B 0000
40: 1019 2606 0001 C002 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
60: 1001 0000 1401 0000 1801 0000 0000 0000 0000 0000 0000 FEC8 0000 FEFE 2001 0000
80: 1000 FEFE 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 30D4 0080 0001 0000 0000 0000 0000 0000 0040 0140 0010 0000 0005 0000 0000 0000
E0: 1088 0004 4004 0702 1280 2000 4441 1144 FF02 BF1E 0001 8000 0010 0000 0000 0000

Bus : 00 Device: 01 Function : 02 --> 03F510DE Vendor : 10DE Device : 03F5 (rev A2) - <Unknown device>
00: 10DE 03F5 0400 00A0 00A2 0500 0000 0080 0000 0000 0000 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 1019 2606 0000 0000 0000 0000 0000 0000 0000 0000
40: 0000 0000 0000 0000 0210 1080 0010 1010 1010 1010 0000 0000 0000 0000 4210 0000
60: 000B 0000 1CC0 0652 0021 0A10 0000 0063 0009 0000 0000 0000 0000 0000 0000 0000
80: 0000 0000 0000 0040 0000 0000 18A0 0000 0000 0000 0000 1200 8120 0004 0000 0000
A0: 1400 0600 0000 0000 0000 0000 0001 0000 0000 0000 8042 0430 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000

Bus : 00 Device: 02 Function : 00 --> 03F110DE Vendor : 10DE Device : 03F1 (rev A3) - <Unknown device>
00: 10DE 03F1 0006 00B0 10A3 0C03 0000 0080 F000 FE02 0000 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 1019 2606 0000 0000 0044 0000 0000 0000 0116 0103
40: 1019 2606 0001 FE02 0000 0000 0000 0000 0002 0000 471D 0040 0010 0000 0000 0000
60: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000

Bus : 00 Device: 02 Function : 01 --> 03F210DE Vendor : 10DE Device : 03F2 (rev A3) - <Unknown device>
00: 10DE 03F2 0006 00B0 20A3 0C03 0000 0080 E000 FE02 0000 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 1019 2606 0000 0000 0044 0000 0000 0000 0215 0103
40: 1019 2606 800A 2098 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
60: 2020 0001 6000 8518 13C3 010F 0000 0000 0000 0508 1000 8020 3D89 22B6 2577 00D4
80: 0001 FE02 0000 0000 0000 0000 1615 0000 0100 0000 0000 0000 0000 0000 0000 0000
A0: 0001 0000 0000 C000 0000 0000 0000 0000 0033 2211 0044 0000 03FF 0000 0000 0000
C0: 1010 0D2D 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0010 0000 0000 0000

Bus : 00 Device: 04 Function : 00 --> 03F310DE Vendor : 10DE Device : 03F3 (rev A1) - <Unknown device>
00: 10DE 03F3 0407 00B0 01A1 0604 0000 0001 0000 0000 0000 0000 0100 2001 B0B0 2280
20: FD70 FD70 FDE0 FDE0 0000 0000 0000 0000 0000 0000 00B8 0000 0000 0000 00FF 0204
40: 0000 0773 0001 0002 0007 0000 0000 0048 0000 0000 0000 0000 1FFF 1FFF 0000 0000
60: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0600 0000 0000 0000 0000 0000 0008 A801 0000 FEE0 0000 0000 0000 0000 0000 0000
A0: 0004 0000 0000 0000 0000 0000 0000 0000 0000 0000 FFFF 0000 8C0D 0000 10DE CB84
C0: 10DE CB84 0003 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000

Bus : 00 Device: 05 Function : 00 --> 03F010DE Vendor : 10DE Device : 03F0 (rev A2) - <Unknown device>
00: 10DE 03F0 0006 00B0 00A2 0403 0000 0080 4000 FE02 0000 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 1019 2107 0000 0000 0044 0000 0000 0000 0216 0502
40: 1019 2107 5001 C002 0000 0000 0101 000F 6C05 0180 0000 0000 0000 0000 0000 0000
60: 0000 0000 0000 0000 000F 0000 0008 A803 0000 0000 0000 0000 0000 0000 0000 0000
80: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 4700 2900 0000 0000 0000

Bus : 00 Device: 06 Function : 00 --> 03EC10DE Vendor : 10DE Device : 03EC (rev A2) - <Unknown device>
00: 10DE 03EC 0005 00B0 8AA2 0101 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
20: F001 0000 0000 0000 0000 0000 1019 2606 0000 0000 0044 0000 0000 0000 0000 0103
40: 1019 2606 0001 0002 0000 0000 0000 0000 F002 0004 0000 0000 A8A8 20A8 006A 2099
60: 0000 C000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0101
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0010 0000 0000 0000

Bus : 00 Device: 07 Function : 00 --> 03EF10DE Vendor : 10DE Device : 03EF (rev A2) - <Unknown device>
00: 10DE 03EF 0006 00B0 00A2 0680 0000 0000 D000 FE02 0001 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 1019 2606 0000 0000 0044 0000 0000 0000 0115 1401
40: 1019 2606 5001 FE02 0100 0000 0008 2000 6C05 0186 0000 0000 0000 0000 0000 0000
60: 0000 0000 0000 0000 00FF 0000 0008 A803 0000 0000 0000 0000 0000 0000 0000 0000
80: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0142 0000 0000 0000

Bus : 00 Device: 08 Function : 00 --> 03F610DE Vendor : 10DE Device : 03F6 (rev A2) - <Unknown device>
00: 10DE 03F6 0007 00B0 85A2 0101 0000 0080 09F1 0000 0BF1 0000 0971 0000 0B71 0000
20: D801 0000 C000 FE02 0000 0000 1019 2606 0000 0000 0044 0000 0000 0000 0117 0103
40: 1019 2606 B001 0002 0000 0000 0000 0000 682F 0008 0000 0000 20A8 A8A8 00A6 9920
60: 0000 0000 0C41 0000 0F00 4206 0000 0000 782C 40C4 1001 0000 1001 0000 0020 0120
80: 0000 8000 EFFE EFB7 0000 1FF1 2000 39EB 0000 A984 0000 0000 0006 1006 03F6 0101
A0: 0008 0F00 0000 0000 0000 0000 3133 0200 CC05 0084 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 000A 000A 0008 A803 0008 4400 0800 0008 0008 7700 0800 0003
E0: 0000 0040 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 000C 0000 0000

Bus : 00 Device: 09 Function : 00 --> 03E810DE Vendor : 10DE Device : 03E8 (rev A2) - <Unknown device>
00: 10DE 03E8 0407 0010 00A2 0604 0010 0001 0000 0000 0000 0000 0200 0002 A1A1 0000
20: FDD0 FDD0 FDC1 FDC1 0000 0000 0000 0000 0000 0000 0040 0000 0000 0000 0000 0004
40: 480D 0000 10DE 0000 5001 F802 0000 0000 6005 0093 300C FEE0 0000 0000 4970 0000
60: 8008 A801 0000 FEE0 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0010 0141 8001 0000 2830 0000 3D01 0011 0000 1101 2580 0008 01C0 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000

Bus : 00 Device: 11 Function : 00 --> 03E910DE Vendor : 10DE Device : 03E9 (rev A2) - <Unknown device>
00: 10DE 03E9 0407 0010 00A2 0604 0010 0001 0000 0000 0000 0000 0300 0003 9191 0000
20: FDB0 FDB0 FDA1 FDA1 0000 0000 0000 0000 0000 0000 0040 0000 0000 0000 0000 0004
40: 480D 0000 10DE 0000 5001 F802 0000 0000 6005 0093 300C FEE0 0000 0000 4960 0000
60: 8008 A801 0000 FEE0 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0010 0141 8001 0000 2830 0000 3C11 0111 0000 1011 0500 0010 01C0 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000

Bus : 00 Device: 12 Function : 00 --> 03E910DE Vendor : 10DE Device : 03E9 (rev A2) - <Unknown device>
00: 10DE 03E9 0407 0010 00A2 0604 0010 0001 0000 0000 0000 0000 0400 0004 8181 0000
20: FD90 FD90 FD81 FD81 0000 0000 0000 0000 0000 0000 0040 0000 0000 0000 0000 0004
40: 480D 0000 10DE 0000 5001 F802 0000 0000 6005 0093 300C FEE0 0000 0000 49B2 0000
60: 8008 A801 0000 FEE0 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0010 0141 8001 0000 2830 0000 3C11 0211 0000 1011 0500 0018 01C0 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000

Bus : 00 Device: 13 Function : 00 --> 03D010DE Vendor : 10DE Device : 03D0 (rev A2) - <Unknown device>
00: 10DE 03D0 0007 00B0 00A2 0300 0000 0000 0000 FB00 000C E000 0000 0000 0004 FC00
20: 0000 0000 0000 0000 0000 0000 1019 2606 0000 0000 0048 0000 0000 0000 0114 0000
40: 1019 2606 0000 0300 5001 0002 0000 0000 0005 0080 0000 0000 0000 0000 0000 0000
60: 0001 0000 041C 0004 0000 0000 0000 0000 FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF
80: FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF
A0: 0000 0170 0000 0800 0000 0000 FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF
C0: FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF
E0: FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF

Bus : 00 Device: 24 Function : 00 --> 11001022 Vendor : 1022 Device : 1100 (rev 00) - Advanced Micro Devices Athlon 64 / Opteron HyperTransport Technology Configuration
00: 1022 1100 0000 0010 0000 0600 0000 0080 0000 0000 0000 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0080 0000 0000 0000 0000 0000
40: 0101 0001 0101 0001 0101 0001 0101 0001 0101 0001 0101 0001 0101 0001 0101 0001
60: 0000 0001 00E4 0000 C820 0F2E 000C 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0008 2101 0020 1111 0622 8075 0002 0000 0169 0161 0000 0004 0007 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000

Bus : 00 Device: 24 Function : 01 --> 11011022 Vendor : 1022 Device : 1101 (rev 00) - Advanced Micro Devices Athlon 64 / Opteron Address Map
00: 1022 1101 0000 0000 0000 0600 0000 0080 0000 0000 0000 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
40: 0003 0000 0000 00BF 0000 0000 0001 0000 0000 0000 0002 0000 0000 0000 0003 0000
60: 0000 0000 0004 0000 0000 0000 0005 0000 0000 0000 0006 0000 0000 0000 0007 0000
80: 0A03 0000 0B00 0000 0000 0000 0000 0000 0003 00C0 FF00 00EF 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0003 00F4 0200 00FE 0003 00F0 3F80 00F0 0000 0000 0000 0000
C0: 8013 0000 F000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0003 0400 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000

Bus : 00 Device: 24 Function : 02 --> 11021022 Vendor : 1022 Device : 1102 (rev 00) - Advanced Micro Devices Athlon 64 / Opteron DRAM Controller
00: 1022 1102 0000 0000 0000 0600 0000 0080 0000 0000 0000 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
40: 0000 0000 0000 0000 0001 0000 0000 0000 0001 0040 0000 0000 0001 0080 0000 0000
60: 0000 0000 3FE0 0038 3FE0 0038 3FE0 0038 0000 0000 0000 0000 0046 0000 0000 0000
80: 5550 0000 0000 0000 FA24 AE7D 1320 4902 0430 0001 006B 7710 0039 8000 0031 0000
A0: 02FF 0C00 0000 0000 0000 0000 0000 0000 6A49 5661 008B 0000 0EF4 7800 E7C0 5EA9
C0: 0000 0003 0000 0000 0000 0000 0000 0000 1411 7C20 6319 BC44 246E 04EC D60C 1D64
E0: 8099 6713 2309 B802 02E6 10FE 0311 003F 0000 0000 0000 0000 0000 0000 0000 0000

Bus : 00 Device: 24 Function : 03 --> 11031022 Vendor : 1022 Device : 1103 (rev 00) - Advanced Micro Devices Athlon 64 / Opteron Miscellaneous Control
00: 1022 1103 0000 0010 0000 0600 0000 0080 0000 0000 0000 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 00F0 0000 0000 0000 0000 0000
40: 3BFF 0004 0040 0A10 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 EB80 C6CC
60: 006C 0000 0000 0000 0000 0000 0000 0000 0111 5132 4021 5070 2A00 0800 2117 0000
80: 0000 2327 2113 2113 0000 0000 0000 0000 0000 0000 0100 0000 FA00 FABF 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 A701 000D 0000 0CC0 2625 0026
E0: 0000 0000 E13E 003C 1719 0000 0000 0000 000F 0010 0000 0000 0000 0000 0FB2 0006

Bus : 01 Device: 06 Function : 00 --> 03011814 Vendor : 1814 Device : 0301 (rev 00) - Ralink Technology, Corp unknown rt2500
00: 1814 0301 0006 0410 0000 0280 0010 0000 8000 FD7F 0000 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0601 0000 1737 0055 0000 0000 0040 0000 0000 0000 0111 0000
40: 0001 0002 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
60: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000

***************************** ISA SCAN

ISA Dump from address $290 --> <IT8712F-J> (ISA at $0290) (No error)
00: 13 10 FF 00 FF FF 00 00 00 80 01 09 07 A9 FF 00   ................
10: FF FF FF 33 D0 26 00 FF 01 FF 00 FF FF FF FF FF   ...3.&..........
20: 4B 9C 70 D2 BE 49 B4 BD C0 11 22 16 07 99 99 99   K.p..I....".....
30: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
40: 41 7F 7F 7F 7F 7F 5F 74 2D 40 AB 22 FF FF FF FF   A....._t-@."....
50: FF 31 7F 7F 7F 50 EA 5D 90 5D 03 12 84 F8 08 88   .1...P.].]......
60: FF 37 7F 2D B0 83 FF FF FF 37 7F 2D B2 83 FF FF   .7.-.....7.-....
70: 7F 7F 7F 00 00 3F FF FF FF FF FF FF FF FF FF FF   .....?..........
80: 00 00 00 00 FF FF FF FF 00 00 FF CA 02 00 99 99   ................
90: 7F 7F 7F 00 00 7F FF FF 7F 7F 7F 00 00 7F FF FF   ................
A0: 00 00 00 00 00 00 00 FF FF FF FF FF FF FF FF FF   ................
B0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
C0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
D0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
E0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
F0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................

***************************** SMBUS SCAN

SMB Dump from address $51 --> <RAM> (SMBus at $1C00) (No error)
00: 80 08 08 0E 0A 60 40 00 05 25 40 00 82 08 00 00   .....`@..%@.....
10: 0C 08 38 01 02 00 03 3D 50 50 60 32 1E 32 2D 01   ..8....=PP`2.2-.
20: 17 25 05 12 3C 1E 1E 00 36 39 7F 80 14 1E 00 00   .%..<...69......
30: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 12 F8   ................
40: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
50: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
60: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
70: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
80: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
90: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
A0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
B0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
C0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
D0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
E0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
F0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
SMB Dump from address $52 --> <RAM> (SMBus at $1C00) (No error)
00: 80 08 08 0E 0A 60 40 00 05 25 40 00 82 08 00 00   .....`@..%@.....
10: 0C 08 38 01 02 00 03 3D 50 50 60 32 1E 32 2D 01   ..8....=PP`2.2-.
20: 17 25 05 12 3C 1E 1E 00 36 39 7F 80 14 1E 00 00   .%..<...69......
30: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 12 F8   ................
40: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
50: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
60: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
70: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
80: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
90: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
A0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
B0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
C0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
D0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
E0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
F0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
SMB Dump from address $53 --> <RAM> (SMBus at $1C00) (No error)
00: 80 08 08 0E 0A 60 40 00 05 25 40 00 82 08 00 00   .....`@..%@.....
10: 0C 08 38 01 02 00 03 3D 50 50 60 32 1E 32 2D 01   ..8....=PP`2.2-.
20: 17 25 05 12 3C 1E 1E 00 36 39 7F 80 14 1E 00 00   .%..<...69......
30: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 12 F8   ................
40: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
50: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
60: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
70: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
80: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
90: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
A0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
B0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
C0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
D0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
E0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
F0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
SMB Dump from address $50 --> <RAM> (SMBus at $3D403637) (unknown error)
00: 00 FF FF FF FF FF FF 00 05 E3 00 19 05 15 00 00   ................
10: 09 13 01 03 68 29 17 78 2A EE D1 A5 55 48 9B 26   ....h).x*...UH.&
20: 12 50 54 BF EE 00 31 0A 61 4C 01 01 01 01 01 01   .PT...1.aL......
30: 01 01 01 01 01 01 66 21 56 AA 51 00 1E 30 46 8F   ......f!V.Q..0F.
40: 33 00 9D EA 10 00 00 1E 66 21 50 B0 51 00 1B 30   3.......f!P.Q..0
50: 40 70 36 00 22 13 00 00 00 1E 00 00 00 FD 00 37   @p6."..........7
60: 4B 1E 51 09 00 0A 20 20 20 20 20 20 00 00 00 FC   K.Q...      ....
70: 00 46 31 39 0A 20 20 20 20 20 20 20 20 20 00 92   .F19.         ..
80: 00 FF FF FF FF FF FF 00 05 E3 00 19 05 15 00 00   ................
90: 09 13 01 03 68 29 17 78 2A EE D1 A5 55 48 9B 26   ....h).x*...UH.&
A0: 12 50 54 BF EE 00 31 0A 61 4C 01 01 01 01 01 01   .PT...1.aL......
B0: 01 01 01 01 01 01 66 21 56 AA 51 00 1E 30 46 8F   ......f!V.Q..0F.
C0: 33 00 9D EA 10 00 00 1E 66 21 50 B0 51 00 1B 30   3.......f!P.Q..0
D0: 40 70 36 00 22 13 00 00 00 1E 00 00 00 FD 00 37   @p6."..........7
E0: 4B 1E 51 09 00 0A 20 20 20 20 20 20 00 00 00 FC   K.Q...      ....
F0: 00 46 31 39 0A 20 20 20 20 20 20 20 20 20 00 92   .F19.         ..

***************************** SMBUS RETRIES

Retry attempts info for SMBus at $1C00
  [ -1]=171
  [  1]=171
Retry attempts info for SMBus at $F400
  [ -1]=174
  [  1]=174
Retry attempts info for SMBus at $3E3F
  [ -1]=1560
  [  1]=1560
Retry attempts info for SMBus at $3637
  [ -1]=1300
  [  1]=1300
Retry attempts info for SMBus at $5051
  [ -1]=1560
  [  1]=1560

***************************** SMBUS PAUSES

Pause stats for SMBusnForce2@$1C00: min=49815 max=50000 avg=49999(2997) touts=342 count=3339
Pause stats for SMBusnForce2@$F400: min=49999 max=50000 avg=50000(696) touts=348 count=1044

***************************** DIMM INFO

***************************** SMBUS DEVICE SCAN RESULTS

***************************** FAN SPEED CONTROL

Can change fan speeds : YES
Can smoothly change fan speeds : YES
Can stop fans : DON'T KNOW

***************************** WMI SCAN

WMI interface is registered : ON
MB manufacturer: eMachines
MB model: MCP61PM-GM
MB version: 2.2      
ACPI temp: 40.0
ACPI active trip point: 0.0
ACPI passive trip point: 122.0
ACPI critical trip point: 124.0
WMI quick analysis results -->
EXPLORING : root\CIMV2\Win32_BaseBoard
  -> Object Start
  Caption = Base Board
  CreationClassName = Win32_BaseBoard
  Description = Base Board
  HostingBoard = True
  HotSwappable = False
  Manufacturer = eMachines
  Name = Base Board
  PoweredOn = True
  Product = MCP61PM-GM
  Removable = True
  Replaceable = True
  RequiresDaughterBoard = False
  SerialNumber = OEM
  Status = OK
  Tag = Base Board
  Version = 2.2      
  Method -> IsCompatible(ElementToCheck)
EXPLORING : root\WMI\msacpi_thermalzonetemperature
  -> Object Start
  Active = True
  ActiveTripPoint =  0 0 0 0 0 0 0 0 0 (0.0C)
  ActiveTripPointCount = 1
  CriticalTripPoint = 3972 (124.0C)
  CurrentTemperature = 3132 (40.0C)
  InstanceName = ACPI\ThermalZone\THRM_0
  PassiveTripPoint = 3952 (122.0C)
  Reserved = 0
  SamplingPeriod = 60
  ThermalConstant1 = 4
  ThermalConstant2 = 3
  ThermalStamp = 25
EXPLORING : root\CIMV2\CIM_AssociatedSensor
EXPLORING : root\CIMV2\CIM_CoolingDevice
EXPLORING : root\CIMV2\CIM_Fan
EXPLORING : root\CIMV2\CIM_HeatPipe
EXPLORING : root\CIMV2\CIM_ManagementController
EXPLORING : root\CIMV2\CIM_NumericSensor
EXPLORING : root\CIMV2\CIM_PackageAlarm
EXPLORING : root\CIMV2\CIM_PackageCooling
EXPLORING : root\CIMV2\CIM_Refrigeration
EXPLORING : root\CIMV2\CIM_Sensor
EXPLORING : root\CIMV2\CIM_Tachometer
EXPLORING : root\CIMV2\CIM_TemperatureSensor
EXPLORING : root\CIMV2\CIM_VoltageSensor
EXPLORING : root\CIMV2\Win32_CurrentProbe
EXPLORING : root\CIMV2\Win32_Fan
EXPLORING : root\CIMV2\Win32_HeatPipe
EXPLORING : root\CIMV2\Win32_Refrigeration
EXPLORING : root\CIMV2\Win32_TemperatureProbe
EXPLORING : root\CIMV2\Win32_VoltageProbe
EXPLORING : SMBIOS
  -> Object Start
Structure 188 - 0025 - fixed len is 212 bytes -> Unknown (188)
  -> 00 00 00 C0 00 00 00 00 00 00 00 00 00 00 00 00 01 06 16 00 00 00 00 00 03 00 00 00 00 00 BF 00 00 00 00 00 01 00 00 00 00 00 00 00 02 00 00 00 00 00 00 00 03 00 00 00 00 00 00 00 04 00 00 00 00 00 00 00 05 00 00 00 00 00 00 00 06 00 00 00 00 00 00 00 07 00 00 00 00 00 00 00 40 00 10 0A 00 00 00 00 00 00 04 00 FF 02 00 0C 00 00 00 00 00 00 00 00 01 00 00 00 00 00 00 00 01 00 40 00 00 00 00 00 01 00 80 00 00 00 00 00 00 00 00 00 E0 3F 38 00 E0 3F 38 00 E0 3F 38 00 46 00 00 00 00 00 00 00 50 55 00 00 00 00 00 00 24 FA 7D AE 20 13 02 49 30 04 01 00 6B 00 10 77 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
Structure 190 - 0026 - fixed len is 212 bytes -> Unknown (190)
  -> 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
Structure 192 - 0027 - fixed len is 244 bytes -> Unknown (192)
  -> 16 14 15 15 15 14 15 15 16 00 00 00 14 15 14 16 15 16 16 15 14 00 00 00 34 34 34 34 16 14 14 14 14 14 15 14 16 14 14 16 13 14 14 15 14 14 32 32 32 32 22 32 11 20 20 25 20 10 22 33 11 10 20 25 20 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
Structure 194 - 0028 - fixed len is 244 bytes -> Unknown (194)
  -> 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<-- End of WMI quick analysis results

***************************** DMI SCAN

DMI structures from SMBIOS ver. 2.4
MBManufacturer : eMachines
MBModel : MCP61PM-GM
MBVersion : 2.2
BIOSVendor : Phoenix Technologies, LTD
BIOSVersion : 6.00 PG
SysManufacturer : eMachines
SysProductName : ET1161-07
SysVersion : 9000
SysSerialNumber : PTNAD0X0029020097B9000
Structure   0 - 0000 - fixed len is 20 bytes -> BIOS information
  -> 01 02 00 E0 03 0F 90 9E CB 7F 00 00 00 00 33 07 FF FF FF FF
  -> 'Phoenix Technologies, LTD'
  -> '6.00 PG'
  -> '10/29/2008'
Structure   1 - 0001 - fixed len is 23 bytes -> System information
  -> 01 02 03 04 40 65 67 28 E1 DC DD 11 AD B6 EB CC 9B 83 63 94 06 05 06
  -> 'eMachines'
  -> 'ET1161-07'
  -> '9000'
  -> 'PTNAD0X0029020097B9000'
  -> ' '
  -> ' '
Structure   2 - 0002 - fixed len is 4 bytes -> Base board (or module) information
  -> 01 02 03 04
  -> 'eMachines'
  -> 'MCP61PM-GM'
  -> '2.2      '
  -> 'OEM'
Structure   3 - 0003 - fixed len is 13 bytes -> System enclosure or chassis
  -> 01 03 02 03 04 02 02 02 02 00 00 00 00
  -> 'eMachines'
  -> 'Unknow'
  -> '0000000000'
  -> 'Unknow'
Structure   4 - 0004 - fixed len is 31 bytes -> Processor information
  -> 01 03 01 02 B2 0F 06 00 FF FB 8B 17 03 8C C9 00 B8 0B 34 08 41 11 0A 00 0C 00 FF FF 04 05 06
  -> 'Socket AM2 '
  -> 'AMD'
  -> 'AMD Athlon(tm) Dual Core Processor 4050e  '
  -> ' '
  -> ' '
  -> ' '
Structure   5 - 0005 - fixed len is 20 bytes -> Memory controller information
  -> 06 04 03 03 0C 1C 00 04 01 04 04 06 00 07 00 08 00 09 00 00
Structure   6 - 0006 - fixed len is 8 bytes -> Memory module information
  -> 01 FF 00 13 00 7F 7F 00
  -> 'A0'
Structure   6 - 0007 - fixed len is 8 bytes -> Memory module information
  -> 01 2F 00 13 00 0A 0A 00
  -> 'A1'
Structure   6 - 0008 - fixed len is 8 bytes -> Memory module information
  -> 01 4F 00 13 00 0A 0A 00
  -> 'A2'
Structure   6 - 0009 - fixed len is 8 bytes -> Memory module information
  -> 01 6F 00 13 00 0A 0A 00
  -> 'A3'
Structure   9 - 0017 - fixed len is 9 bytes -> System slots
  -> 01 06 05 03 04 01 00 02 01
  -> 'PCI0'
Structure   9 - 0018 - fixed len is 9 bytes -> System slots
  -> 01 06 05 04 04 02 00 02 01
  -> 'PCI1'
Structure  13 - 0019 - fixed len is 18 bytes -> BIOS language information
  -> 03 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 01
  -> 'n|US|iso8859-1'
  -> 'n|US|iso8859-1'
  -> 'r|CA|iso8859-1'
  -> 'a|JP|unicode'
Structure  16 - 001A - fixed len is 11 bytes -> Physical memory array
  -> 03 03 03 00 00 00 01 FE FF 04 00
Structure  17 - 001B - fixed len is 23 bytes -> Memory device
  -> 1A 00 FE FF 40 00 40 00 00 00 09 00 01 02 02 00 00 00 00 03 04 05 06
  -> 'A0'
  -> 'Bank0/1'
  -> 'None'
  -> 'None'
  -> 'None'
  -> 'None'
Structure  17 - 001C - fixed len is 23 bytes -> Memory device
  -> 1A 00 FE FF 40 00 40 00 00 04 09 00 01 02 02 00 00 00 00 03 04 05 06
  -> 'A1'
  -> 'Bank2/3'
  -> 'None'
  -> 'None'
  -> 'None'
  -> 'None'
Structure  17 - 001D - fixed len is 23 bytes -> Memory device
  -> 1A 00 FE FF 40 00 40 00 00 04 09 00 01 02 02 00 00 00 00 03 04 05 06
  -> 'A2'
  -> 'Bank4/5'
  -> 'None'
  -> 'None'
  -> 'None'
  -> 'None'
Structure  17 - 001E - fixed len is 23 bytes -> Memory device
  -> 1A 00 FE FF 40 00 40 00 00 04 09 00 01 02 02 00 00 00 00 03 04 05 06
  -> 'A3'
  -> 'Bank6/7'
  -> 'None'
  -> 'None'
  -> 'None'
  -> 'None'
Structure  19 - 001F - fixed len is 11 bytes -> Memory array mapped address
  -> 00 00 00 00 FF FF 2F 00 1A 00 01
Structure  20 - 0020 - fixed len is 15 bytes -> Memory device mapped address
  -> 00 00 00 00 00 00 00 00 1B 00 1F 00 01 00 00
Structure  20 - 0021 - fixed len is 15 bytes -> Memory device mapped address
  -> 00 00 00 00 FF FF 0F 00 1C 00 1F 00 01 00 00
Structure  20 - 0022 - fixed len is 15 bytes -> Memory device mapped address
  -> 00 00 10 00 FF FF 1F 00 1D 00 1F 00 01 00 00
Structure  20 - 0023 - fixed len is 15 bytes -> Memory device mapped address
  -> 00 00 20 00 FF FF 2F 00 1E 00 1F 00 01 00 00
Structure  32 - 0024 - fixed len is 7 bytes -> System boot information
  -> 00 00 00 00 00 00 00
Structure 188 - 0025 - fixed len is 208 bytes -> Unknown (188)
  -> 00 00 00 C0 00 00 00 00 00 00 00 00 00 00 00 00 01 06 16 00 00 00 00 00 03 00 00 00 00 00 BF 00 00 00 00 00 01 00 00 00 00 00 00 00 02 00 00 00 00 00 00 00 03 00 00 00 00 00 00 00 04 00 00 00 00 00 00 00 05 00 00 00 00 00 00 00 06 00 00 00 00 00 00 00 07 00 00 00 00 00 00 00 40 00 10 0A 00 00 00 00 00 00 04 00 FF 02 00 0C 00 00 00 00 00 00 00 00 01 00 00 00 00 00 00 00 01 00 40 00 00 00 00 00 01 00 80 00 00 00 00 00 00 00 00 00 E0 3F 38 00 E0 3F 38 00 E0 3F 38 00 46 00 00 00 00 00 00 00 50 55 00 00 00 00 00 00 24 FA 7D AE 20 13 02 49 30 04 01 00 6B 00 10 77 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
Structure 190 - 0026 - fixed len is 208 bytes -> Unknown (190)
  -> 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
Structure 192 - 0027 - fixed len is 240 bytes -> Unknown (192)
  -> 16 14 15 15 15 14 15 15 16 00 00 00 14 15 14 16 15 16 16 15 14 00 00 00 34 34 34 34 16 14 14 14 14 14 15 14 16 14 14 16 13 14 14 15 14 14 32 32 32 32 22 32 11 20 20 25 20 10 22 33 11 10 20 25 20 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
Structure 194 - 0028 - fixed len is 240 bytes -> Unknown (194)
  -> 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
Structure 127 - 0029 - fixed len is 0 bytes -> End of table
  -> 

***************************** EVENTS

1 events defined
Loaded event : sensor[5].temp[1].value>=60

***************************** EXTRA UNCATEGORIZED INFO

Tray icon size : 16x16
UPTIME : 0 days 12:51:25
SpeedFan UPTIME : 0 days 00:31:50

***************************** MAIN WINDOW INFO

Win9x:NO  64Bit:YES  GiveIO:NO  SpeedFan:YES
Found nVidia GeForce 6150SE nForce 430
Scanning ISA BUS at $0290...
SuperIO Chip=IT8726F
IT8712F(J) found on ISA at $290
Scanning nForce2 SMBus at $1C00...
Scanning nForce2 SMBus at $F400...
Scanning I2CNVidia SMBus at $3D403E3F...
Address $2D appears to be WRITE ONLY...
Address $2E appears to be WRITE ONLY...
Address $48 appears to be WRITE ONLY...
Address $49 appears to be WRITE ONLY...
Address $4C appears to be WRITE ONLY...
Address $50 appears to be WRITE ONLY...
Scanning I2CNVidia SMBus at $3D403637...
Address $2D appears to be WRITE ONLY...
Address $2E appears to be WRITE ONLY...
Address $48 appears to be WRITE ONLY...
Address $49 appears to be WRITE ONLY...
Address $4C appears to be WRITE ONLY...
Scanning I2CNVidia SMBus at $3D405051...
Address $2D appears to be WRITE ONLY...
Address $2E appears to be WRITE ONLY...
Address $48 appears to be WRITE ONLY...
Address $49 appears to be WRITE ONLY...
Address $4C appears to be WRITE ONLY...
Address $50 appears to be WRITE ONLY...
Found ST3500410AS on AdvSMART
Found WDC WD3200AAJS-22L7A0 on AdvSMART
Found ACPI temperature (40.0C)
Loaded 1 events

***************************** DEBUG INFO

Win9x:NO  64Bit:YES  GiveIO:NO  SpeedFan:YES
SpeedFan.sys ver. 1.002
  -> Can read memory
  -> Can read MSR
  -> Can't map memory
About to do a test on INTEL MSRs...
End of INTEL MSR test
I/O properly initialized
Starting PCI scan...
SMBus at $1C00 WRITEQ failed ($01)
nForce2 SMBus at $1C00 returned <unknown error>
SMBus at $F400 WRITEQ failed ($01)
nForce2 SMBus at $F400 returned <unknown error>
PCI scan done!
NVAPI linking - Debug notes start
  DLL found
  nvapi_QueryInterface properly linked ($02F21384)
  Answer from nvapi_QueryInterface=$02F230DA
  Answer from nvapi_Unknown1=$00000000
  $02F21A4B <- NVAPI_GetErrorMessage
  $02F2210D <- NVAPI_EnumPhysicalGPUs
  $02F2104B <- NvAPI_GPU_GetThermalSettings
  $02F21F78 <- NvAPI_I2CRead
  $02F218B6 <- NVAPI_GetInterfaceVersionString
  $02F23161 <- NVAPI_GetDisplayDriverVersion
  $02F226EE <- NVAPI_EnumNvidiaDisplayHandle
  $02F233A0 <- NVAPI_EnumNvidiaUnAttachedDisplayHandle
  $02F221D5 <- NVAPI_GPU_GetFullName
  $02F21488 <- NVAPI_GPU_GetPCIIdentifiers
  $02F2101E <- NVAPI_GPU_GetBusId
  $02F23251 <- NVAPI_GPU_GetBusSlotId
NVAPI linking - Debug notes end
NVAPI Version string=NVidia Complete Version 1.10
NVAPI - Enumerating displays -->
  Found display #0 ($DE000001)
NVAPI - Enumerating unattached displays -->
  SafetyCount=1
DrvVer=19107  BldChangeListNum=4743138  Branch=r190_93-10178
  GpuCount=1
GPU#0 (BB0000D0) is GeForce 6150SE nForce 430
  DevId=$03D010DE  SubSysId=$26061019  RevId=$000000A2  ExtDevId=$000003D0
NVAPI_GPU_GetBusId=02F2101E
  BusId=0
NVAPI_GPU_GetBusSlotId=02F23251
  BusSlotId=13
Found nVidia GeForce 6150SE nForce 430
 --> bus : 0  dev : 13  func : 0  r=$03D010DE
  --> BA[$10]=$FB000000 is MEM (type 0) 
    [$10F0]=00007FFF
    [$15A0]=80000000
    [$15A4]=00000000
    [$15A8]=00000000
    [$15AC]=00000000
    [$15B0]=40000000
    [$15B4]=20000000
    [$15B8]=00000000
    [$15BC]=3FFF0000
    [$15F0]=00000000
    [$15F4]=00000000
    [$15F8]=7FFFFFFF
    [$15FC]=00000000
    [$4000]=C0000033
    [$4004]=00071614
    [$4008]=00000000
    [$400C]=00000000
    [$4010]=00000000
    [$4014]=00000000
    [$4018]=00000000
    [$401C]=00000000
    [$4020]=00000000
    [$4024]=00000000
    [$4028]=00000000
    [$402C]=00000000
    [$4030]=00000000
    [$4034]=00000000
    [$4038]=00000000
    [$403C]=00000000
    [$4040]=00000000
    [$4044]=00000000
    [$4048]=00000000
    [$404C]=00000000
    [$4050]=00000000
    [$4054]=00000000
    [$4058]=00000000
    [$405C]=00000000
  --> BA[$14]=$E0000000 is MEM (type 2) (prefetchable) 
  --> BA[$1C]=$FC000000 is MEM (type 2) 
  Found in NVAPI listed GPUs
  NVAPI reported temperature=0.00C
 -> Temperature 1 offset : 0
Scanning ISA BUS at $0290...
Second pass...
ITE r[$20]=$87 r[$21]=$26 r[$22]=$03 r[$07]=$00 
NEW --> SuperIO chip=ITE IT8726F ($002E)
Checking $002E for ITE (1)...
ITE Registers [$002E] : $87 $26 $03
SuperIO Chip=IT8726F
 --> [$25]=$41
 --> [$26]=$90
 --> [$27]=$01
 --> [$28]=$41
 --> [$29]=$28
 --> [$2A]=$01
 --> LDN0 [$60]=$0000 [$62]=$0000 [$64]=$0000 (disabled)
 --> LDN1 [$60]=$0000 [$62]=$0000 [$64]=$0000 (disabled)
 --> LDN2 [$60]=$02F8 [$62]=$0000 [$64]=$0000 (disabled)
 --> LDN3 [$60]=$0000 [$62]=$0000 [$64]=$0080 (disabled)
 --> LDN4 [$60]=$0290 [$62]=$0000 [$64]=$0000 (enabled)
 --> LDN5 [$60]=$0060 [$62]=$0064 [$64]=$0000 (enabled)
 --> LDN6 [$60]=$0000 [$62]=$0000 [$64]=$0000 (enabled)
 --> LDN7 [$60]=$0000 [$62]=$0800 [$64]=$0000 (disabled)
 --> LDN8 [$60]=$0300 [$62]=$0000 [$64]=$0000 (disabled)
 --> LDN9 [$60]=$0201 [$62]=$0000 [$64]=$0000 (disabled)
 --> LDNA [$60]=$0310 [$62]=$0000 [$64]=$0000 (disabled)
 --> LDNB [$60]=$0000 [$62]=$0000 [$64]=$0000 (disabled)
IT8712F(J) found on ISA at $290
 -> Temperature sensor diode 1 : Diode
 -> Temperature sensor diode 2 : Thermistor
 -> Temperature sensor diode 3 : Thermistor
 -> PWM 1 mode : Software controlled
 -> PWM 2 mode : Software controlled
 -> PWM 3 mode : ON/OFF
 -> PWM 4 mode : Software controlled
 -> PWM 5 mode : Software controlled
 -> PWMOUT clock : 3M
 -> Temperature 1 offset : 0
 -> Temperature 2 offset : 0
 -> Temperature 3 offset : 0
 -> FAN1 mult : 1
 -> FAN1 div : 1
 -> FAN2 mult : 1
 -> FAN2 div : 1
 -> FAN3 mult : 1
 -> FAN3 div : 1
 -> FAN4 mult : 1
 -> FAN4 div : 1
 -> FAN5 mult : 1
 -> FAN5 div : 1
 -> Reverse PWM01 logic : OFF
 -> Reverse PWM02 logic : OFF
 -> Reverse PWM03 logic : OFF
 -> Reverse PWM04 logic : OFF
 -> Reverse PWM05 logic : OFF
Scanning nForce2 SMBus at $1C00...
Scanning nForce2 SMBus at $F400...
Scanning I2CNVidia SMBus at $3D403E3F...
Address $2D appears to be WRITE ONLY...
Address $2E appears to be WRITE ONLY...
Address $48 appears to be WRITE ONLY...
Address $49 appears to be WRITE ONLY...
Address $4C appears to be WRITE ONLY...
Address $50 appears to be WRITE ONLY...
Scanning I2CNVidia SMBus at $3D403637...
Address $2D appears to be WRITE ONLY...
Address $2E appears to be WRITE ONLY...
Address $48 appears to be WRITE ONLY...
Address $49 appears to be WRITE ONLY...
Address $4C appears to be WRITE ONLY...
Scanning I2CNVidia SMBus at $3D405051...
Address $2D appears to be WRITE ONLY...
Address $2E appears to be WRITE ONLY...
Address $48 appears to be WRITE ONLY...
Address $49 appears to be WRITE ONLY...
Address $4C appears to be WRITE ONLY...
Address $50 appears to be WRITE ONLY...
About to probe Intel QST...
    HECI driver not found
End of Intel QST probing
About to probe Intel FB-DIMM support...
End of Intel FB-DIMM support probing
About to probe TOSHIBA SUPPORT...
End of TOSHIBA SUPPORT probing
About to probe Areca RAID support...
ARECA : interface properly linked
ARECA : 0 Areca RAID controller(s) found
End of Areca RAID probing
About to probe 3ware RAID support...
DLL properly linked
API version is <2.04.00.003>
3ware Controllers found : 0
End of 3ware RAID probing
About to probe SMART (Advanced Methods)...
AdvSMART debug messages start -->
DeviceID=PCI\VEN_10DE&DEV_03F1&SUBSYS_26061019&REV_A3\3&2411E6FE&1&10
Name=Standard OpenHCD USB Host Controller
  DeviceID=USB\ROOT_HUB\4&20D185F2&0
  Name=USB Root Hub
  DeviceID=USB\VID_046D&PID_C517\5&299DC760&0&2
  Name=USB Composite Device
  DeviceID=USB\VID_046D&PID_C517&MI_00\6&28A341C9&0&0000
  Name=USB Input Device
  DeviceID=HID\VID_046D&PID_C517&MI_00\7&E7F4F9E&0&0000
  Name=HID Keyboard Device
  DeviceID=USB\VID_046D&PID_C517&MI_01\6&28A341C9&0&0001
  Name=USB Input Device
  DeviceID=HID\VID_046D&PID_C517&MI_01&COL01\7&1557EE24&0&0000
  Name=HID-compliant mouse
  DeviceID=HID\VID_046D&PID_C517&MI_01&COL02\7&1557EE24&0&0001
  Name=HID-compliant consumer control device
  DeviceID=HID\VID_046D&PID_C517&MI_01&COL03\7&1557EE24&0&0002
  Name=HID-compliant device
  DeviceID=HID\VID_046D&PID_C517&MI_01&COL04\7&1557EE24&0&0003
  Name=HID-compliant device
  DeviceID=HID\VID_046D&PID_C517&MI_01&COL05\7&1557EE24&0&0004
  Name=HID-compliant device
DeviceID=PCI\VEN_10DE&DEV_03F2&SUBSYS_26061019&REV_A3\3&2411E6FE&1&11
Name=Standard Enhanced PCI to USB Host Controller
  DeviceID=USB\ROOT_HUB20\4&30388C88&0
  Name=USB Root Hub
  DeviceID=USB\VID_058F&PID_6377\920321111113
  Name=USB Mass Storage Device
  DeviceID=USBSTOR\DISK&VEN_GENERIC&PROD_USB_SD_READER&REV_1.00\920321111113&0
    --> USB disk found
        Owner Device Id is USB\VID_058F&PID_6377\920321111113
        VID=$058F  PID=$6377
  Name=Generic USB SD Reader USB Device
  DeviceID=USBSTOR\DISK&VEN_GENERIC&PROD_USB_CF_READER&REV_1.01\920321111113&1
    --> USB disk found
        Owner Device Id is USBSTOR\DISK&VEN_GENERIC&PROD_USB_SD_READER&REV_1.00\920321111113&0
  Name=Generic USB CF Reader USB Device
  DeviceID=USBSTOR\DISK&VEN_GENERIC&PROD_USB_SM_READER&REV_1.02\920321111113&2
    --> USB disk found
        Owner Device Id is USBSTOR\DISK&VEN_GENERIC&PROD_USB_CF_READER&REV_1.01\920321111113&1
  Name=Generic USB SM Reader USB Device
  DeviceID=USBSTOR\DISK&VEN_GENERIC&PROD_USB_MS_READER&REV_1.03\920321111113&3
    --> USB disk found
        Owner Device Id is USBSTOR\DISK&VEN_GENERIC&PROD_USB_SM_READER&REV_1.02\920321111113&2
  Name=Generic USB MS Reader USB Device
 
BytesPerSector=512
Caption=ST350041 0AS SCSI Disk Device
DeviceID=\\.\PHYSICALDRIVE0
InterfaceType=SCSI
MediaLoaded=True
Model=ST350041 0AS SCSI Disk Device
Name=\\.\PHYSICALDRIVE0
Partitions=1
SCSIBus=1
SCSILogicalUnit=0
SCSIPort=2
SCSITargetId=1
Using TSmartHardDiskPhysical
  Error identifying using TSmartHardDiskPhysical
  Error reading attrs using TSmartHardDiskPhysical
  Error reading thrs using TSmartHardDiskPhysical
  Error reading Smart Log Directory using TSmartHardDiskPhysical
  Error reading Summary Smart Error Log using TSmartHardDiskPhysical
  Error reading Smart Self-Test Log using TSmartHardDiskPhysical
Using TSmartHardDiskSCSI
    Identify Sector -->
      000  5A 0C FF 3F 37 C8 10 00 00 00 00 00 3F 00 00 00 00 00 00 00 20 20 20 20 20 20 20 20 20 20 20 20 Z.ÿ?7È......?.......            
      020  35 56 4D 30 35 39 33 33 00 00 00 80 04 00 43 43 33 33 20 20 20 20 53 54 33 35 30 30 34 31 30 41 5VM05933...€..CC33    ST3500410A
      040  53 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 10 80 S                             .€
      060  00 00 00 2F 00 40 00 02 00 02 07 00 FF 3F 10 00 3F 00 10 FC FB 00 10 01 FF FF FF 0F 00 00 07 00 .../.@......ÿ?..?..üû...ÿÿÿ.....
      080  03 00 78 00 78 00 78 00 78 00 00 00 00 00 00 00 00 00 00 00 00 00 1F 00 06 05 00 00 40 00 40 00 ..x.x.x.x...................@.@.
      0A0  F0 01 29 00 6B 34 61 7F 63 41 49 34 01 BE 63 41 7F 40 28 00 28 00 00 00 FE FF 00 00 00 FE 00 00 ð.).k4acAI4.¾cA@(.(...þÿ...þ..
      0C0  00 00 00 00 00 00 00 00 30 60 38 3A 00 00 00 00 00 00 00 00 00 00 00 00 00 50 00 C5 4B 12 CD 87 ........0`8:.............P.ÅK.Í‡
      0E0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 1E 40 1C 40 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ...............@.@..............
      100  29 00 30 60 38 3A 30 60 38 3A 20 20 02 00 40 01 00 01 00 50 06 3C 0A 3C 00 00 3C 00 00 00 08 00 ).0`8:0`8:  ..@....P.<.<..<.....
      120  00 00 00 00 4F 00 80 02 00 00 00 00 08 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 3F 00 80 ....O.€......................?.€
      140  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................................
      160  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................................
      180  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 3F 10 00 00 ............................?...
      1A0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 20 1C 00 00 00 00 00 00 00 00 10 10 00 00 .................. .............
      1C0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................................
      1E0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 A5 DD ..............................¥Ý
      000  0A 00 01 0F 00 75 63 3C 23 69 08 00 00 00 03 03 00 61 61 00 00 00 00 00 00 00 04 32 00 62 62 E7
      020  0A 00 00 00 00 00 05 33 00 64 64 00 00 00 00 00 00 00 07 0F 00 46 3C E3 D8 A0 00 01 00 00 09 32
      040  00 5C 5C 98 1E 00 00 00 00 00 0A 13 00 64 64 00 00 00 00 00 00 00 0C 32 00 64 25 21 01 00 00 00
      060  00 00 B8 32 00 64 64 00 00 00 00 00 00 00 BB 32 00 64 64 00 00 00 00 00 00 00 BC 32 00 64 64 00
      080  00 00 00 00 00 00 BD 3A 00 64 64 00 00 00 00 00 00 00 BE 22 00 44 2C 20 00 16 23 03 00 00 C2 22
      0A0  00 20 38 20 00 00 00 0A 00 00 C3 1A 00 28 16 3C 23 69 08 00 00 00 C5 12 00 64 64 00 00 00 00 00
      0C0  00 00 C6 10 00 64 64 00 00 00 00 00 00 00 C7 3E 00 C8 C8 00 00 00 00 00 00 00 F0 00 00 64 FD D9
      0E0  1B 00 00 0C 65 08 F1 00 00 64 FD 19 E1 F8 66 00 00 00 F2 00 00 64 FD 43 6F 30 E1 00 00 00 00 00
      100  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      120  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      140  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      160  00 00 00 00 00 00 00 00 00 00 82 00 58 02 00 7B 03 00 01 00 01 5E 02 00 00 00 00 00 00 00 00 00
      180  00 00 00 00 0C 0B 00 00 00 03 03 03 03 03 03 03 03 00 00 00 00 00 00 00 00 01 00 00 00 00 00 00
      1A0  00 00 00 00 00 00 00 00 EF 4A 4F 97 AE 19 00 00 00 00 00 00 01 00 A8 00 19 E1 F8 66 27 04 00 00
      1C0  43 6F 30 E1 9B 02 00 00 00 00 00 00 B9 B9 08 03 00 00 00 00 00 00 00 00 19 1E 00 00 7D 00 0B 00
      1E0  00 00 00 00 A4 00 01 00 00 00 00 00 00 00 00 23 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 95
    Smart Log Directory -->
      000  01 00 01 00 05 00 05 00 00 00 00 00 01 00 01 00 00 00 01 00 00 00 00 00 00 00 00 00 00 00 00 00
      020  01 00 01 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      040  00 00 01 00 01 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      060  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      080  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      0A0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      0C0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      0E0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      100  10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00
      120  10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00
      140  00 00 14 00 00 00 00 00 00 00 00 00 00 00 00 00 81 00 01 00 00 00 00 00 00 00 00 00 00 00 00 00
      160  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 FC 00 00 00 00 00
      180  01 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      1A0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      1C0  01 00 01 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      1E0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      Smart Logging Version=$0001
      Log #$01 contains 1 pages
      Log #$02 contains 5 pages
      Log #$03 contains 5 pages
      Log #$06 contains 1 pages
      Log #$07 contains 1 pages
    Smart Summary Error Log -->
      000  01 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      020  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      040  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      060  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      080  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      0A0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      0C0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      0E0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      100  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      120  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      140  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      160  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      180  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      1A0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      1C0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      1E0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 FF
      Error Log Version=$0001
      Error Log Index=0
      Device Error Count=0
    Smart Self-Test Log -->
      000  01 00 01 00 06 00 09 00 00 00 00 00 39 00 00 00 00 00 00 00 00 00 00 00 00 00 01 00 1E 12 09 00
      020  00 00 00 00 39 00 00 00 00 00 00 00 00 00 00 00 00 00 02 19 1E 12 06 00 00 00 00 00 F9 01 00 00
      040  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      060  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      080  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      0A0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      0C0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      0E0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      100  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      120  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      140  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      160  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      180  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      1A0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      1C0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      1E0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 03 00 00 F5
      Revision=$0001
      Self-Test Index=3
      Entry  1 : Short offline       -  Completed without error       - 100%  -  Failure Checkpoint is   9  -  Failing LBA is --------
      Entry  2 : Short offline       -  Completed without error       - 100%  -  Failure Checkpoint is   9  -  Failing LBA is --------
      Entry  3 : Extended offline    -  Aborted by host               -  90%  -  Failure Checkpoint is   6  -  Failing LBA is --------
 
BytesPerSector=512
Caption=WDC WD32 00AAJS-22L7A SCSI Disk Device
DeviceID=\\.\PHYSICALDRIVE1
InterfaceType=SCSI
MediaLoaded=True
Model=WDC WD32 00AAJS-22L7A SCSI Disk Device
Name=\\.\PHYSICALDRIVE1
Partitions=4
SCSIBus=1
SCSILogicalUnit=0
SCSIPort=3
SCSITargetId=1
Using TSmartHardDiskPhysical
  Error identifying using TSmartHardDiskPhysical
  Error reading attrs using TSmartHardDiskPhysical
  Error reading thrs using TSmartHardDiskPhysical
  Error reading Smart Log Directory using TSmartHardDiskPhysical
  Error reading Summary Smart Error Log using TSmartHardDiskPhysical
  Error reading Smart Self-Test Log using TSmartHardDiskPhysical
Using TSmartHardDiskSCSI
    Identify Sector -->
      000  7A 42 FF 3F 37 C8 10 00 00 00 00 00 3F 00 00 00 00 00 00 00 20 20 20 20 20 57 44 2D 57 4D 41 56 zBÿ?7È......?.......     WD-WMAV
      020  32 30 38 37 34 34 35 33 00 00 00 40 32 00 30 31 2E 30 33 45 30 31 57 44 43 20 57 44 33 32 30 30 20874453...@2.01.03E01WDC WD3200
      040  41 41 4A 53 2D 32 32 4C 37 41 30 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 10 80 AAJS-22L7A0                   .€
      060  00 00 00 2F 01 40 00 00 00 00 07 00 FF 3F 10 00 3F 00 10 FC FB 00 10 01 FF FF FF 0F 00 00 07 00 .../.@......ÿ?..?..üû...ÿÿÿ.....
      080  03 00 78 00 78 00 78 00 78 00 00 00 00 00 00 00 00 00 00 00 00 00 1F 00 06 07 00 00 44 00 40 00 ..x.x.x.x...................D.@.
      0A0  FE 01 00 00 6B 74 61 7F 23 41 69 74 41 BC 23 41 7F 40 1D 00 1D 00 00 00 FE FF 00 00 FE 80 00 00 þ...kta#AitA¼#A@......þÿ..þ€..
      0C0  00 00 00 00 00 00 00 00 B0 EA 42 25 00 00 00 00 00 00 00 00 00 00 00 00 01 50 E0 4E A9 AB 01 7D ........°êB%.............PàN©«.}
      0E0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 10 40 10 40 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ...............@.@..............
      100  29 00 00 00 00 00 00 00 00 00 CB 16 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 04 00 00 00 ).........Ë.....................
      120  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................................
      140  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................................
      160  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................................
      180  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 3F 30 00 00 ............................?0..
      1A0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 0E 10 00 00 ................................
      1C0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 01 00 00 10 00 00 00 00 00 00 00 00 ................................
      1E0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 A5 9F ..............................¥Ÿ
      000  10 00 01 2F 00 C8 C8 00 00 00 00 00 00 00 03 27 00 8A 88 04 10 00 00 00 00 00 04 32 00 64 64 FD
      020  01 00 00 00 00 00 05 33 00 C8 C8 00 00 00 00 00 00 00 07 2E 00 64 FD 00 00 00 00 00 00 00 09 32
      040  00 58 58 04 24 00 00 00 00 00 0A 32 00 64 64 00 00 00 00 00 00 00 0B 32 00 64 64 00 00 00 00 00
      060  00 00 0C 32 00 64 64 FA 01 00 00 00 00 00 C0 32 00 C8 C8 53 00 00 00 00 00 00 C1 32 00 C8 C8 FD
      080  01 00 00 00 00 00 C2 22 00 6C 63 23 00 00 00 00 00 00 C4 32 00 C8 C8 00 00 00 00 00 00 00 C5 32
      0A0  00 C8 C8 02 00 00 00 00 00 00 C6 30 00 C8 C8 00 00 00 00 00 00 00 C7 32 00 C8 C8 00 00 00 00 00
      0C0  00 00 C8 08 00 C8 C8 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      0E0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      100  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      120  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      140  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      160  00 00 00 00 00 00 00 00 00 00 84 00 80 16 01 7B 03 00 01 00 02 46 05 00 00 00 00 00 00 00 00 00
      180  00 00 01 02 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      1A0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      1C0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      1E0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 D5
    Smart Log Directory -->
      000  01 00 01 00 05 00 00 00 00 00 00 00 01 00 00 00 00 00 01 00 00 00 00 00 00 00 00 00 00 00 00 00
      020  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      040  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      060  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      080  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      0A0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      0C0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      0E0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      100  10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00
      120  10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00
      140  10 00 10 00 10 00 10 00 10 00 10 00 10 00 10 00 01 00 01 00 01 00 01 00 01 00 01 00 01 00 01 00
      160  01 00 01 00 01 00 01 00 01 00 01 00 01 00 01 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      180  01 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      1A0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      1C0  01 00 01 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      1E0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      Smart Logging Version=$0001
      Log #$01 contains 1 pages
      Log #$02 contains 5 pages
      Log #$06 contains 1 pages
    Smart Summary Error Log -->
      000  01 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      020  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      040  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      060  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      080  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      0A0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      0C0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      0E0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      100  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      120  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      140  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      160  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      180  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      1A0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      1C0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      1E0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 FF
      Error Log Version=$0001
      Error Log Index=0
      Device Error Count=0
    Smart Self-Test Log -->
      000  01 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      020  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      040  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      060  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      080  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      0A0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      0C0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      0E0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      100  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      120  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      140  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      160  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      180  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      1A0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      1C0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      1E0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 FF
      Revision=$0001
      Self-Test Index=0
 
Caption=Generic USB CF Reader USB Device
DeviceID=\\.\PHYSICALDRIVE3
InterfaceType=USB
MediaLoaded=True
Model=Generic USB CF Reader USB Device
Name=\\.\PHYSICALDRIVE3
Partitions=0
Using TSmartHardDiskPhysical
  Error identifying using TSmartHardDiskPhysical
  Error reading attrs using TSmartHardDiskPhysical
  Error reading thrs using TSmartHardDiskPhysical
  Error reading Smart Log Directory using TSmartHardDiskPhysical
  Error reading Summary Smart Error Log using TSmartHardDiskPhysical
  Error reading Smart Self-Test Log using TSmartHardDiskPhysical
 
Caption=Generic USB MS Reader USB Device
DeviceID=\\.\PHYSICALDRIVE5
InterfaceType=USB
MediaLoaded=True
Model=Generic USB MS Reader USB Device
Name=\\.\PHYSICALDRIVE5
Partitions=0
Using TSmartHardDiskPhysical
  Error identifying using TSmartHardDiskPhysical
  Error reading attrs using TSmartHardDiskPhysical
  Error reading thrs using TSmartHardDiskPhysical
  Error reading Smart Log Directory using TSmartHardDiskPhysical
  Error reading Summary Smart Error Log using TSmartHardDiskPhysical
  Error reading Smart Self-Test Log using TSmartHardDiskPhysical
 
BytesPerSector=512
Caption=Generic USB SD Reader USB Device
DeviceID=\\.\PHYSICALDRIVE2
InterfaceType=USB
MediaLoaded=True
Model=Generic USB SD Reader USB Device
Name=\\.\PHYSICALDRIVE2
Partitions=1
\\.\PHYSICALDRIVE2 (Generic USB SD Reader USB Device) - VID=$058F  PID=$6377
Using TSmartHardDiskPhysical
  Error identifying using TSmartHardDiskPhysical
  Error reading attrs using TSmartHardDiskPhysical
  Error reading thrs using TSmartHardDiskPhysical
  Error reading Smart Log Directory using TSmartHardDiskPhysical
  Error reading Summary Smart Error Log using TSmartHardDiskPhysical
  Error reading Smart Self-Test Log using TSmartHardDiskPhysical
 
Caption=Generic USB SM Reader USB Device
DeviceID=\\.\PHYSICALDRIVE4
InterfaceType=USB
MediaLoaded=True
Model=Generic USB SM Reader USB Device
Name=\\.\PHYSICALDRIVE4
Partitions=0
Using TSmartHardDiskPhysical
  Error identifying using TSmartHardDiskPhysical
  Error reading attrs using TSmartHardDiskPhysical
  Error reading thrs using TSmartHardDiskPhysical
  Error reading Smart Log Directory using TSmartHardDiskPhysical
  Error reading Summary Smart Error Log using TSmartHardDiskPhysical
  Error reading Smart Self-Test Log using TSmartHardDiskPhysical
AdvSMART debug messages end <--
SMART Hard disks found: 2
Found ST3500410AS on AdvSMART
  HD00 -> <\\.\PHYSICALDRIVE0> (SCSI    ) Model: <ST3500410AS> - Firmware: <CC33> - Serial: <5VM05933>
    AAM:supported (currently enabled)
    APM:unsupported (currently disabled)
    Power Management:supported (currently enabled)
    SMART:supported (currently enabled)
    48-bit Addressing:supported
    Max Queue Depth=32
    NCQ:supported
    SATA I (1.5Gb/s):unsupported
    SATA II (3.0Gb/s):supported
    UDMA0:supported (currently disabled)
    UDMA1:supported (currently disabled)
    UDMA2:supported (currently disabled)
    UDMA3:supported (currently disabled)
    UDMA4:supported (currently disabled)
    UDMA5:supported (currently disabled)
    UDMA6:supported (currently enabled)
SMART Structure Revision : $000A
ID=$01  NAME=Raw Read Error Rate  VALUE=$75  WORST=$63  RAW=$00000869233C  THRSHLD=$06  FLAGS=$000F
ID=$03  NAME=Spin Up Time  VALUE=$61  WORST=$61  RAW=$000000000000  THRSHLD=$00  FLAGS=$0003
ID=$04  NAME=Start/Stop Count  VALUE=$62  WORST=$62  RAW=$000000000AE7  THRSHLD=$14  FLAGS=$0032
ID=$05  NAME=Reallocated Sector Count  VALUE=$64  WORST=$64  RAW=$000000000000  THRSHLD=$24  FLAGS=$0033
ID=$07  NAME=Seek Error Rate  VALUE=$46  WORST=$3C  RAW=$000100A0D8E3  THRSHLD=$1E  FLAGS=$000F
ID=$09  NAME=Power On Hours Count  VALUE=$5C  WORST=$5C  RAW=$000000001E98  THRSHLD=$00  FLAGS=$0032
ID=$0A  NAME=Spin Retry Count  VALUE=$64  WORST=$64  RAW=$000000000000  THRSHLD=$61  FLAGS=$0013
ID=$0C  NAME=Power Cycle Count  VALUE=$64  WORST=$25  RAW=$000000000121  THRSHLD=$14  FLAGS=$0032
ID=$B8  NAME=(Unknown Attribute)  VALUE=$64  WORST=$64  RAW=$000000000000  THRSHLD=$63  FLAGS=$0032
ID=$BB  NAME=(Unknown Attribute)  VALUE=$64  WORST=$64  RAW=$000000000000  THRSHLD=$00  FLAGS=$0032
ID=$BC  NAME=(Unknown Attribute)  VALUE=$64  WORST=$64  RAW=$000000000000  THRSHLD=$00  FLAGS=$0032
ID=$BD  NAME=(Unknown Attribute)  VALUE=$64  WORST=$64  RAW=$000000000000  THRSHLD=$00  FLAGS=$003A
ID=$BE  NAME=(Unknown Attribute)  VALUE=$44  WORST=$2C  RAW=$000323160020  THRSHLD=$2D  FLAGS=$0022
ID=$C2  NAME=Temperature  VALUE=$20  WORST=$38  RAW=$000A00000020  THRSHLD=$00  FLAGS=$0022
Current HD temperature is 32C
ID=$C3  NAME=Hardware ECC Recovered  VALUE=$28  WORST=$16  RAW=$00000869233C  THRSHLD=$00  FLAGS=$001A
ID=$C5  NAME=Current Pending Sector  VALUE=$64  WORST=$64  RAW=$000000000000  THRSHLD=$00  FLAGS=$0012
ID=$C6  NAME=Offline Correctable  VALUE=$64  WORST=$64  RAW=$000000000000  THRSHLD=$00  FLAGS=$0010
ID=$C7  NAME=UltraATA CRC Error Rate  VALUE=$C8  WORST=$C8  RAW=$000000000000  THRSHLD=$00  FLAGS=$003E
ID=$F0  NAME=Write Head  VALUE=$64  WORST=$FD  RAW=$650C00001BD9  THRSHLD=$00  FLAGS=$0000
ID=$F1  NAME=(Unknown Attribute)  VALUE=$64  WORST=$FD  RAW=$000066F8E119  THRSHLD=$00  FLAGS=$0000
ID=$F2  NAME=(Unknown Attribute)  VALUE=$64  WORST=$FD  RAW=$0000E1306F43  THRSHLD=$00  FLAGS=$0000
Adding drive #0 (ST3500410AS) found on AdvSMART
 -> Temperature 1 offset : 0
Found WDC WD3200AAJS-22L7A0 on AdvSMART
  HD01 -> <\\.\PHYSICALDRIVE1> (SCSI    ) Model: <WDC WD3200AAJS-22L7A0> - Firmware: <01.03E01> - Serial: <WD-WMAV20874453>
    AAM:supported (currently disabled)
    APM:unsupported (currently disabled)
    Power Management:supported (currently enabled)
    SMART:supported (currently enabled)
    48-bit Addressing:supported
    Max Queue Depth=32
    NCQ:supported
    SATA I (1.5Gb/s):unsupported
    SATA II (3.0Gb/s):supported
    UDMA0:supported (currently disabled)
    UDMA1:supported (currently disabled)
    UDMA2:supported (currently disabled)
    UDMA3:supported (currently disabled)
    UDMA4:supported (currently disabled)
    UDMA5:supported (currently disabled)
    UDMA6:supported (currently enabled)
SMART Structure Revision : $0010
ID=$01  NAME=Raw Read Error Rate  VALUE=$C8  WORST=$C8  RAW=$000000000000  THRSHLD=$33  FLAGS=$002F
ID=$03  NAME=Spin Up Time  VALUE=$8A  WORST=$88  RAW=$000000001004  THRSHLD=$15  FLAGS=$0027
ID=$04  NAME=Start/Stop Count  VALUE=$64  WORST=$64  RAW=$0000000001FD  THRSHLD=$00  FLAGS=$0032
ID=$05  NAME=Reallocated Sector Count  VALUE=$C8  WORST=$C8  RAW=$000000000000  THRSHLD=$8C  FLAGS=$0033
ID=$07  NAME=Seek Error Rate  VALUE=$64  WORST=$FD  RAW=$000000000000  THRSHLD=$00  FLAGS=$002E
ID=$09  NAME=Power On Hours Count  VALUE=$58  WORST=$58  RAW=$000000002404  THRSHLD=$00  FLAGS=$0032
ID=$0A  NAME=Spin Retry Count  VALUE=$64  WORST=$64  RAW=$000000000000  THRSHLD=$00  FLAGS=$0032
ID=$0B  NAME=Calibration Retry Count  VALUE=$64  WORST=$64  RAW=$000000000000  THRSHLD=$00  FLAGS=$0032
ID=$0C  NAME=Power Cycle Count  VALUE=$64  WORST=$64  RAW=$0000000001FA  THRSHLD=$00  FLAGS=$0032
ID=$C0  NAME=Power Off Retract Count  VALUE=$C8  WORST=$C8  RAW=$000000000053  THRSHLD=$00  FLAGS=$0032
ID=$C1  NAME=Load Cycle Count  VALUE=$C8  WORST=$C8  RAW=$0000000001FD  THRSHLD=$00  FLAGS=$0032
ID=$C2  NAME=Temperature  VALUE=$6C  WORST=$63  RAW=$000000000023  THRSHLD=$00  FLAGS=$0022
Current HD temperature is 35C
ID=$C4  NAME=Reallocated Event Count  VALUE=$C8  WORST=$C8  RAW=$000000000000  THRSHLD=$00  FLAGS=$0032
ID=$C5  NAME=Current Pending Sector  VALUE=$C8  WORST=$C8  RAW=$000000000002  THRSHLD=$00  FLAGS=$0032
ID=$C6  NAME=Offline Correctable  VALUE=$C8  WORST=$C8  RAW=$000000000000  THRSHLD=$00  FLAGS=$0030
ID=$C7  NAME=UltraATA CRC Error Rate  VALUE=$C8  WORST=$C8  RAW=$000000000000  THRSHLD=$00  FLAGS=$0032
ID=$C8  NAME=Write Error Rate  VALUE=$C8  WORST=$C8  RAW=$000000000000  THRSHLD=$00  FLAGS=$0008
Adding drive #1 (WDC WD3200AAJS-22L7A0) found on AdvSMART
 -> Temperature 1 offset : 0
End of SMART (Advanced Methods) probing
11:57:15.327 About to probe SCSI...
11:57:15.329 ProbeSCSI: before first LogSense
11:57:15.331 ProbeSCSI: before first LogSense
11:57:15.332 ProbeSCSI: before first LogSense
11:57:15.336 ProbeSCSI: before first LogSense
11:57:15.339 ProbeSCSI: before first LogSense
11:57:15.342 ProbeSCSI: before first LogSense
11:57:15.347 End of SCSI probing
About to probe UGURU support...
Motherboard is eMachines MCP61PM-GM
End of UGURU support probing
About to probe ACPI temperatures...
Found ACPI temperature (40.0C)
 -> Temperature 1 offset : 0
End of ACPI temperatures probing
About to probe AMD Internal Sensors...
Found AMD Athlon(tm) Dual Core Processor 4050e internal sensor for K8 CPU#0 : 16C
 -> [$E4]=$0041613E
 -> TCaseMax=49
 -> Core=1
 -> Sensor=0
 -> Offset=33
 -> Temperature 1 offset : 0
End of AMD Internal Sensors probing
About to probe INTEL Internal Sensors...
End of INTEL Internal Sensors probing
About to probe NVIDIA ControlPanel Sensors...
End of NVIDIA ControlPanel Sensors probing
End of detection
Reading Cfg Version 2.01
Old sensor no longer detected -->
Old sensor properly detected -->
  IT8712F-J on ISA @ $290
Old sensor no longer detected -->
Old sensor no longer detected -->
Old sensor properly detected -->
  AMD K8 on PCI @ $0
Old sensor no longer detected -->
PWM from IT8712F-J@$290(onISA@$290) -->
  Speed01 0 100
  properly added
PWM from IT8712F-J@$290(onISA@$290) -->
  Speed02 0 100
  properly added
PWM from IT8712F-J@$290(onISA@$290) -->
  Speed03 0 100
  properly added
PWM from IT8712F-J@$290(onISA@$290) -->
  Speed04 0 100
  properly added
PWM from IT8712F-J@$290(onISA@$290) -->
  Speed05 0 100
  properly added
Temperature from UNKNOWN (GeForce040210DE020000) -->
  GPU 40 50 0
  not found in list
Temperature from IT8712F-J@$290(onISA@$290) -->
  Temp1 40 50 0
  PWM 1 from 1
  PWM 2 from 1
  PWM 3 from 1
  PWM 4 from 1
  PWM 5 from 1
  properly added
Temperature from IT8712F-J@$290(onISA@$290) -->
  Temp2 40 50 0
  PWM 1 from 1
  PWM 2 from 1
  PWM 3 from 1
  PWM 4 from 1
  PWM 5 from 1
  properly added
Temperature from IT8712F-J@$290(onISA@$290) -->
  Temp3 40 50 0
  PWM 1 from 1
  PWM 2 from 1
  PWM 3 from 1
  PWM 4 from 1
  PWM 5 from 1
  properly added
Temperature from UNKNOWN (LM75@$4F(onSMBusnForce2@$1C40)) -->
  Temp 40 50 0
  not found in list
Temperature from AMD K8@$0(onPCI@$0) -->
  Core 40 50 0
  PWM 1 from 1
  PWM 2 from 1
  PWM 3 from 1
  PWM 4 from 1
  PWM 5 from 1
  properly added
Temperature from UNKNOWN (NVidia Video Card@$0(onNVCPL@$0)) -->
  Core 40 50 0
  not found in list
Temperature from UNKNOWN (NVidia Video Card@$0(onNVCPL@$0)) -->
  Ambient 40 50 0
  not found in list
Fan from IT8712F-J@$290(onISA@$290) -->
  Fan1
  properly added
Fan from IT8712F-J@$290(onISA@$290) -->
  Fan2
  properly added
Fan from IT8712F-J@$290(onISA@$290) -->
  Fan3
  properly added
Fan from IT8712F-J@$290(onISA@$290) -->
  Fan4
  properly added
Fan from IT8712F-J@$290(onISA@$290) -->
  Fan5
  properly added
Volt from IT8712F-J@$290(onISA@$290) -->
  Vcore1
  properly added
Volt from IT8712F-J@$290(onISA@$290) -->
  Vcore2
  properly added
Volt from IT8712F-J@$290(onISA@$290) -->
  +3.3V
  properly added
Volt from IT8712F-J@$290(onISA@$290) -->
  +5V
  properly added
Volt from IT8712F-J@$290(onISA@$290) -->
  +12V
  properly added
Volt from IT8712F-J@$290(onISA@$290) -->
  -12V
  properly added
Volt from IT8712F-J@$290(onISA@$290) -->
  -5V
  properly added
Volt from IT8712F-J@$290(onISA@$290) -->
  +5V
  properly added
Volt from IT8712F-J@$290(onISA@$290) -->
  Vbat
  properly added
Loaded 1 events
Preparing report...