Sender : th4m4st4h@yahoo.com
SpeedFan version : SpeedFan 4.21 beta 19
Motherboard model : Asus P4SD-LA

*****************************

BIOS CopyRight : A M I  - 8000427BIOS Date: 08/27/04 11:09:23 Ver: 08.00.09BIOS Date: 08/27/04 11:09:23 Ver: 08.00.09
BIOS Date : 08/27/04
BIOS Extended Info : 
BIOS Name : AT/AT COMPATIBLE

Windows NT Multiprocessor Free version 5.1.2600

2 processor(s)
Intel Corporation Intel(R) Pentium(R) 4 CPU 3.00GHz family 15 model 2 stepping 9 brand 9 3000 MHz (0 bytes level 1 - 512.0 Kb level 2 - 0 bytes level 3)
Running at 3000 MHz
I Agree to receive beta versions : ON

*****************************

LPC47M192 on ISA at $680 Fan1 : 122875   min=122875   max=122875   mean=122875
LPC47M192 on ISA at $680 Fan2 : 122875   min=122875   max=122875   mean=122875
LPC47M192 on ISA at $680 Pwm1 : 100%   min=100%   max=100%   mean=100%
LPC47M192 on ISA at $680 Pwm2 : 100%   min=100%   max=100%   mean=100%
[$56]=$FF  [$57]=$FF  [$58]=$FF  [$59]=$FF
[$5A]=$FF  [$5B]=$FF  [$5C]=$FF
SMSC H/M Block on Intel SMBus at $2D Ambient : 36.0   min=35.0   max=37.0   mean=35.9
SMSC H/M Block on Intel SMBus at $2D Remote 1 : 46.0   min=46.0   max=51.0   mean=47.7
SMSC H/M Block on Intel SMBus at $2D Remote 2 : 35.0   min=35.0   max=35.0   mean=35.0
SMSC H/M Block on Intel SMBus at $2D +2.5V : 2.49   min=2.47   max=2.49   mean=2.48
SMSC H/M Block on Intel SMBus at $2D Vcore : 1.45   min=1.44   max=1.45   mean=1.44
SMSC H/M Block on Intel SMBus at $2D +3.3V : 3.33   min=3.33   max=3.33   mean=3.33
SMSC H/M Block on Intel SMBus at $2D +5V : 5.05   min=5.05   max=5.05   mean=5.05
SMSC H/M Block on Intel SMBus at $2D +12V : 12.06   min=12.00   max=12.06   mean=12.05
SMSC H/M Block on Intel SMBus at $2D +3.3V : 3.33   min=3.32   max=3.33   mean=3.33
SMSC H/M Block on Intel SMBus at $2D +1.5V : 1.52   min=1.52   max=1.53   mean=1.53
SMSC H/M Block on Intel SMBus at $2D +1.8V : 1.75   min=1.75   max=1.75   mean=1.75
HD0 (40.0GB) on SMART at $0 HD0 : 39.0   min=39.0   max=39.0   mean=39.0
ST340014AS (drive 0) : fitness=43%   performance=100%

*****************************

Ambient --> active=ON  chip=1  index=1 wanted=40  warning=50  offset=0  InTray=OFF Used pwms=1 2 
CPU --> active=ON  chip=1  index=2 wanted=40  warning=50  offset=0  InTray=ON Used pwms=1 2 
Mobo --> active=ON  chip=1  index=3 wanted=40  warning=50  offset=0  InTray=OFF Used pwms=1 2 
HD0 --> active=ON  chip=2  index=1 wanted=40  warning=50  offset=0  InTray=OFF Used pwms=1 2 
Fan01 --> active=ON  chip=0  index=1
Fan02 --> active=ON  chip=0  index=2
Speed01 --> active=ON  chip=0  index=1  min=0  max=100  variate=OFF
Speed02 --> active=ON  chip=0  index=2  min=0  max=100  variate=OFF
+2.5V --> active=ON  chip=1  index=1
Vcore --> active=ON  chip=1  index=2
+3.3V --> active=ON  chip=1  index=3
+5V --> active=ON  chip=1  index=4
+12V --> active=ON  chip=1  index=5
+3.3V --> active=ON  chip=1  index=6
+1.5V --> active=ON  chip=1  index=7
+1.8V --> active=ON  chip=1  index=8
Set Fans to 100% on exit : ON
Debug Mode : ON
Use ISA : ON
Use SMB : ON
Scan PCI : ON
Scan SMB : ON
Slow SMB detection : OFF
Detect SuperIO : ON
ASUS Card Detect : ON
DELL Support : OFF
Command line : "C:\Program Files\SpeedFan\speedfan.exe" 
Delta Fan Speed : 10

*****************************

Chipset : Intel 82801EB ICH5
SMBus Base Address : $0400
SMBus Revision : 00000002
SMBus I/O Enabled : ON

*****************************

Bus : 00 Device: 00 Function : 00 --> 25708086 Vendor : 8086 Device : 2570 (rev 02) - Intel Corporation 82865G/PE/P, 82848P DRAM Controller / Host-Hub Interface
00: 8086 2570 0006 2090 0002 0600 0000 0000 0008 F800 0000 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 1043 80A5 0000 0000 00E4 0000 0000 0000 0000 0000
40: 0000 0000 0000 0000 0000 0000 0000 0000 0200 0008 8040 001C 0000 0000 0000 0000
60: 0500 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0000 0000 0000 0000 0000 0000 0000 0000 1110 0011 3300 0033 0000 0000 0A00 0038
A0: 0002 0030 4A1B 1F00 0312 0000 0000 0000 0080 0000 0030 0000 5000 0000 1020 0000
C0: 0000 0000 4000 280E 0000 0000 0000 0000 2802 0E04 0D0B 0000 0000 0000 0000 0140
E0: 0000 0000 A009 0106 0200 0000 0000 0000 0000 0000 0000 0000 0F68 0003 0000 0000

Bus : 00 Device: 01 Function : 00 --> 25718086 Vendor : 8086 Device : 2571 (rev 02) - Intel Corporation 82865G/PE/P, 82848P PCI-to-AGP Bridge
00: 8086 2571 0107 00A0 0002 0604 4000 0001 0000 0000 0000 0000 0100 4001 A0A0 22A0
20: FE90 FE90 D7F0 F7E0 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0008
40: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
60: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0F68 0003 0000 0000

Bus : 00 Device: 29 Function : 00 --> 24D28086 Vendor : 8086 Device : 24D2 (rev 02) - Intel Corporation 82801EB/ER USB UHCI Controller #1
00: 8086 24D2 0005 0280 0002 0C03 0000 0080 0000 0000 0000 0000 0000 0000 0000 0000
20: E001 0000 0000 0000 0000 0000 1043 80A6 0000 0000 0000 0000 0000 0000 0110 0000
40: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
60: 0010 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 2F00 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0F66 0005 0000 0000

Bus : 00 Device: 29 Function : 01 --> 24D48086 Vendor : 8086 Device : 24D4 (rev 02) - Intel Corporation 82801EB/ER USB UHCI Controller #2
00: 8086 24D4 0005 0280 0002 0C03 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
20: E401 0000 0000 0000 0000 0000 1043 80A6 0000 0000 0000 0000 0000 0000 0213 0000
40: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
60: 0010 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 2F00 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0F66 0005 0000 0000

Bus : 00 Device: 29 Function : 02 --> 24D78086 Vendor : 8086 Device : 24D7 (rev 02) - Intel Corporation 82801EB/ER USB UHCI Controller #3
00: 8086 24D7 0005 0280 0002 0C03 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
20: E801 0000 0000 0000 0000 0000 1043 80A6 0000 0000 0000 0000 0000 0000 0312 0000
40: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
60: 0010 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 2F00 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0F66 0005 0000 0000

Bus : 00 Device: 29 Function : 03 --> 24DE8086 Vendor : 8086 Device : 24DE (rev 02) - Intel Corporation 82801EB/ER USB UHCI Controller #4
00: 8086 24DE 0005 0280 0002 0C03 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
20: EC01 0000 0000 0000 0000 0000 1043 80A6 0000 0000 0000 0000 0000 0000 0110 0000
40: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
60: 0010 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 2F00 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0F66 0005 0000 0000

Bus : 00 Device: 29 Function : 07 --> 24DD8086 Vendor : 8086 Device : 24DD (rev 02) - Intel Corporation 82801EB/ER USB EHCI Controller
00: 8086 24DD 0106 0290 2002 0C03 0000 0000 FC00 FEBF 0000 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 1043 80A6 0000 0000 0050 0000 0000 0000 0417 0000
40: 0000 0000 0000 0000 0000 0000 0000 0000 5801 C9C2 0000 0000 000A 20A0 0000 0000
60: 2020 01FF 0000 0000 0001 0101 0005 E000 0000 3FCF 0000 0000 0000 0000 0000 0000
80: 0000 0000 0001 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 5555 0000 0000 003F
E0: 0000 0000 0000 0000 0000 0000 0000 0000 8000 0000 8388 0040 0F66 0005 1406 0000

Bus : 00 Device: 30 Function : 00 --> 244E8086 Vendor : 8086 Device : 244E (rev C2) - Intel Corporation 82801BA/CA/DB/DBL/Ex/Fx/FRW, 6300ESB Hub Interface to PCI Bridge
00: 8086 244E 0107 0080 00C2 0604 0000 0001 0000 0000 0000 0000 0200 4002 B0B0 2280
20: FEA0 FEA0 FFF0 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0006
40: 2802 7630 0000 0000 0000 0000 0000 0000 6402 0073 0000 0000 0150 0034 0000 0000
60: 0000 0000 0000 0000 0000 0000 0000 0000 0010 0000 0000 0000 0000 0000 0000 0000
80: 0000 0086 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0001 0002 0000 00C0 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0F66 0005 0000 3151

Bus : 00 Device: 31 Function : 00 --> 24D08086 Vendor : 8086 Device : 24D0 (rev 02) - Intel Corporation 82801EB/ER LPC Interface Bridge
00: 8086 24D0 000F 0280 0002 0601 0000 0080 0000 0000 0000 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
40: 0801 0000 0010 0000 0000 0000 0000 0000 0000 0000 0000 0000 0481 0000 0010 0000
60: 8A8A 8385 00D0 0000 8080 8B80 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0000 0000 0000 0000 0000 0000 0000 0000 FCFF 0000 0000 0000 0000 0000 0000 0000
A0: 0220 0000 0001 0000 000D 0000 0300 0000 0000 0000 0000 0000 8000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 2186 0000 0F02 0000 0004 0000 0000 0000
E0: 0000 8000 0000 1408 2233 0011 0000 4567 0000 0060 0004 0000 0F66 3E05 0000 0000

Bus : 00 Device: 31 Function : 01 --> 24DB8086 Vendor : 8086 Device : 24DB (rev 02) - Intel Corporation 82801EB/ER EIDE Controller
00: 8086 24DB 0007 0288 8A02 0101 0000 0000 0001 0000 0001 0000 0001 0000 0001 0000
20: FC01 0000 FC00 FFEF 0000 0000 1043 80A6 0000 0000 0000 0000 0000 0000 0100 0000
40: 8000 A303 0000 0000 0004 0200 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
60: 0008 0000 0000 0000 0008 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0F66 0005 0000 0000

Bus : 00 Device: 31 Function : 02 --> 24D18086 Vendor : 8086 Device : 24D1 (rev 02) - Intel Corporation 82801EB SATA Controller
00: 8086 24D1 0005 02A0 8F02 0101 0000 0000 DC01 0000 D801 0000 D401 0000 D001 0000
20: CC01 0000 0000 0000 0000 0000 1043 80A6 0000 0000 0000 0000 0000 0000 0112 0000
40: A307 8000 0000 0000 0001 0001 0000 0000 0000 0000 1030 0010 0000 0000 0000 0000
60: 0000 0000 0000 0000 0000 0000 0000 0000 0001 0002 0000 0000 0000 0000 0000 0000
80: 7005 0000 0000 0000 0000 0000 0000 0000 0000 0013 0020 0000 0000 0000 0000 0000
A0: 0040 0000 0043 0022 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0F66 0005 0000 0000

Bus : 00 Device: 31 Function : 03 --> 24D38086 Vendor : 8086 Device : 24D3 (rev 02) - Intel Corporation 82801EB/ER SMBus Controller
00: 8086 24D3 0001 0280 0002 0C05 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
20: 0401 0000 0000 0000 0000 0000 1043 80A6 0000 0000 0000 0000 0000 0000 020A 0000
40: 0001 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
60: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0F66 0005 0000 0000

Bus : 01 Device: 00 Function : 00 --> 4E481002 Vendor : 1002 Device : 4E48 (rev 00) - ATI R350 Radeon 9800 Pro
00: 1002 4E48 0187 02B0 0000 0300 FF04 0080 0008 E800 A801 0000 0000 FE9F 0000 0000
20: 0000 0000 0000 0000 0000 0000 1002 0002 0000 FE9C 0058 0000 0000 0000 0110 0008
40: 0000 0000 0000 0000 0000 0000 1002 0002 0001 0602 0000 0000 5002 0030 021B FF00
60: 4312 1F00 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0005 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000

Bus : 01 Device: 00 Function : 01 --> 4E681002 Vendor : 1002 Device : 4E68 (rev 00) - ATI R350 Radeon 9800 Pro - Secondary
00: 1002 4E68 0087 02B0 0000 0380 4004 0000 0008 E000 0000 FE9E 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 1002 0003 0000 0000 0050 0000 0000 0000 00FF 0008
40: 0000 0000 0000 0000 0000 0000 0000 0000 0001 0602 0000 0000 5002 0030 021B FF00
60: 0200 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000

Bus : 02 Device: 11 Function : 00 --> 00061102 Vendor : 1102 Device : 0006 (rev 00) - Creative Labs emu10k1x Soundblaster Live! 5.1
00: 1102 0006 0105 0290 0000 0401 4000 0080 B801 0000 0000 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 1102 1003 0000 0000 00DC 0000 0000 0000 0117 1402
40: 0000 0000 0000 0000 0000 0000 8200 0000 8000 0000 0000 0000 0000 0000 0000 0000
60: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0001 0622
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000

Bus : 02 Device: 11 Function : 01 --> 70041102 Vendor : 1102 Device : 7004 (rev 00) - <Unknown device>
00: 1102 7004 0105 0290 0000 0980 4000 0080 BC01 0000 0000 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 1102 1003 0000 0000 00DC 0000 0000 0000 0000 0000
40: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
60: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0001 0622
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000

Bus : 02 Device: 15 Function : 00 --> 813910EC Vendor : 10EC Device : 8139 (rev 10) - Realtek Semiconductor RTL8139A/B/C Fast Ethernet Adapter
00: 10EC 8139 0105 0290 0010 0200 4000 0000 B401 0000 F400 FEAF 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 1043 80B3 0000 0000 0050 0000 0000 0000 0113 4020
40: 0000 0000 0000 0000 0000 0000 0000 0000 0001 F7C2 0100 0000 0000 0000 0000 0000
60: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000

*****************************

ISA Dump from address $290 --> <Unknown> (ISA at $0290) (No error)
00: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
10: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
20: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
30: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
40: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
50: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
60: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
70: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
80: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
90: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
A0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
B0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
C0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
D0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
E0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
F0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................

*****************************

SMB Dump from address $2D --> <SMSC H/M Block> (SMBus at $0400) (No error)
00: -- -- -- -- -- -- -- -- -- -- -- -- -- -- -- --   ................
10: -- -- -- -- -- -- -- -- -- -- -- -- -- -- 00 00   ................
20: BE 79 C2 C3 BF C1 2F 23 -- -- -- FD EF FF FF FF   .y..../#........
30: FF FF FF FF FD DF FF 41 80 7F 80 -- -- -- 55 20   .......A......U
40: 09 0F 0F -- -- -- -- 0F -- 80 00 32 00 00 -- 04   ...........2....
50: C3 BB 23 -- 7F FF FF FF 7F 80 -- -- -- -- -- --   ..#.............
60: -- -- -- -- -- -- -- -- -- -- -- -- -- -- -- --   ................
70: -- -- -- -- -- -- -- -- -- -- -- -- -- -- -- --   ................
80: -- -- -- -- -- -- -- -- -- -- -- -- -- -- -- --   ................
90: -- -- -- -- -- -- -- -- -- -- -- -- -- -- -- --   ................
A0: -- -- -- -- -- -- -- -- -- -- -- -- -- -- -- --   ................
B0: -- -- -- -- -- -- -- -- -- -- -- -- -- -- -- --   ................
C0: -- -- -- -- -- -- -- -- -- -- -- -- -- -- -- --   ................
D0: -- -- -- -- -- -- -- -- -- -- -- -- -- -- -- --   ................
E0: -- -- -- -- -- -- -- -- -- -- -- -- -- -- -- --   ................
F0: -- -- -- -- -- -- -- -- -- -- -- -- -- -- -- --   ................
SMB Dump from address $30 --> <Unknown> (SMBus at $0400) (No error)
00: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
10: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
20: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
30: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
40: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
50: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
60: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
70: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
80: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
90: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
A0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
B0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
C0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
D0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
E0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
F0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
SMB Dump from address $32 --> <Unknown> (SMBus at $0400) (No error)
00: -- -- -- -- -- -- -- -- -- -- -- -- -- -- -- --   ................
10: -- -- -- -- -- -- -- -- -- -- -- -- -- -- -- --   ................
20: -- -- -- -- -- -- -- -- -- -- -- -- -- -- -- --   ................
30: -- -- -- -- -- -- -- -- -- -- -- -- -- -- -- --   ................
40: -- -- -- -- -- -- -- -- -- -- -- -- -- -- -- --   ................
50: -- -- -- -- -- -- -- -- -- -- -- -- -- -- -- --   ................
60: -- -- -- -- -- -- -- -- -- -- -- -- -- -- -- --   ................
70: -- -- -- -- -- -- -- -- -- -- -- -- -- -- -- --   ................
80: -- -- -- -- -- -- -- -- -- -- -- -- -- -- -- --   ................
90: -- -- -- -- -- -- -- -- -- -- -- -- -- -- -- --   ................
A0: -- -- -- -- -- -- -- -- -- -- -- -- -- -- -- --   ................
B0: -- -- -- -- -- -- -- -- -- -- -- -- -- -- -- --   ................
C0: -- -- -- -- -- -- -- -- -- -- -- -- -- -- -- --   ................
D0: -- -- -- -- -- -- -- -- -- -- -- -- -- -- -- --   ................
E0: -- -- -- -- -- -- -- -- -- -- -- -- -- -- -- --   ................
F0: -- -- -- -- -- -- -- -- -- -- -- -- -- -- -- --   ................
SMB Dump from address $44 --> <Unknown> (SMBus at $0400) (No error)
00: 00 00 0F 04 00 00 00 00 00 00 00 00 00 00 00 00   ................
10: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
20: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
30: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
40: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
50: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
60: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
70: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
80: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
90: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
A0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
B0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
C0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
D0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
E0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
F0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
SMB Dump from address $50 --> <RAM> (SMBus at $0400) (No error)
00: 80 08 07 0D 0A 02 40 00 04 50 65 00 82 08 00 01   ......@..Pe.....
10: 0E 04 18 01 02 20 C0 60 70 00 00 3C 28 3C 28 40   ..... .`p..<(<(@
20: 60 60 40 40 00 00 00 00 00 37 46 28 28 50 00 00   ``@@.....7F((P..
30: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 10 7E   ...............~
40: CE 00 00 00 00 00 00 00 01 4D 33 20 36 38 4C 36   .........M3 68L6
50: 34 32 33 46 54 4E 2D 43 43 43 20 4E 46 04 24 41   423FTN-CCC NF.$A
60: 0F 3A A3 00 59 57 42 32 33 30 43 00 00 00 00 00   .:..YWB230C.....
70: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
80: 01 FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
90: 00 01 B6 10 10 38 FF FF FF FF FF 10 14 01 FF FF   .....8..........
A0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
B0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
C0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
D0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
E0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
F0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
SMB Dump from address $52 --> <RAM> (SMBus at $0400) (No error)
00: 80 08 07 0D 0A 02 40 00 04 50 65 00 82 08 00 01   ......@..Pe.....
10: 0E 04 18 01 02 20 C0 60 70 00 00 3C 28 3C 28 40   ..... .`p..<(<(@
20: 60 60 40 40 00 00 00 00 00 37 46 28 28 50 00 00   ``@@.....7F((P..
30: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 10 7E   ...............~
40: CE 00 00 00 00 00 00 00 02 4D 33 20 36 38 4C 36   .........M3 68L6
50: 34 32 33 46 54 4E 2D 43 43 43 20 4E 46 04 19 F6   423FTN-CCC NF...
60: 06 55 84 00 53 41 43 36 43 30 41 00 00 00 00 00   .U..SAC6C0A.....
70: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
80: 00 24 B6 73 80 1B FF FF FF FF FF 04 07 30 FF FF   .$.s.........0..
90: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
A0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
B0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
C0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
D0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
E0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
F0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
SMB Device at address $69 --> (SMBus at $0400) (No error)

*****************************

Retry attempts info for SMBus at $0400
  [ -1]=441
  [  1]=441

*****************************

*****************************

*****************************

Can change fan speeds : NO
Can smoothly change fan speeds : NO
Can stop fans : NO

*****************************

WMI interface is registered : ON
MB manufacturer: ASUSTeK Computer INC.
MB model: Cobra    
MB version: 1.xx
ACPI temp: 0.0
ACPI active trip point: 0.0
ACPI passive trip point: 0.0
ACPI critical trip point: 0.0
WMI quick analysis results -->
EXPLORING : root\CIMV2\Win32_BaseBoard
  -> Object Start
  Caption = Base Board
  CreationClassName = Win32_BaseBoard
  Description = Base Board
  HostingBoard = True
  Manufacturer = ASUSTeK Computer INC.
  Name = Base Board
  PoweredOn = True
  Product = Cobra    
  SerialNumber = X312345678
  Tag = Base Board
  Version = 1.xx
  Method -> IsCompatible(ElementToCheck)
EXPLORING : root\WMI\msacpi_thermalzonetemperature
EXPLORING : root\CIMV2\CIM_AssociatedSensor
EXPLORING : root\CIMV2\CIM_CoolingDevice
EXPLORING : root\CIMV2\CIM_Fan
EXPLORING : root\CIMV2\CIM_HeatPipe
EXPLORING : root\CIMV2\CIM_ManagementController
EXPLORING : root\CIMV2\CIM_NumericSensor
EXPLORING : root\CIMV2\CIM_PackageAlarm
EXPLORING : root\CIMV2\CIM_PackageCooling
EXPLORING : root\CIMV2\CIM_Refrigeration
EXPLORING : root\CIMV2\CIM_Sensor
EXPLORING : root\CIMV2\CIM_Tachometer
EXPLORING : root\CIMV2\CIM_TemperatureSensor
EXPLORING : root\CIMV2\CIM_VoltageSensor
EXPLORING : root\CIMV2\Win32_CurrentProbe
EXPLORING : root\CIMV2\Win32_Fan
EXPLORING : root\CIMV2\Win32_HeatPipe
EXPLORING : root\CIMV2\Win32_Refrigeration
EXPLORING : root\CIMV2\Win32_TemperatureProbe
EXPLORING : root\CIMV2\Win32_VoltageProbe
<-- End of WMI quick analysis results

*****************************

Tray icon size : 16x16
UPTIME : 0 days 09:49:52

*****************************

I/O properly initialized
Linked ISA BUS at $0290
Linked Intel 82801EB ICH5 SMBUS at $0400
Scanning ISA BUS at $0290...
SuperIO Chip=LPC47m192 (PLEASE REPORT)
Sensor's Base Address : $0680
Scanning Intel SMBus at $0400...
SMSC H/M Block (ID=$20) found on SMBus at $2D
Address $32 appears to be WRITE ONLY...
SMART Enabled for drive 0
Found ST340014AS (40.0GB)
ProbeSCSI: before first LogSense
End of detection

*****************************

I/O properly initialized
Linked ISA BUS at $0290
Linked PCI
Starting PCI scan...
FUNC_DIS=$0060
Command Register : $0001
I/O Space Enabled
Host Configuration Register : $01
SMBus Host Enabled
Linked Intel 82801EB ICH5 SMBUS at $0400
HST_CNT=$08
PCI scan done!
Scanning ISA BUS at $0290...
About to check DELL support
PCI scanning is enabled
End of DELL support check
INFO: ISA seems to be unused
Second pass...
SMSC (1) r[$0D]=$00 r[$0E]=$00 r[$20]=$60 r[$21]=$01 r[$07]=$0A 
NEW --> SuperIO chip=SMSC LPC47m192 (PLEASE REPORT) ($002E)
SMSC (2) r[$0D]=$00 r[$0E]=$00 r[$20]=$60 r[$21]=$01 r[$07]=$0A 
ITE r[$20]=$60 r[$21]=$01 r[$22]=$08 r[$07]=$0A 
Checking $0370 for SMSC (2)...
Checking $0370 for SMSC (1)...
Checking $03F0 for SMSC (2)...
Checking $03F0 for SMSC (1)...
Checking $002E for SMSC (1)...
Registers [$002E] : $60 $01 $00 $00
SuperIO Chip=LPC47m192 (PLEASE REPORT)
Accessing SuperIO at $002E ($FF)
 --> LDN0 [$60]=$03F0 [$62]=$0000 [$64]=$0000 (disabled)
 --> LDN1 [$60]=$0000 [$62]=$0000 [$64]=$0000 (disabled)
 --> LDN2 [$60]=$0000 [$62]=$0000 [$64]=$0000 (disabled)
 --> LDN3 [$60]=$0378 [$62]=$0000 [$64]=$0000 (enabled)
 --> LDN4 [$60]=$03F8 [$62]=$0000 [$64]=$0000 (disabled)
 --> LDN5 [$60]=$0000 [$62]=$0000 [$64]=$0000 (disabled)
 --> LDN6 [$60]=$0000 [$62]=$0000 [$64]=$0000 (disabled)
 --> LDN7 [$60]=$0000 [$62]=$0000 [$64]=$0000 (enabled)
 --> LDN8 [$60]=$0000 [$62]=$0000 [$64]=$0000 (disabled)
 --> LDN9 [$60]=$0000 [$62]=$0000 [$64]=$0000 (disabled)
 --> LDNA [$60]=$0680 [$62]=$0000 [$64]=$0000 (disabled)
 --> LDNB [$60]=$0330 [$62]=$0000 [$64]=$0000 (disabled)
 --> Base address is $0680
 --> [$00]=$FF
 --> [$01]=$FF
 --> [$02]=$FF
 --> [$03]=$FF
 --> [$04]=$FF
 --> [$05]=$FF
 --> [$06]=$FF
 --> [$07]=$FF
 --> [$08]=$FF
 --> [$09]=$FF
 --> [$0A]=$FF
 --> [$0B]=$FF
 --> [$0C]=$FF
 --> [$0D]=$FF
 --> [$0E]=$FF
 --> [$0F]=$FF
 --> [$10]=$FF
 --> [$11]=$FF
 --> [$12]=$FF
 --> [$13]=$FF
 --> [$14]=$FF
 --> [$15]=$FF
 --> [$16]=$FF
 --> [$17]=$FF
 --> [$18]=$FF
 --> [$19]=$FF
 --> [$1A]=$FF
 --> [$1B]=$FF
 --> [$1C]=$FF
 --> [$1D]=$FF
 --> [$1E]=$FF
 --> [$1F]=$FF
 --> [$20]=$FF
 --> [$21]=$FF
 --> [$22]=$FF
 --> [$23]=$FF
 --> [$24]=$FF
 --> [$25]=$FF
 --> [$26]=$FF
 --> [$27]=$FF
 --> [$28]=$FF
 --> [$29]=$FF
 --> [$2A]=$FF
 --> [$2B]=$FF
 --> [$2C]=$FF
 --> [$2D]=$FF
 --> [$2E]=$FF
 --> [$2F]=$FF
 --> [$30]=$FF
 --> [$31]=$FF
 --> [$32]=$FF
 --> [$33]=$FF
 --> [$34]=$FF
 --> [$35]=$FF
 --> [$36]=$FF
 --> [$37]=$FF
 --> [$38]=$FF
 --> [$39]=$FF
 --> [$3A]=$FF
 --> [$3B]=$FF
 --> [$3C]=$FF
 --> [$3D]=$FF
 --> [$3E]=$FF
 --> [$3F]=$FF
 --> [$40]=$FF
 --> [$41]=$FF
 --> [$42]=$FF
 --> [$43]=$FF
 --> [$44]=$FF
 --> [$45]=$FF
 --> [$46]=$FF
 --> [$47]=$FF
 --> [$48]=$FF
 --> [$49]=$FF
 --> [$4A]=$FF
 --> [$4B]=$FF
 --> [$4C]=$FF
 --> [$4D]=$FF
 --> [$4E]=$FF
 --> [$4F]=$FF
 --> [$50]=$FF
 --> [$51]=$FF
 --> [$52]=$FF
 --> [$53]=$FF
 --> [$54]=$FF
 --> [$55]=$FF
 --> [$56]=$FF
 --> [$57]=$FF
 --> [$58]=$FF
 --> [$59]=$FF
 --> [$5A]=$FF
 --> [$5B]=$FF
 --> [$5C]=$FF
 --> [$5D]=$FF
 --> [$5E]=$FF
 --> [$5F]=$FF
 --> [$60]=$FF
 --> [$61]=$FF
 --> [$62]=$FF
 --> [$63]=$FF
 --> [$64]=$FF
 --> [$65]=$FF
 --> [$66]=$FF
 --> [$67]=$FF
 --> [$68]=$FF
 --> [$69]=$FF
 --> [$6A]=$FF
 --> [$6B]=$FF
 --> [$6C]=$FF
 --> [$6D]=$FF
 --> [$6E]=$FF
 --> [$6F]=$FF
 --> [$70]=$FF
 --> [$71]=$FF
 --> [$72]=$FF
 --> [$73]=$FF
 --> [$74]=$FF
 --> [$75]=$FF
 --> [$76]=$FF
 --> [$77]=$FF
 --> [$78]=$FF
 --> [$79]=$FF
 --> [$7A]=$FF
 --> [$7B]=$FF
 --> [$7C]=$FF
 --> [$7D]=$FF
 --> [$7E]=$FF
 --> [$7F]=$FF
Sensor's Base Address : $0680
Fan Speed Control and Monitoring is DISABLED
 -> PWMOUT1 clock : Always HIGH ($F)
 -> PWMOUT2 clock : Always HIGH ($F)
 -> FAN1 mult : 1
 -> FAN1 div : 1
 -> FAN2 mult : 1
 -> FAN2 div : 1
 -> Reverse PWM01 logic : OFF
 -> Reverse PWM02 logic : OFF
Scanning Intel SMBus at $0400...
Something is at address $2D
SMSC H/M Block (ID=$20) found on SMBus at $2D
 -> Temperature 1 offset : 0
 -> Temperature 2 offset : 0
 -> Temperature 3 offset : 0
Something is at address $30
Something is at address $32
Address $32 appears to be WRITE ONLY...
Something is at address $44
Something is at address $50
About to probe TOSHIBA SUPPORT...
End of TOSHIBA SUPPORT probing
Version 1.1 04 00000007
SMART Enabled for drive 0
 --> S.M.A.R.T. attributes properly read
 --> S.M.A.R.T. thresholds properly read
Start of DEBUG DATA for drive 0
--> cylinders : 4863
--> tracks per cilinder : 255
--> sectors per track : 63
--> bytes per sector : 512
--> disk size : 40.0
End of DEBUG DATA for drive 0
Found ST340014AS (40.0GB)
Found ST340014AS Firmware revision <8.05> (40.0GB) Serial <5JXFY8B0>
 --> ATA device
 --> Fixed Drive
 --> S.M.A.R.T. Supported (enabled)
 --> Power Management Supported (enabled)
 --> Automatic Acoustic Management Supported (Current:$80  Reccomended:$80)
 --> 48-bit Addressing ($17C8 $04A8 $0000 $0000)
 --> UDMA Mode 0 Supported
 --> UDMA Mode 1 Supported
 --> UDMA Mode 2 Supported
 --> UDMA Mode 3 Supported
 --> UDMA Mode 4 Supported
 --> UDMA Mode 5 Supported
 --> UDMA Mode 6 Supported
 --> UDMA Mode 5 Active
SMART Structure Revision : $000A
ID=$01  NAME=Raw Read Error Rate  VALUE=$54  WORST=$4A  RAW=$00000B4EB591  THRSHLD=$06  FLAGS=$000F
ID=$03  NAME=Spin Up Time  VALUE=$62  WORST=$62  RAW=$000000000000  THRSHLD=$00  FLAGS=$0003
ID=$04  NAME=Start/Stop Count  VALUE=$64  WORST=$64  RAW=$000000000002  THRSHLD=$14  FLAGS=$0032
ID=$05  NAME=Reallocated Sector Count  VALUE=$64  WORST=$64  RAW=$000000000000  THRSHLD=$24  FLAGS=$0033
ID=$07  NAME=Seek Error Rate  VALUE=$4B  WORST=$3C  RAW=$0000024597F6  THRSHLD=$1E  FLAGS=$000F
ID=$09  NAME=Power On Hours Count  VALUE=$64  WORST=$64  RAW=$0000000002D5  THRSHLD=$00  FLAGS=$0032
ID=$0A  NAME=Spin Retry Count  VALUE=$64  WORST=$64  RAW=$000000000000  THRSHLD=$61  FLAGS=$0013
ID=$0C  NAME=Power Cycle Count  VALUE=$64  WORST=$64  RAW=$0000000000B3  THRSHLD=$14  FLAGS=$0032
ID=$C2  NAME=Temperature  VALUE=$27  WORST=$39  RAW=$000000000027  THRSHLD=$00  FLAGS=$0022
Current HD temperature is 39C
ID=$C3  NAME=Hardware ECC Recovered  VALUE=$54  WORST=$4A  RAW=$00000B4EB591  THRSHLD=$00  FLAGS=$001A
ID=$C5  NAME=Current Pending Sector  VALUE=$64  WORST=$64  RAW=$000000000000  THRSHLD=$00  FLAGS=$0012
ID=$C6  NAME=Offline Correctable  VALUE=$64  WORST=$64  RAW=$000000000000  THRSHLD=$00  FLAGS=$0010
ID=$C7  NAME=UltraATA CRC Error Rate  VALUE=$C8  WORST=$C8  RAW=$000000000000  THRSHLD=$00  FLAGS=$003E
ID=$C8  NAME=Write Error Rate  VALUE=$64  WORST=$FD  RAW=$000000000000  THRSHLD=$00  FLAGS=$0000
ID=$CA  NAME=TA Increase Count  VALUE=$64  WORST=$FD  RAW=$000000000000  THRSHLD=$00  FLAGS=$0032
Linked S.M.A.R.T.
 -> Temperature 1 offset : 0
About to probe SCSI...
ProbeSCSI: before first LogSense
End of SCSI probing
About to probe ACPI temperatures...
End of ACPI temperatures probing
End of detection
Reading Cfg Version 2.01
Old sensor properly detected -->
  LPC47M192 on ISA @ $680
PROP PWMOUT1 clock (4) = Always HIGH ($F)
PROP PWMOUT2 clock (5) = Always HIGH ($F)
Old sensor properly detected -->
  SMSC H/M Block on Intel SMBus @ $2D
Old sensor properly detected -->
  HD0 (40.0GB) on SMART @ $0
PWM from LPC47M192@$680(onISA@$290) -->
  Speed01 0 100
  properly added
PWM from LPC47M192@$680(onISA@$290) -->
  Speed02 0 100
  properly added
Temperature from SMSC H/M Block@$2D(onSMBusIntel@$400) -->
  Ambient 40 50 0
  PWM 1 from 0
  PWM 2 from 0
  properly added
Temperature from SMSC H/M Block@$2D(onSMBusIntel@$400) -->
  CPU 40 50 0
  PWM 1 from 0
  PWM 2 from 0
  properly added
Temperature from SMSC H/M Block@$2D(onSMBusIntel@$400) -->
  Mobo 40 50 0
  PWM 1 from 0
  PWM 2 from 0
  properly added
Temperature from ST340014AS5JXFY8B0 -->
  HD0 40 50 0
  PWM 1 from 0
  PWM 2 from 0
  properly added
Fan from LPC47M192@$680(onISA@$290) -->
  Fan01
  properly added
Fan from LPC47M192@$680(onISA@$290) -->
  Fan02
  properly added
Volt from SMSC H/M Block@$2D(onSMBusIntel@$400) -->
  +2.5V
  properly added
Volt from SMSC H/M Block@$2D(onSMBusIntel@$400) -->
  Vcore
  properly added
Volt from SMSC H/M Block@$2D(onSMBusIntel@$400) -->
  +3.3V
  properly added
Volt from SMSC H/M Block@$2D(onSMBusIntel@$400) -->
  +5V
  properly added
Volt from SMSC H/M Block@$2D(onSMBusIntel@$400) -->
  +12V
  properly added
Volt from SMSC H/M Block@$2D(onSMBusIntel@$400) -->
  +3.3V
  properly added
Volt from SMSC H/M Block@$2D(onSMBusIntel@$400) -->
  +1.5V
  properly added
Volt from SMSC H/M Block@$2D(onSMBusIntel@$400) -->
  +1.8V
  properly added
Preparing report...