Sender : 
SpeedFan version : SpeedFan 4.43
Motherboard model : 

***************************** BIOS INFO

BIOS CopyRight : AWARD  - 42302e31Version 3.08Phoenix - AwardBIOS v6.00PGPhoenix - AwardBIOS v6.00PGRev. Version 3.08
BIOS Date : 07/16/03
BIOS Extended Info : 
BIOS Name : AT/AT COMPATIBLE

Windows NT Multiprocessor Free version 5.1.2600 (Windows XP)

2 processor(s)
Intel Corporation Intel(R) Pentium(R) 4 CPU 3.06GHz family 15 model 2 stepping 7 brand 9 3066 MHz
Running at 3066 MHz
I Agree to receive beta versions : ON

***************************** CPUID INFO

CPU Name : Intel(R) Pentium(R) 4 CPU 3.06GHz
 - Identified CPU Name : Intel Pentium 4 Processor 3.06 GHZ
 - Vendor : GenuineIntel
 - Family : 15 (Full : 15 ($0F))
 - Model : 2 (Full : 2 ($02))
 - Stepping : 7
 - L1 Data Cache : 8 KB 4-way
 - L2 Cache : 512 KB 8-way
 - Core Name : Northwood 
 - Die Revision : C1 
 - Socket Type : Socket 478
 - Manufacturing Technology : 130 nm
 - BUS Speed : 533 MHz
 - Hardwired bus speed : 533 MHz
 - L2 Cache Speed : 3.06 GHz
 - sSpec : SL6SM
 - Digital Thermometer : no
 - Thermal Monitor : yes
 - Thermal Monitor 2 : no
 - Thermal Monitor and Software Controlled Clock Supported : yes
 - IA64 : no
 - Enhanced Intel SpeedStep Technology : no
 - Intel Dynamic Acceleration : no
 - Safer Mode Extensions : no
 - EM64T : no
 - Virtual Machine Extensions : no
 - Logical Processors Per Physical Package : 2
 - Cores Per Physical Package : 1
 - CPUs in system : 1
 - TDP : 81.8 W
 - Execute Disable : no
 - Hyper-Threading Technology : yes
 - Engineering sample : no
$00000000 - $00000002 $756E6547 $6C65746E $49656E69 - .... Genu ntel ineI
$80000000 - $80000004 $00000000 $00000000 $00000000 - .... .... .... ....
$00000001 - $00000F27 $00020809 $00004400 $BFEBFBFF - '... .... .D.. ....
$00000002 - $665B5001 $00000000 $00000000 $007B7040 - .P[f .... .... @p{.
$80000001 - $00000000 $00000000 $00000000 $00000000 - .... .... .... ....
$80000002 - $20202020 $20202020 $20202020 $6E492020 -                  In
$80000003 - $286C6574 $50202952 $69746E65 $52286D75 - tel( R) P enti um(R
$80000004 - $20342029 $20555043 $36302E33 $007A4847 - ) 4  CPU  3.06 GHz.
 - DEBUG : MSR0017=$000A000000000000  MSR002A=$0000000000000000  MSR002C=$0000000017110017  MSR00CD=$FFFFFFFFFFFFFFFF  MSR00CE=$FFFFFFFFFFFFFFFF
 -         MSR0194=$FFFFFFFFFFFFFFFF  MSR0198=$FFFFFFFFFFFFFFFF  MSR0199=$FFFFFFFFFFFFFFFF  MSR019A=$0000000000000008  MSR019D=$FFFFFFFFFFFFFFFF
 -         MSR01A0=$0000000000000081  MSR01A2=$FFFFFFFFFFFFFFFF  MSR01AD=$FFFFFFFFFFFFFFFF
 -         FID0=31.5  FID1=31.5  FID2=31.5  FID3=31.5  FID4=31.5  FID5=31.5  FID6=31.5  FID7=31.5
 -         VID0=1.61250  VID1=1.61250  VID2=1.61250  VID3=1.61250  VID4=1.61250  VID5=1.61250  VID6=1.61250  VID7=1.61250
 -         D01=$0000
 -         D02=$0007
 -         D03=$001F
 -         D04=$0001
 -         D05=$0017
 -         D06=$0000
 -         D07=$0000
 -         !!!STRONG CHECK (HARD BUS SPEED) Name='1.80 GHZ' sSPEC='SL6QL' CpuSpeed=1.800 BusSpeed=400 Ratio=18.0 TDP=68.40 ThermSpec=77.0 VMin=1.4750 VMax=1.5250 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!STRONG CHECK (HARD BUS SPEED) Name='2.50 GHZ' sSPEC='SL6P2' CpuSpeed=2.500 BusSpeed=400 Ratio=25.0 TDP=35.00 ThermSpec=100.0 VMin=1.3000 VMax=1.3000 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!STRONG CHECK (HARD BUS SPEED) Name='2.40 GHZ' sSPEC='SL6K5' CpuSpeed=2.400 BusSpeed=400 Ratio=24.0 TDP=35.00 ThermSpec=100.0 VMin=1.3000 VMax=1.3000 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!STRONG CHECK (HARD BUS SPEED) Name='2.40 GHZ' sSPEC='SL6LS' CpuSpeed=2.400 BusSpeed=400 Ratio=24.0 TDP=30.00 ThermSpec=100.0 VMin=1.3000 VMax=1.3000 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!STRONG CHECK (HARD BUS SPEED) Name='2.20 GHZ' sSPEC='SL6J5' CpuSpeed=2.200 BusSpeed=400 Ratio=22.0 TDP=35.00 ThermSpec=100.0 VMin=1.3000 VMax=1.3000 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!STRONG CHECK (HARD BUS SPEED) Name='2.20 GHZ' sSPEC='SL6LR' CpuSpeed=2.200 BusSpeed=400 Ratio=22.0 TDP=30.00 ThermSpec=100.0 VMin=1.3000 VMax=1.3000 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!STRONG CHECK (HARD BUS SPEED) Name='2 GHZ' sSPEC='SL6FK' CpuSpeed=2.000 BusSpeed=400 Ratio=20.0 TDP=32.00 ThermSpec=100.0 VMin=1.3000 VMax=1.3000 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!STRONG CHECK (HARD BUS SPEED) Name='1.90 GHZ' sSPEC='SL6FJ' CpuSpeed=1.900 BusSpeed=400 Ratio=19.0 TDP=32.00 ThermSpec=100.0 VMin=1.3000 VMax=1.3000 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!STRONG CHECK (HARD BUS SPEED) Name='1.80 GHZ' sSPEC='SL6FH' CpuSpeed=1.800 BusSpeed=400 Ratio=18.0 TDP=30.00 ThermSpec=100.0 VMin=1.3000 VMax=1.3000 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!STRONG CHECK (HARD BUS SPEED) Name='1.70 GHZ' sSPEC='SL6FG' CpuSpeed=1.700 BusSpeed=400 Ratio=17.0 TDP=30.00 ThermSpec=100.0 VMin=1.3000 VMax=1.3000 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!STRONG CHECK (HARD BUS SPEED) Name='1.60 GHZ' sSPEC='SL6FF' CpuSpeed=1.600 BusSpeed=400 Ratio=16.0 TDP=30.00 ThermSpec=100.0 VMin=1.3000 VMax=1.3000 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!WEAK CHECK (NAME KEY) Name='3.06 GHZ' sSPEC='SL6GH' CpuSpeed=3.060 BusSpeed=533 Ratio=23.0 TDP=85.00 ThermSpec=73.0 VMin=1.5250 VMax=1.5250 Socket='Micro-FCPGA' Tech='130 nm' Core='prestonia' Revision='C1'
 -         !!!WEAK CHECK (NAME KEY) Name='3.06 GHZ' sSPEC='SL6RR' CpuSpeed=3.060 BusSpeed=533 Ratio=23.0 TDP=85.00 ThermSpec=73.0 VMin=1.5000 VMax=1.5000 Socket='Micro-FCPGA' Tech='130 nm' Core='prestonia' Revision='C1'
 -         !!!STRONG CHECK (HARD BUS SPEED) Name='3 GHZ' sSPEC='SL6X4' CpuSpeed=3.000 BusSpeed=400 Ratio=30.0 TDP=85.00 ThermSpec=73.0 VMin=1.5250 VMax=1.5250 Socket='Micro-FCPGA' Tech='130 nm' Core='prestonia' Revision='C1'
 -         !!!STRONG CHECK (HARD BUS SPEED) Name='3 GHZ' sSPEC='SL6VW' CpuSpeed=3.000 BusSpeed=400 Ratio=30.0 TDP=85.00 ThermSpec=73.0 VMin=1.5250 VMax=1.5250 Socket='Micro-FCPGA' Tech='130 nm' Core='prestonia' Revision='C1'
 -         !!!STRONG CHECK (HARD RATIO) Name='2.80 GHZ' sSPEC='SL6NS' CpuSpeed=2.800 BusSpeed=533 Ratio=21.0 TDP=74.00 ThermSpec=75.0 VMin=1.5000 VMax=1.5000 Socket='Micro-FCPGA' Tech='130 nm' Core='prestonia' Revision='C1'
 -         !!!STRONG CHECK (HARD RATIO) Name='2.80 GHZ' sSPEC='SL6GG' CpuSpeed=2.800 BusSpeed=533 Ratio=21.0 TDP=74.00 ThermSpec=75.0 VMin=1.5000 VMax=1.5000 Socket='Micro-FCPGA' Tech='130 nm' Core='prestonia' Revision='C1'
 -         !!!STRONG CHECK (HARD BUS SPEED) Name='2.80 GHZ' sSPEC='SL6M7' CpuSpeed=2.800 BusSpeed=400 Ratio=28.0 TDP=68.00 ThermSpec=70.0 VMin=1.4800 VMax=1.4800 Socket='Micro-FCPGA' Tech='130 nm' Core='prestonia' Revision='C1'
 -         !!!STRONG CHECK (HARD BUS SPEED) Name='2.80 GHZ' sSPEC='SL6MS' CpuSpeed=2.800 BusSpeed=400 Ratio=28.0 TDP=68.00 ThermSpec=70.0 VMin=1.4750 VMax=1.4750 Socket='Micro-FCPGA' Tech='130 nm' Core='prestonia' Revision='C1'
 -         !!!STRONG CHECK (HARD RATIO) Name='2.66 GHZ' sSPEC='SL6NR' CpuSpeed=2.660 BusSpeed=533 Ratio=20.0 TDP=72.00 ThermSpec=74.0 VMin=1.5000 VMax=1.5000 Socket='Micro-FCPGA' Tech='130 nm' Core='prestonia' Revision='C1'
 -         !!!STRONG CHECK (HARD RATIO) Name='2.66 GHZ' sSPEC='SL6GF' CpuSpeed=2.660 BusSpeed=533 Ratio=20.0 TDP=72.00 ThermSpec=74.0 VMin=1.5000 VMax=1.5000 Socket='Micro-FCPGA' Tech='130 nm' Core='prestonia' Revision='C1'
 -         !!!STRONG CHECK (HARD BUS SPEED) Name='2.60 GHZ' sSPEC='SL6K3' CpuSpeed=2.600 BusSpeed=400 Ratio=26.0 TDP=60.00 ThermSpec=70.0 VMin=1.4750 VMax=1.4750 Socket='Micro-FCPGA' Tech='130 nm' Core='prestonia' Revision='C1'
 -         !!!STRONG CHECK (HARD BUS SPEED) Name='2.60 GHZ' sSPEC='SL6EQ' CpuSpeed=2.600 BusSpeed=400 Ratio=26.0 TDP=60.00 ThermSpec=70.0 VMin=1.4800 VMax=1.4800 Socket='Micro-FCPGA' Tech='130 nm' Core='prestonia' Revision='C1'
 -         !!!STRONG CHECK (HARD BUS SPEED) Name='2.40 GHZ' sSPEC='SL6K2' CpuSpeed=2.400 BusSpeed=400 Ratio=24.0 TDP=65.00 ThermSpec=74.0 VMin=1.4750 VMax=1.4750 Socket='Micro-FCPGA' Tech='130 nm' Core='prestonia' Revision='C1'
 -         !!!STRONG CHECK (HARD BUS SPEED) Name='2.40 GHZ' sSPEC='SL6EP' CpuSpeed=2.400 BusSpeed=400 Ratio=24.0 TDP=65.00 ThermSpec=74.0 VMin=1.5000 VMax=1.5000 Socket='Micro-FCPGA' Tech='130 nm' Core='prestonia' Revision='C1'
 -         !!!STRONG CHECK (HARD RATIO) Name='2.40 GHZ' sSPEC='SL6GD' CpuSpeed=2.400 BusSpeed=533 Ratio=18.0 TDP=65.00 ThermSpec=74.0 VMin=1.4750 VMax=1.4750 Socket='Micro-FCPGA' Tech='130 nm' Core='prestonia' Revision='C1'
 -         !!!STRONG CHECK (HARD RATIO) Name='2.40 GHZ' sSPEC='SL6NQ' CpuSpeed=2.400 BusSpeed=533 Ratio=18.0 TDP=65.00 ThermSpec=74.0 VMin=1.5000 VMax=1.5000 Socket='Micro-FCPGA' Tech='130 nm' Core='prestonia' Revision='C1'
 -         !!!STRONG CHECK (HARD BUS SPEED) Name='2.20 GHZ' sSPEC='SL6JZ' CpuSpeed=2.200 BusSpeed=400 Ratio=22.0 TDP=61.00 ThermSpec=75.0 VMin=1.4750 VMax=1.4750 Socket='Micro-FCPGA' Tech='130 nm' Core='prestonia' Revision='C1'
 -         !!!STRONG CHECK (HARD BUS SPEED) Name='2.20 GHZ' sSPEC='SL6EN' CpuSpeed=2.200 BusSpeed=400 Ratio=22.0 TDP=61.00 ThermSpec=75.0 VMin=1.4750 VMax=1.4750 Socket='Micro-FCPGA' Tech='130 nm' Core='prestonia' Revision='C1'
 -         !!!STRONG CHECK (HARD BUS SPEED) Name='2 GHZ' sSPEC='SL6JY' CpuSpeed=2.000 BusSpeed=400 Ratio=20.0 TDP=58.00 ThermSpec=70.0 VMin=1.4750 VMax=1.4750 Socket='Micro-FCPGA' Tech='130 nm' Core='prestonia' Revision='C1'
 -         !!!STRONG CHECK (HARD BUS SPEED) Name='2 GHZ' sSPEC='SL6EM' CpuSpeed=2.000 BusSpeed=400 Ratio=20.0 TDP=58.00 ThermSpec=70.0 VMin=1.4750 VMax=1.4750 Socket='Micro-FCPGA' Tech='130 nm' Core='prestonia' Revision='C1'
 -         !!!STRONG CHECK (HARD RATIO) Name='2 GHZ' sSPEC='SL6RQ' CpuSpeed=2.000 BusSpeed=533 Ratio=15.0 TDP=58.00 ThermSpec=70.0 VMin=1.5000 VMax=1.5000 Socket='Micro-FCPGA' Tech='130 nm' Core='prestonia' Revision='C1'
 -         !!!STRONG CHECK (HARD RATIO) Name='2 GHZ' sSPEC='SL6NP' CpuSpeed=2.000 BusSpeed=533 Ratio=15.0 TDP=58.00 ThermSpec=70.0 VMin=1.5000 VMax=1.5000 Socket='Micro-FCPGA' Tech='130 nm' Core='prestonia' Revision='C1'
 -         !!!STRONG CHECK (HARD BUS SPEED) Name='1.80 GHZ' sSPEC='SL6EL' CpuSpeed=1.800 BusSpeed=400 Ratio=18.0 TDP=55.80 ThermSpec=69.0 VMin=1.4750 VMax=1.4750 Socket='Micro-FCPGA' Tech='130 nm' Core='prestonia' Revision='C1'
 -         !!!STRONG CHECK (HARD BUS SPEED) Name='1.80 GHZ' sSPEC='SL6JX' CpuSpeed=1.800 BusSpeed=400 Ratio=18.0 TDP=55.00 ThermSpec=69.0 VMin=1.4750 VMax=1.4750 Socket='Micro-FCPGA' Tech='130 nm' Core='prestonia' Revision='C1'
 -         !!!STRONG CHECK (HARD BUS SPEED) Name='1.80 GHZ' sSPEC='SL6E6' CpuSpeed=1.800 BusSpeed=400 Ratio=18.0 TDP=66.10 ThermSpec=77.0 VMin=1.5250 VMax=1.5250 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!STRONG CHECK (HARD BUS SPEED) Name='1.80 GHZ' sSPEC='SL6LA' CpuSpeed=1.800 BusSpeed=400 Ratio=18.0 TDP=66.10 ThermSpec=77.0 VMin=1.5300 VMax=1.5300 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!STRONG CHECK (HARD BUS SPEED) Name='1.80 GHZ' sSPEC='SL6SN' CpuSpeed=1.800 BusSpeed=400 Ratio=18.0 TDP=66.10 ThermSpec=77.0 VMin=1.5250 VMax=1.5250 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!STRONG CHECK (HARD BUS SPEED) Name='1.80 GHZ' sSPEC='SL6S6' CpuSpeed=1.800 BusSpeed=400 Ratio=18.0 TDP=0.00 ThermSpec=0.0 VMin=0.0000 VMax=0.0000 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!STRONG CHECK (HARD RATIO) Name='2.80 GHZ' sSPEC='SL6S4' CpuSpeed=2.800 BusSpeed=533 Ratio=21.0 TDP=68.40 ThermSpec=75.0 VMin=0.0000 VMax=0.0000 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!STRONG CHECK (HARD RATIO) Name='2.80 GHZ' sSPEC='SL6SL' CpuSpeed=2.800 BusSpeed=533 Ratio=21.0 TDP=68.40 ThermSpec=75.0 VMin=0.0000 VMax=0.0000 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!STRONG CHECK (HARD RATIO) Name='2.80 GHZ' sSPEC='SL6K6' CpuSpeed=2.800 BusSpeed=533 Ratio=21.0 TDP=68.40 ThermSpec=73.0 VMin=1.5250 VMax=1.5250 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!STRONG CHECK (HARD RATIO) Name='2.80 GHZ' sSPEC='SL6HL' CpuSpeed=2.800 BusSpeed=533 Ratio=21.0 TDP=68.40 ThermSpec=73.0 VMin=1.5250 VMax=1.5250 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!STRONG CHECK (HARD RATIO) Name='2.66 GHZ' sSPEC='SL6SK' CpuSpeed=2.660 BusSpeed=533 Ratio=20.0 TDP=66.10 ThermSpec=74.0 VMin=0.0000 VMax=0.0000 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!STRONG CHECK (HARD RATIO) Name='2.66 GHZ' sSPEC='SL6EH' CpuSpeed=2.660 BusSpeed=533 Ratio=20.0 TDP=66.10 ThermSpec=73.0 VMin=1.5250 VMax=1.5250 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!STRONG CHECK (HARD RATIO) Name='2.66 GHZ' sSPEC='SL6S3' CpuSpeed=2.660 BusSpeed=533 Ratio=20.0 TDP=66.10 ThermSpec=74.0 VMin=1.5250 VMax=1.5250 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!STRONG CHECK (HARD RATIO) Name='2.66 GHZ' sSPEC='SL6DX' CpuSpeed=2.660 BusSpeed=533 Ratio=20.0 TDP=66.10 ThermSpec=73.0 VMin=1.5250 VMax=1.5250 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!STRONG CHECK (HARD BUS SPEED) Name='2.60 GHZ' sSPEC='SL6SB' CpuSpeed=2.600 BusSpeed=400 Ratio=26.0 TDP=62.60 ThermSpec=72.0 VMin=0.0000 VMax=0.0000 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!STRONG CHECK (HARD BUS SPEED) Name='2.60 GHZ' sSPEC='SL6GU' CpuSpeed=2.600 BusSpeed=400 Ratio=26.0 TDP=62.60 ThermSpec=72.0 VMin=1.5000 VMax=1.5000 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!STRONG CHECK (HARD BUS SPEED) Name='2.60 GHZ' sSPEC='SL6HB' CpuSpeed=2.600 BusSpeed=400 Ratio=26.0 TDP=62.60 ThermSpec=72.0 VMin=1.5000 VMax=1.5000 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!STRONG CHECK (HARD RATIO) Name='2.53 GHZ' sSPEC='SL6SJ' CpuSpeed=2.530 BusSpeed=533 Ratio=19.0 TDP=61.50 ThermSpec=72.0 VMin=0.0000 VMax=0.0000 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!STRONG CHECK (HARD RATIO) Name='2.53 GHZ' sSPEC='SL6S2' CpuSpeed=2.530 BusSpeed=533 Ratio=19.0 TDP=61.50 ThermSpec=72.0 VMin=0.0000 VMax=0.0000 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!STRONG CHECK (HARD RATIO) Name='2.53 GHZ' sSPEC='SL6DW' CpuSpeed=2.530 BusSpeed=533 Ratio=19.0 TDP=61.50 ThermSpec=72.0 VMin=1.5250 VMax=1.5250 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!STRONG CHECK (HARD RATIO) Name='2.53 GHZ' sSPEC='SL6EG' CpuSpeed=2.530 BusSpeed=533 Ratio=19.0 TDP=61.50 ThermSpec=72.0 VMin=1.5250 VMax=1.5250 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!STRONG CHECK (HARD BUS SPEED) Name='2.50 GHZ' sSPEC='SL6SA' CpuSpeed=2.500 BusSpeed=400 Ratio=25.0 TDP=61.00 ThermSpec=72.0 VMin=0.0000 VMax=0.0000 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!STRONG CHECK (HARD BUS SPEED) Name='2.50 GHZ' sSPEC='SL6EB' CpuSpeed=2.500 BusSpeed=400 Ratio=25.0 TDP=61.00 ThermSpec=72.0 VMin=1.5250 VMax=1.5250 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!STRONG CHECK (HARD BUS SPEED) Name='2.50 GHZ' sSPEC='SL6GT' CpuSpeed=2.500 BusSpeed=400 Ratio=25.0 TDP=61.00 ThermSpec=72.0 VMin=1.5250 VMax=1.5250 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!STRONG CHECK (HARD RATIO) Name='2.40 GHZ' sSPEC='SL6SH' CpuSpeed=2.400 BusSpeed=533 Ratio=18.0 TDP=59.80 ThermSpec=71.0 VMin=0.0000 VMax=0.0000 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!STRONG CHECK (HARD BUS SPEED) Name='2.40 GHZ' sSPEC='SL6S9' CpuSpeed=2.400 BusSpeed=400 Ratio=24.0 TDP=59.80 ThermSpec=71.0 VMin=0.0000 VMax=0.0000 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!STRONG CHECK (HARD RATIO) Name='2.40 GHZ' sSPEC='SL6EF' CpuSpeed=2.400 BusSpeed=533 Ratio=18.0 TDP=59.80 ThermSpec=71.0 VMin=1.5250 VMax=1.5250 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!STRONG CHECK (HARD BUS SPEED) Name='2.40 GHZ' sSPEC='SL6GS' CpuSpeed=2.400 BusSpeed=400 Ratio=24.0 TDP=59.80 ThermSpec=71.0 VMin=1.5250 VMax=1.5250 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!STRONG CHECK (HARD BUS SPEED) Name='2.40 GHZ' sSPEC='SL6SR' CpuSpeed=2.400 BusSpeed=400 Ratio=24.0 TDP=59.80 ThermSpec=71.0 VMin=1.5250 VMax=1.5250 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!STRONG CHECK (HARD BUS SPEED) Name='2.40 GHZ' sSPEC='SL6E9' CpuSpeed=2.400 BusSpeed=400 Ratio=24.0 TDP=59.80 ThermSpec=71.0 VMin=1.5250 VMax=1.5250 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!STRONG CHECK (HARD RATIO) Name='2.40 GHZ' sSPEC='SL6DV' CpuSpeed=2.400 BusSpeed=533 Ratio=18.0 TDP=59.80 ThermSpec=71.0 VMin=1.5250 VMax=1.5250 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!STRONG CHECK (HARD RATIO) Name='2.40 GHZ' sSPEC='SL6RZ' CpuSpeed=2.400 BusSpeed=533 Ratio=18.0 TDP=59.80 ThermSpec=71.0 VMin=1.5300 VMax=1.5300 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!STRONG CHECK (HARD RATIO) Name='2.26 GHZ' sSPEC='SL6RY' CpuSpeed=2.260 BusSpeed=533 Ratio=17.0 TDP=58.00 ThermSpec=70.0 VMin=1.5300 VMax=1.5300 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!STRONG CHECK (HARD RATIO) Name='2.26 GHZ' sSPEC='SL6DU' CpuSpeed=2.260 BusSpeed=533 Ratio=17.0 TDP=58.00 ThermSpec=70.0 VMin=1.5000 VMax=1.5000 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!STRONG CHECK (HARD RATIO) Name='2.26 GHZ' sSPEC='SL6EE' CpuSpeed=2.260 BusSpeed=533 Ratio=17.0 TDP=58.00 ThermSpec=70.0 VMin=1.5000 VMax=1.5000 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!STRONG CHECK (HARD BUS SPEED) Name='2.20 GHZ' sSPEC='SL6S8' CpuSpeed=2.200 BusSpeed=400 Ratio=22.0 TDP=57.10 ThermSpec=70.0 VMin=0.0000 VMax=0.0000 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!STRONG CHECK (HARD BUS SPEED) Name='2.20 GHZ' sSPEC='SL6E8' CpuSpeed=2.200 BusSpeed=400 Ratio=22.0 TDP=57.10 ThermSpec=70.0 VMin=1.5250 VMax=1.5250 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!STRONG CHECK (HARD BUS SPEED) Name='2.20 GHZ' sSPEC='SL6GR' CpuSpeed=2.200 BusSpeed=400 Ratio=22.0 TDP=57.10 ThermSpec=70.0 VMin=1.5250 VMax=1.5250 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!STRONG CHECK (HARD BUS SPEED) Name='2 GHZ' sSPEC='SL6S7' CpuSpeed=2.000 BusSpeed=400 Ratio=20.0 TDP=54.30 ThermSpec=69.0 VMin=0.0000 VMax=0.0000 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!STRONG CHECK (HARD BUS SPEED) Name='2 GHZ' sSPEC='SL6SP' CpuSpeed=2.000 BusSpeed=400 Ratio=20.0 TDP=75.30 ThermSpec=76.0 VMin=1.5250 VMax=1.5250 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!STRONG CHECK (HARD BUS SPEED) Name='2 GHZ' sSPEC='SL6GQ' CpuSpeed=2.000 BusSpeed=400 Ratio=20.0 TDP=54.30 ThermSpec=69.0 VMin=1.5250 VMax=1.5250 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!STRONG CHECK (HARD BUS SPEED) Name='2 GHZ' sSPEC='SL6E7' CpuSpeed=2.000 BusSpeed=400 Ratio=20.0 TDP=54.30 ThermSpec=69.0 VMin=1.5250 VMax=1.5250 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!Found more than one corresponding Intel revision
 -         !!!  Name='3.06 GHZ' sSPEC='SL6SM' CpuSpeed=3.060 BusSpeed=533 Ratio=23.0 TDP=81.80 ThermSpec=69.0 VMin=0.0000 VMax=0.0000 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!  Name='3.06 GHZ' sSPEC='SL6S5' CpuSpeed=3.060 BusSpeed=533 Ratio=23.0 TDP=81.80 ThermSpec=69.0 VMin=0.0000 VMax=0.0000 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!  Name='3.06 GHZ' sSPEC='SL6JJ' CpuSpeed=3.060 BusSpeed=533 Ratio=23.0 TDP=0.00 ThermSpec=69.0 VMin=1.5250 VMax=1.5250 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'
 -         !!!  Name='3.06 GHZ' sSPEC='SL6K7' CpuSpeed=3.060 BusSpeed=533 Ratio=23.0 TDP=0.00 ThermSpec=69.0 VMin=1.5500 VMax=1.5500 Socket='Socket 478' Tech='130 nm' Core='northwood' Revision='C1'

***************************** SENSORS' READINGS

IT8712F on ISA at $290 Temp1 : 56.0   min=52.0   max=58.0   mean=55.5
IT8712F on ISA at $290 Temp2 : 39.0   min=39.0   max=39.0   mean=39.0
IT8712F on ISA at $290 Temp3 : -55.0   min=-55.0   max=-55.0   mean=-55.0
IT8712F on ISA at $290 Fan1 : 2033   min=1918   max=4441   mean=2028
IT8712F on ISA at $290 Fan2 : 0   min=0   max=2058   mean=0
IT8712F on ISA at $290 Fan3 : 0   min=0   max=0   mean=0
IT8712F on ISA at $290 Pwm1 : 6%   min=6%   max=100%   mean=67%
IT8712F on ISA at $290 Pwm2 : 100%   min=0%   max=100%   mean=67%
IT8712F on ISA at $290 Pwm3 : 100%   min=0%   max=100%   mean=67%
IT8712F on ISA at $290 Vcore1 : 1.49   min=1.47   max=1.50   mean=1.49
IT8712F on ISA at $290 Vcore2 : 1.82   min=1.82   max=1.82   mean=1.82
IT8712F on ISA at $290 +3.3V : 3.22   min=3.18   max=3.25   mean=3.22
IT8712F on ISA at $290 +5V : 5.13   min=5.13   max=5.16   mean=5.14
IT8712F on ISA at $290 +12V : 12.03   min=11.97   max=12.10   mean=12.06
IT8712F on ISA at $290 -12V : 0.48   min=0.48   max=0.48   mean=0.48
IT8712F on ISA at $290 -5V : -5.81   min=-5.86   max=-5.66   mean=-5.73
IT8712F on ISA at $290 +5V : 4.81   min=4.73   max=4.81   mean=4.79
IT8712F on ISA at $290 Vbat : 3.20   min=3.20   max=3.20   mean=3.20
[$13]=$37  [$14]=$80  [$15]=$08  [$16]=$7F
[$17]=$7F  [$20]=$5D  [$21]=$72  [$22]=$C9
[$23]=$BF  [$24]=$BC  [$25]=$D4  [$26]=$3B
[$27]=$B3  [$28]=$C8
HD1 (41.1GB) on AdvSMART at $0 HD1 : 48.0   min=48.0   max=53.0   mean=49.6
Maxtor 2F040L0 (drive 1) : fitness=97%   performance=99%
HD0 (80.0GB) on AdvSMART at $1 HD0 : 43.0   min=43.0   max=43.0   mean=43.0
ST380013A (drive 0) : fitness=97%   performance=97%
ACPI on ISA at $0 Temp1 : 40.0   min=40.0   max=40.0   mean=40.0

***************************** SENSORS' ASSOCIATIONS AND GENERAL CONFIG OPTIONS

Temp1 --> active=ON  chip=0  index=1 wanted=40  warning=50  offset=0  InTray=ON Used pwms=1 2 3 
Temp2 --> active=ON  chip=0  index=2 wanted=40  warning=50  offset=0  InTray=OFF Used pwms=1 2 3 
Temp3 --> active=ON  chip=0  index=3 wanted=40  warning=50  offset=0  InTray=OFF Used pwms=1 2 3 
HD1 --> active=ON  chip=1  index=1 wanted=40  warning=50  offset=0  InTray=OFF Used pwms=1 2 3 
HD0 --> active=ON  chip=2  index=1 wanted=40  warning=50  offset=0  InTray=OFF Used pwms=1 2 3 
Temp1 --> active=ON  chip=3  index=1 wanted=40  warning=50  offset=0  InTray=OFF Used pwms=1 2 3 
Fan1 --> active=ON  chip=0  index=1
Fan2 --> active=ON  chip=0  index=2
Fan3 --> active=ON  chip=0  index=3
Speed01 --> active=ON  chip=0  index=1  min=100  max=100  variate=ON
Speed02 --> active=ON  chip=0  index=2  min=100  max=100  variate=ON
Speed03 --> active=ON  chip=0  index=3  min=100  max=100  variate=ON
Vcore1 --> active=ON  chip=0  index=1
Vcore2 --> active=ON  chip=0  index=2
+3.3V --> active=ON  chip=0  index=3
+5V --> active=ON  chip=0  index=4
+12V --> active=ON  chip=0  index=5
-12V --> active=ON  chip=0  index=6
-5V --> active=ON  chip=0  index=7
+5V --> active=ON  chip=0  index=8
Vbat --> active=ON  chip=0  index=9
Set Fans to 100% on exit : OFF
Debug Mode : ON
Use ISA : ON
Use SMB : ON
Scan PCI : ON
Scan SMB : ON
Slow SMB detection : OFF
Detect SuperIO : ON
ASUS Card Detect : ON
DELL Support : OFF
Summary Log Scan : OFF
Command line : "C:\Program Files\SpeedFan\speedfan.exe" 
Delta Fan Speed : 10

***************************** CHIPSET SMBUS

Chipset : SiS651
SMBus Base Address : $1040
SMBus Revision : 00
SMBus I/O Enabled : ON

***************************** PCI SCAN

Bus : 00 Device: 00 Function : 00 --> 06511039 Vendor : 1039 Device : 0651 (rev 02) - Silicon Integrated Systems SiS651 Host-to-PCI Bridge
00: 1039 0651 0007 2210 0002 0600 2000 0080 0000 E000 0000 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 1019 1814 0000 0000 00C0 0000 0000 0000 0000 0000
40: 0000 0000 0000 0000 0000 0000 0000 0000 09FE 8B70 0303 0DB3 2542 50C8 D512 0022
60: 4F6F 6D6D 0003 809B 1001 00E0 0248 0000 9F3F 0030 0002 0060 0000 0000 0082 0011
80: 2622 0330 0085 2B80 0C20 0100 0000 6004 0000 0000 0040 0100 1600 1074 0000 1000
A0: E5C2 C233 0303 7701 5000 C242 0942 0600 0000 1000 0080 4F00 7F05 3330 0C00 0000
C0: 0002 0020 0207 1F00 0304 0000 0000 0000 0222 C233 FF49 01FF 6666 00AA 8000 A1AA
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000

Bus : 00 Device: 01 Function : 00 --> 00011039 Vendor : 1039 Device : 0001 (rev 00) - Silicon Integrated Systems SiS 630/730 Virtual PCI-to-PCI bridge (AGP)
00: 1039 0001 0107 0000 0000 0604 4000 0001 0000 0000 0000 0000 0100 2001 D0D0 2000
20: C000 DFF0 FFF0 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 000E
40: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
60: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000

Bus : 00 Device: 02 Function : 00 --> 00081039 Vendor : 1039 Device : 0008 (rev 14) - Silicon Integrated Systems SiS 85C503 PCI System I/O (PSIO)
00: 1039 0008 000F 0200 0014 0601 0000 0080 0000 0000 0000 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
40: 8590 8A83 448B DD3D 1010 0000 3011 0104 3811 0102 0B20 0B20 0000 0012 0A97 00B6
60: 8A85 898B C1FF 120C 8009 4600 00F7 1402 0000 FFFF 1000 3C00 0020 8020 00F6 0000
80: 0000 0000 0000 0000 0000 0000 0000 0000 00FF 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0040 8000 007C 0004 7FF3 0000 0000 0000 000A 0000 0000 0000 0000 0000 0000 0000

Bus : 00 Device: 02 Function : 03 --> 70071039 Vendor : 1039 Device : 7007 (rev 00) - <Unknown device>
00: 1039 7007 0006 0210 1000 0C00 2000 0000 0000 E500 0000 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 1019 1814 0000 0000 0064 0000 0000 0000 0211 0C04
40: 003E 0000 0011 0001 0002 0404 0000 0008 0000 0010 0000 0000 00FF 8888 0400 0000
60: 0000 0000 0001 FE42 8000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000

Bus : 00 Device: 02 Function : 05 --> 55131039 Vendor : 1039 Device : 5513 (rev 00) - Silicon Integrated Systems SiS5513 PCI IDE Controller
00: 1039 5513 0005 0210 8A00 0101 8000 0000 01F1 0000 03F5 0000 0171 0000 0375 0000
20: 4001 0000 0000 0000 0000 0000 1019 1814 0000 0000 0058 0000 0000 0000 0100 0000
40: 0000 0000 0000 0000 0020 0006 0000 0000 07FA 87FB 96AA D0D5 0001 8402 0000 0000
60: AAFB AAFB 0000 0000 0000 0000 0000 0000 2116 0406 2116 0406 2356 0406 6000 1E1C
80: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000

Bus : 00 Device: 02 Function : 07 --> 70121039 Vendor : 1039 Device : 7012 (rev A0) - Silicon Integrated Systems SiS7012 PCI Audio Accelerator
00: 1039 7012 0005 0290 00A0 0401 2000 0000 E001 0000 E401 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 1019 1814 0000 0000 0048 0000 0000 0000 030A 0B34
40: 0004 0000 0000 0000 0001 C642 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
60: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0002 0000 0000 0000 0000 0000 0000 0000

Bus : 00 Device: 03 Function : 00 --> 70011039 Vendor : 1039 Device : 7001 (rev 0F) - Silicon Integrated Systems SiS5571 USB Host Controller
00: 1039 7001 0007 8280 100F 0C03 2008 0080 1000 E500 0000 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 1019 1814 0000 0000 0000 0000 0000 0000 0114 5000
40: 0000 0000 AC5C 0001 027F 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
60: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0001 C9C2
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000

Bus : 00 Device: 03 Function : 03 --> 70021039 Vendor : 1039 Device : 7002 (rev 00) - Silicon Integrated Systems SiS7002 USB 2.0 Enhanced Host Controller
00: 1039 7002 0006 0290 2000 0C03 2008 0000 4000 E500 0000 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 1019 1814 0000 0000 0050 0000 0000 0000 0417 5000
40: 0000 0800 0000 0000 0000 0000 0000 0000 0001 C9C2 0000 0000 000A 2100 0000 0000
60: 2020 007F 0000 0000 0000 0000 0000 0000 0001 0000 0000 C000 0000 0000 0000 0000
80: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000

Bus : 00 Device: 10 Function : 00 --> 212017FE Vendor : 17FE Device : 2120 (rev 00) - <Unknown device>
00: 17FE 2120 0006 0290 0000 0200 2000 0000 5000 E500 0000 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0401 0000 1737 0020 0000 0000 0040 0000 0000 0000 0112 2020
40: 0001 0002 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
60: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000

Bus : 00 Device: 13 Function : 00 --> 813910EC Vendor : 10EC Device : 8139 (rev 10) - Realtek Semiconductor RTL8139 10/100 Mbps Fast Ethernet NIC
00: 10EC 8139 0005 0290 0010 0200 8000 0000 E801 0000 6000 E500 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 1019 1814 0000 0000 0050 0000 0000 0000 0113 4020
40: 0000 0000 0000 0000 0000 0000 0000 0000 0001 F7C2 0000 0000 0000 0000 0000 0000
60: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000

Bus : 01 Device: 00 Function : 00 --> 71C71002 Vendor : 1002 Device : 71C7 (rev 9E) - <Unknown device>
00: 1002 71C7 0007 02B0 009E 0300 2008 0080 000C C000 0000 0000 0004 D100 0000 0000
20: D001 0000 0000 0000 0000 0000 18BC 3030 0000 0000 0050 0000 0000 0000 0105 0008
40: 0000 0000 0000 0000 0000 0000 18BC 3030 5801 0602 0000 0000 8002 0020 0217 4F00
60: 0304 1F00 0D01 0000 0000 1101 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0005 0080 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000

Bus : 01 Device: 00 Function : 01 --> 71E71002 Vendor : 1002 Device : 71E7 (rev 9E) - <Unknown device>
00: 1002 71E7 0000 02B0 009E 0380 2008 0000 0004 D101 0000 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 18BC 3031 0000 0000 0050 0000 0000 0000 00FF 0008
40: 0000 0000 0000 0000 0000 0000 0000 0000 0001 0602 0000 0000 0002 0020 0217 4F00
60: 0200 0000 0D01 0000 0000 1101 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000

***************************** ISA SCAN

ISA Dump from address $290 --> <IT8712F> (ISA at $0290) (No error)
00: 13 00 FF 00 FF FF 00 00 00 00 00 5B 00 53 FF FF   ...........[.S..
10: FF FF FF 37 80 08 7F 7F 00 00 00 00 00 00 00 00   ...7............
20: 5D 72 C9 BF BC D4 3B B3 C8 38 27 C9 00 00 00 00   ]r....;..8'.....
30: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
40: 3C 00 4B 7F 4B 7F 00 00 2D 00 00 00 00 00 00 00   <.K.K...-.......
50: FF 31 7F 7F 7F 00 00 00 90 63 02 00 80 00 00 00   .1.......c......
60: 7F 7F 7F 7F 7F 00 00 00 7F 7F 7F 7F 7F 00 00 00   ................
70: 7F 7F 7F 7F 7F 00 00 00 00 00 00 00 00 00 00 00   ................
80: 13 00 00 00 FF FF 00 00 00 00 00 5B 00 53 FF FF   ...........[.S..
90: FF FF FF 37 80 08 7F 7F 00 00 00 00 00 00 00 00   ...7............
A0: 5D 72 C9 BF BC D4 3B B3 C8 38 27 C9 00 00 00 00   ]r....;..8'.....
B0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
C0: 3C 00 4B 7F 4B 7F 00 00 2D 00 00 00 00 00 00 00   <.K.K...-.......
D0: FF 31 7F 7F 7F 00 00 00 90 63 02 00 80 00 00 00   .1.......c......
E0: 7F 7F 7F 7F 7F 00 00 00 7F 7F 7F 7F 7F 00 00 00   ................
F0: 7F 7F 7F 7F 7F 00 00 00 00 00 00 00 00 00 00 00   ................

***************************** SMBUS SCAN

SMB Dump from address $10 --> <Unknown> (SMBus at $1040) (No error)
 --> all bytes have the same value ($00)
SMB Dump from address $30 --> <Unknown> (SMBus at $1040) (No error)
 --> all bytes have the same value ($FF)
SMB Dump from address $31 --> <Unknown> (SMBus at $1040) (No error)
 --> all bytes have the same value ($FF)
SMB Dump from address $50 --> <RAM> (SMBus at $1040) (No error)
00: 80 08 07 0D 0B 02 40 00 04 60 70 00 82 08 00 01   ......@..`p.....
10: 0E 04 0C 01 02 20 C0 75 70 00 00 48 30 48 2A 80   ..... .up..H0H*.
20: 80 80 45 45 00 00 00 00 00 3C 48 30 2D 55 00 01   ..EE.....<H0-U..
30: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 10 69   ...............i
40: 2C 00 00 00 00 00 00 00 08 31 36 56 44 44 54 31   ,........16VDDT1
50: 32 38 36 34 41 59 33 33 35 44 33 03 00 07 49 DA   2864AY335D3...I.
60: 1C FA 5E 00 00 00 00 00 00 00 00 00 00 00 00 00   ..^.............
70: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
80: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
90: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
A0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
B0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
C0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
D0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
E0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
F0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
SMB Dump from address $51 --> <RAM> (SMBus at $1040) (No error)
00: 80 08 07 0D 0B 01 40 00 04 60 70 00 82 08 00 01   ......@..`p.....
10: 0E 04 0C 01 02 20 C0 75 70 00 00 48 30 48 2A 80   ..... .up..H0H*.
20: 80 80 45 45 00 00 00 00 00 3C 48 30 2D 55 00 11   ..EE.....<H0-U..
30: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 10 78   ...............x
40: 2C FF FF FF FF FF FF FF 09 38 56 44 44 54 36 34   ,........8VDDT64
50: 36 34 41 47 2D 33 33 35 44 42 20 0B 00 04 2A C5   64AG-335DB ...*.
60: 06 37 A2 00 00 00 00 00 00 00 00 00 00 00 00 00   .7..............
70: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
80: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
90: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
A0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
B0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
C0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
D0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
E0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
F0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
SMB Device at address $69 --> (SMBus at $1040) (No error)
SMB Device at address $6A --> (SMBus at $1040) (No error)

***************************** SMBUS RETRIES

Retry attempts info for SMBus at $1040
  [ -1]=430
  [  1]=430

***************************** SMBUS PAUSES

Pause stats for SMBusSiSx30@$1040: min=49999 max=49999 avg=49999(5691) touts=0 count=5691

***************************** DIMM INFO

***************************** SMBUS DEVICE SCAN RESULTS

***************************** FAN SPEED CONTROL

Can change fan speeds : DON'T KNOW
Can smoothly change fan speeds : DON'T KNOW
Can stop fans : DON'T KNOW

***************************** WMI SCAN

WMI interface is registered : ON
MB manufacturer: Hewlett-Packard
MB model: HP System Board
MB version: HP P/N
ACPI temp: 40.0
ACPI active trip point: 0.0
ACPI passive trip point: -273.2
ACPI critical trip point: 75.0
WMI quick analysis results -->
EXPLORING : root\CIMV2\Win32_BaseBoard
  -> Object Start
  Caption = Base Board
  CreationClassName = Win32_BaseBoard
  Description = Base Board
  HostingBoard = True
  Manufacturer = Hewlett-Packard
  Name = Base Board
  PoweredOn = True
  Product = HP System Board
  SerialNumber =  
  Tag = Base Board
  Version = HP P/N
  Method -> IsCompatible(ElementToCheck)
EXPLORING : root\WMI\msacpi_thermalzonetemperature
  -> Object Start
  Active = True
  ActiveTripPoint =  0 0 0 0 0 0 0 0 0 (0.0C)
  ActiveTripPointCount = 0
  CriticalTripPoint = 3482 (75.0C)
  CurrentTemperature = 3132 (40.0C)
  InstanceName = ACPI\ThermalZone\THRM_0
  PassiveTripPoint = 0 (-273.2C)
  Reserved = 0
  SamplingPeriod = 0
  ThermalConstant1 = 0
  ThermalConstant2 = 0
  ThermalStamp = 247
EXPLORING : root\CIMV2\CIM_AssociatedSensor
EXPLORING : root\CIMV2\CIM_CoolingDevice
EXPLORING : root\CIMV2\CIM_Fan
EXPLORING : root\CIMV2\CIM_HeatPipe
EXPLORING : root\CIMV2\CIM_ManagementController
EXPLORING : root\CIMV2\CIM_NumericSensor
EXPLORING : root\CIMV2\CIM_PackageAlarm
EXPLORING : root\CIMV2\CIM_PackageCooling
EXPLORING : root\CIMV2\CIM_Refrigeration
EXPLORING : root\CIMV2\CIM_Sensor
EXPLORING : root\CIMV2\CIM_Tachometer
EXPLORING : root\CIMV2\CIM_TemperatureSensor
EXPLORING : root\CIMV2\CIM_VoltageSensor
EXPLORING : root\CIMV2\Win32_CurrentProbe
EXPLORING : root\CIMV2\Win32_Fan
EXPLORING : root\CIMV2\Win32_HeatPipe
EXPLORING : root\CIMV2\Win32_Refrigeration
EXPLORING : root\CIMV2\Win32_TemperatureProbe
EXPLORING : root\CIMV2\Win32_VoltageProbe
EXPLORING : SMBIOS
  -> Object Start
Structure 144 - 0026 - fixed len is 12 bytes -> Unknown (144)
  -> FF FF FF FF FF FF 00 01
  -> <SiS630E-MAC>
<-- End of WMI quick analysis results

***************************** ACPI TABLES SCAN

Found ACPI TABLE=DSDT (14912 bytes) (5487 zip)
504B0304140000000800D796B83EA481BBD90B150000403A00000100000074D4
3B4D73DB4696DD0044414DD28264FA338EA355E299C4D949088052ECD44EAD48
801F8805914B5296B3541529CA5294CB06E5B8122B2ED7C84AADED99E49058CE
1EB7A8946ACF73484DCDC155E35FB0951FB0875CB62AA71DDFE2C356B4EF7503
04488AB69CCCEED688E5C6FBECF7FABDEE876E00B66B767DEE6D42A8915DCA56
EDA9EC52D5CE5A15876884B8B542FD08B0B453CBCD4AB5D9F87462F90D04ACCA
629AF0BF03383AE51C75B9594B372799C288F82141E7042A7E48303941163F24
6438C1FF2161861346C4AFB1B56CE77345CAB6186DDC4E08C4CE1575153895F4
6C93C6639A6071AC32DB6C0A960E2CDA650156D139AB52CD5CA0F112E7C43952
C95C103AD5CC451A77021DC42A998B9C55AF662B345ED198842CC42468D25A63
2B7FA5EE9244FAC938615AE3F66B884AD5B2AB6B55B7064DD935103210321132
B5AC9B77A7B839234DE3537E9F88491523DDD404CBA0F1E9906500CBF0592668
A5BB2C13B4CC402B03ACB9D0FF34F89F0E86061DE64296012CC367CD02ABDDED
10B0CAACB065152B651A7F5B6372E3766944A0C54A3A8D8D8E8D818D894D069B
196C66B1790B9B0BD85CC4268B4D0E1B0B1B1B9B3C3605AA9D58266AC5B10A8C
A4124D00A8B781A85AAE15AEC09481CB3CA3A9EC48AD5EB5A40EBBBF7377E3EE
FB7B8C5CBBBBC1684BCD2D16D21312BFEA70F53690E0BD8FE8D7A75B1FB53AC7
EEEF7C7A0F892DC2AF7A8BEC913DDAD8AAD62D97320FC7AD71D8729D05D572ED
ACDAB8338908C29494466BA5C53A84CA59289449620E530D617C05517A29673B
14B49768A56614A8532DCC4BB653CBD31A2881915C3E5FA16C854F360ED7F41C
86DD2A2FD4299B634AE3F6690E5B0BF5B40A8D8E8DA15AF5EABC9AB262B5CAA5
2AF550A9E5B13F20D5638B28E131995F36DA5FBFF5A0CDC82D946132B65E7CBF
B9FAF5E88355463E5ABDC9E9FFEDD38F74E91FB5BD161253B6020BBA5EA31EDB
C715D219D981B876E2D0CA9009581AB7703AB0396CA1877D9CA3FC0AB3EED606
7B8C8B31553AB6DC5CCA5EA277A028D4FFB1592F555DB6D52928D08BD219DFE1
49241EBB82FD05B8E4B1A5280E1E5C0EF12B609EBDCBF1B272FF2BF0E6CEF29B
72B3966B562C27BD58CBA519E9A3E8039434A303323850F4B98791ADF62B67AB
06233771D0F13FEDE3A556C82EB07D0F5754CB6BE1A573CC771C478D7A4BD51C
93762F76A6308437319A4C697526775AD87754E47827B58393A6970C9210AE1E
92761A0AA2D34C8D35DD5A917AAD1640B55A1D21CD7A69B959ACE453479BF3E9
34E9893CA7E98334DD0C2C1616EB35A09D03B9FC60D4A41E27B8546630DA0748
BDD52F651C2435DB2F65F64B9D04A9991EA9AC5B05BF52E78171811C2677DC52
A187014BF4525F2AB894DD2FE5F64B2DC4402CD72582147A1CD1B11C7D80620C
50CC014A668032E30FDFEA71CACD5A6052BBA7CACB486A6C9F42CFD466C9B113
D96F13099C17F52CD96371606172BBAC2351D6C259B8F934BB3C9A725F6C5AD5
1A116534C7D8BFDE1923703B4FC0FD5C26021E27648E08782E026F45E0471198
FF511FDEDF0F61FC633EAC714CC0FF0532920FFF18917FF423CA09F83B0E6F92
DFA19F6C2E6BB9AE00E1969AD50598AAD66A3E7806A88600A780EA83AF02D514
E0DF02D5073340CD08F002507D70036FE4D7F1569D40CB887566EEEFE09D9D78
68132D6C22CA54280748D9C43BBEC0C0112F4EB6D0B4AF65702D033D402D23D0
3250CB08B40CD07A84AE75DEE25A26D732D143D432032D13B5CC40CBF4121835
74DE438F313A7B388AC6F6BDFF9470F60409871D57336B5761719C809D984DA0
CC8B52BC074549D983FBFCF6DC7F3876DEE2628911C88BEA9467EA9317E4C9A3
A3EC06FB26FE0E8DDFA1F12B1220FF32A98DB2181B6567F80F2024286C0CB676
63EC2C4031D09E1DA2FD0D0A8F31C67EC17F0021618425402FC15E45485D74C1
F691188B33E4284C820DC1A20B3D82E438A82255E6D40AB8399918616FB373EC
25A631869459A42C30839D67C7D911D5AA5A75E1326E40833DA9B350AFA39CC4
7FE8B3ED663985F832925A75B1CCC35DBB90494B70D73ED9B8FD4E9223843AE5
6A9A2EDA2E34EE2C34563DAD80A5B4E22C3869255BAFA7634402CB78E1D23A4A
EB28ADA3B48ED23A4AEB28AD0B693D903650DA406903A50D943650DA40694348
1B81B489D2264A9B286DA2B489D2264A9B42DAE4D256299FA6E408077404CE56
F36E851288889DAF4CC82CF53B041829D6DDB40015007501AA001A024C00680A
500330D3D8761B80A583A9963BDE0432F112FBF0D712971571698BCBAAC7B4AB
1E9AC7407B8C20D8C925D1C54E3E767F07A3083B3E8C22A36BD7384AD7AFADAD
AF7D8C416723EBD7596AFDBD8FD7DE6B7DD2825D6167ECFE8316FBC66BAD7418
E6E7D655265DEDBC8059BAB6283A01D9F54FD6195D011EBD1A58D18515DDB7A2
47ACE8112BED4FDA8CB6D14A1BACB457B9151D7A5285151DADE8112BABC05360
88303C1C9BD7C2A0768EDEC4E30ADBF26383D1DD1DF556F0EAB531C081C45C28
6182C42A5EBDAB18EC3D8C7BEA9D97A1C4BBB05F43CCC3BE5BD8EA2BD81A6D6C
CD556C338361CEC7BEB8BFB3C2BB872B231D7BE4268404766B7C56778E7EB5C2
528840A0F102E1DBD54119F11B2B8CADAF7DB4E6AD21D9FB2DAE57BAC60F7F6B
DEA7F770C1AD115C0C1D7B0CACB47C2BB01FEAFC1DEFEFB79FDEC30AC1A07EB5
B8DA3AA8F9344AD609663AA44840C139B05B5084E6CC019A33039A33A1265070
BDAF135C9C62E8ABBE53ABC1D0157FE83A0C7D3518BA2E86AE0743D76FAC4686
AE0F1FBA2E86DEF6ADB4FDA1EBD1A1B7870C5D1F18BADE37F4F690A1EB0343D7
A343D7BB33B1B15DD4ECEAE5EE6275C661B116883701C555C67B74E7CFEB51E4
BDCF6136BB653BFFF97B1897B23D309F4AACBB5EF182515FEB1C17D9C69AEC07
09FBD89DE4A49908A99355F8AC3B2514B0D8F329C705D0DEEE313FD63DD45BD8
B0392E7006468A251CBB8B30A7388844A662DB0DC187EBEFADEDADF981D04520
E860207E1F0DC4EF0F1F085D0442C71C8840E8870F84CE03A18781D00F0C84FE
170D042FDFDD40FCACF2AD0785D51085D5F00BAB1129ACC6B3CAB711966F030B
AB31B47C9BC28AE95B312356CC67956F332CDF265A310F5BBEA79E59BEB5FFB7
F26D44CBB7216A9811D430A3A77C1BC36B987170F9360E53BE8D811A661CB27C
1B0335CC88D630E319E5DB8C966F530CDD0C866EF6946F73F8D0CD83CBB77998
F26D0E0CDD3C64F93607866E46876EFEEF976F43542D03A32EAA9671F8AA65F0
AA658455CB38B06A197F0DE5DB14813031072210E6E10361F240986120CC0303
61FE0503915A381239D1BFC3D8BFDD4B12491CBFF7F9D1BC489F249E24A80A74
9AE0E1F88D42C89652A45BCA9642B580FE85F2039C2B3742B9E4FE383E162852
38106BF451913ED21E6974AECB9FC0D33EF9F3DD1384887EF1BCBFBF1F17209C
39A21C0D387FFA51C08FF78393FD837AF764DFA9975DF79A7F02A70419D713F8
540021E4F1232E3E3A76279D8BD393A71558A3636031F2D4647EE1528E912E8B
F6B2AC084BEA65D91196DCCBCA062C3660CB8AB0E8900ED980AD6887F210E7E3
03B6EC088B0EE9303E602BDAA13CC4F9C4F07125868F2B317C5C89E1E34A0E1F
5772F8B892C3C7951C3E2E69C05636C2A2433A94066C453B9487382F0FD8CA47
587DB60A11569FAD6284D567AB14B094E1315486C750191E4365780CE9F018D2
8362A866617D4E965F9C9E4C06CB137E135D8C0236D9C524C08E763119304D60
FE1BC5C92E46434926F4424939B410177A47BB180D25E3422F9494430B891E7B
891E7B891E7B891E7BC91E7BC91E7BC91E7BC91E7B92D0D3BA180D2525A1174A
CAA10559E8A5BA18EA1DEB62A877BC8BA1DE0981293D7E2A3D7E2A3D7E2A3D7E
D21E3FA9EF67EA54B352AD934EFC3EBEB8DBC38ABC1BDBC3CC37B68FE39371B5
99CB2DC064E00F1531B7826EF4D1994F37FBE8719F9EE9A3277CFA4C1F3D09F4
BC56BB386B080ADE7A1A5B15A7FA0F12CB32457B6399346EBFB6FCA612CC5514
453685260B77946A0E1B0B1B5BE59A86C45A4FD13450338FF2056C8AD8944033
5BB1F2122B31AABD849AA7FB34914DA14983E8E57CB528B1C7C344914D6BB9CB
55F4A766B8122B0E134536BE8DACA9DAC965928AD94ECDA6A99875C9294BA958
6DDE76A5C6F62FF13D4F101EF929CF835150ECAA12F499827EC0A5670A9A4250
7EAAE038BEF4087C5420A9E3D945DB278C624E81E0567D023ED3C43D4F76628C
C55E7EF2EF2737399AE32821807E8628A390E7CB8DED4B2AD6AEEE8B9071B5B9
E8D8B06F3CC3DF95DCC489C0B65A1D150E3B5B7B6C0C3D8AA7E230CF6B04F71D
D9D44413E24A6E09416C532FF07D97501D6F6DC239164DA1740EBBADD6E8671B
DCBCBE8D4DEB237C8D08C2BE33B97E67A48833B9C33A93E3CEE422CEE49EC799
9CEF8CD5EF8C1C71C63AAC331677C68A38633D8F3396EF8CDDEF8C1271C63EAC
333677C68E38633F8F33B6EF4CBEDF99918833F9C33A93E7CEE423CEE49FC799
BCEF4CA1DF9958C499C2619D2970670A11670ACFE34CC177A6D8EFCC68C499E2
619D2972678A11678ACFE34CD177A6D4EF8C1A71A67458674ADC9952C499D2F3
3853D2CE4281DE5AAE59954AF0C951426035D7A9A8A9328BEC989A70B2279D57
F03B97E566B9D64CBAEFAF5EFBE0C30FD6AF4F2DBDFF4F573FF8F843E2B1CBA8
B85B1CEDD8B1A7084E2DC0EDD8684C02D769755E43292719F08C745A879EDEC5
9E3C2661D5F5988C9F5CEC8E7BEC8A20132423BE1411D3E615B8A1149572AD5E
21D1CF365026FA594714277E9FD1CF3A106F6C5B6AEDDD5AB59B28C9AFC12A06
7BA21063ED22858326A15A914E936942CF16A94D6C42CF14699BB409958A70E0
5E23345EA4D7C975388416E997E44B42E184FA35F99ACB7F47BEE3FADF2ADF2A
284F54A2D258917E217D215175136E21AFC33645BC108F67BF15A64FB263453A
45A6B8850EE9C0755A2128FC6B388FEB81C370BFE1E2AFB273E735383DF3C335
D8DA225B844E14E903F280FBF4883C22740AD5CFD5DD6AF7E53BF5D535962CD2
393247A8324DB99573D5BAD5158B47C53CE211458150A0D8347E1B1488A9BE58
92B1225D212B8472997356B91246588974F5983C066FA70938A615C6719A2E39
0B3A656FF0EFA138EC2CD815D5CED62B6AE34E6E143144E0F46F158A4D954CCD
DB0B70994B3876C9511D7BBEAC56CA4B964A4AB1AC55AFC2F58453CE965468E6
A1311032E64121E62C201BDFBCEA70B15DAB04C2BF2E570085C6C0C65453BFCA
2F148A307BEEA2658F5171598C5C6EA13D58A2D0A692F92B5C5A42E75213C51A
EC97BC0D94DA43AF539335A04882E2BD8FA4C6B67BB2605BDD97E3A324F5362F
1168D72338BA4E0247823DEFB1F1DD339D892F71443820414BEEAA0220A94B23
BC6A705DC6957F83BA502ABC16021E0E736513F599DABE857DB4DBA82CBE0FC2
6DD90A5370AFC6E4DD231C5DC12D5B1B6EBDD958E491CE0BEC24644F7E2CE33C
FE41FE41A6747A8E9CC709FA397F702239E5F9B20065A75C7204A838E5EABC00
47002CA1A3DC77FE1405ABDFC48BEC74FAE0AE2F6C92D45C8C17BACF377C031B
A2F7CF389EB5E17A0A6ADF12D0CFC02AB91C06D1A3387E1C118600FFE1B85087
C9E881C7A6F033AFC676E105FC962748C7080DF6647F1F6685D1E74B0B5E527F
13C90CD7F748A0CFE34D52CE5837C0BA581E7C31ABD3C48FAA1E46550FA3AA87
51D545543FE3E01806226A0F5D437D1FA8CE7BC2E192E303D592475B9B2D5C18
5CD74F8C2E1233CB4C48CC13F9890C2EFDF12CC2D2132980BF97BFEFD2BF97BE
1774CC58E199191B7094A7CA4369F4D443717410EF6A4BADEB2D5C842270DD14
4291B15EC22FAE523A26CE0FB384BDDDC4C5CC465BB0B587C3D35EE217FF7C77
6477748FE716FB08B6B9F64824C1BD9A697CDB400F9FEF703D46932E1D90741A
4DBAD19374CD4FBA1126DD08936E844937C2A41BD1584A3F2BE9C6FF5DD2A59F
98740AB5F30CEC89BB07A8112D650DCFE29B3F3589BFE249ECBCBC839FD432FA
946CE2A791C530A199035771264C68264C68264C68264C68E627257453042B9A
CECC5F453A9D97E6F1F6EBA7532141EDED599B7290552887FEDA947EEEDA940F
C8A6949A4B74533973602A67C254CE84A99C095339235229C05190CD7FC6C148
B8E4FEAC62C47AB38AA1AB9660EB8A4CF6D0C3FEE7F3BBAAC7540460FD7A18CD
B5CDD65A34E73322E7E7D92F219F37E41BDDDCDE906E7473FE507E28C39E4FE4
D9197D6A9E011723DBF067E8C6E04086E4FD7637EFB0131948BDD4D8B65FCF5B
9530F5DDDBAE353CF56FFED4CCBF7E70E683CD01532273E0D2D1EE1C9815BB1E
3E07829D366C83C9F9603ACC86D361369C0EB3E174980DA7C3AC980E02644E39
EF0BC401F405124ED9F5A9490079419865137C7FC3C1146C71ACFE59D4F6DA41
7928AD7AABE8C5AD55A670305FC2D62D45671902F90070E79F7FBA218E61439C
3BE44FBF5931FDE61556F2E71F51E13A7A6394E07C3B1F27FE54E4E4D88D5884
8CB392408C1F8E3EEC4AE3045D509F558826FCEDDF406C0E3B316FA3E20A1F51
EBFA0AA308E0CC6821D0376BB72EE5AC3A652D36D2B83DC9E14A7A36AD929370
C9A88D6D388BD40C3798D4E347F129234C66D88AE0FFD36004A7AC8233B2108B
6CFD5436324DB44D7F4FC0CF812DD282B354915E2557E1CAB99DD777F0BF7DC0
2D2D193CB344ED00A31CDB8DF17BB9B8E88DEDB911FCFA3C704896E12826A078
E89AE815170CB8361E398CF63921F163E27CAC5273078ECF72EA624F773052BC
818A51471EB28E0730D81BDFE30111068FB1C97E8390FE53D1071595EA12D99B
8C492C0EE65E8C3C7EC6FD7BC88568F6738D5E6ED02B7EB01E728E3225E52851
C55A4E18ED68FE33052E7784C90181FA849180200584819EF4037A52FA7B52FA
7B520EE8C938A0A7D1FE9E46FB7B1A3DA027F3809E62FD3DC5FA7B8AF5C5171F
9787514CF471F15179C81D811847B9B85A426EB24F17A76EC81D674A63AB9E77
5D92D0F03F43251AB75F4154AA57F49206CD3C3406420640D58AA5D5A01C688D
2DA7D26CD2F857127FC4C091FF19B0371E011A6230E010E10D06F6DC19839D22
43B81C3244748343FC83992BB2B8B8121816F04C49E016642C0111090B794A40
54426D0257430244750248B5472471AA1D1344BCB982427C0318DC415CE60230
259C500D5E78C60B6AA982D589703540A4341316284F4D00790D2C2E0AF215C4
5EB8982330C7CAC3653DA0B2408F43644121D29890B8407472221707D09EFA84
F204A04B4BB8D77025005D08E61481390B782683F68D01239CDB866721F39204
1121901190618B08F0B085818808C8598C5021904802509D12687B12633528A0
4115B4F0646040704CCE6070F377735BC8EAE6EF172FC2072219A09E63101106
4931D483264C2121239220A01A03DA2F14DD2A0BDA3224C21D0F0AA625A0C002
B29D83421896803C0500504B01021400140000000800D796B83EA481BBD90B15
0000403A000001000000000000000000200000000000000074504B0506000000
00010001002F0000002A1500000000
End of ACPI TABLE=DSDT
<-- End of ACPI TABLES SCAN

***************************** CURRENT SENSORS' PROPERTIES

IT8712F at $0290
 -> Temperature sensor diode 1 : Diode
 -> Temperature sensor diode 2 : Thermistor
 -> Temperature sensor diode 3 : Thermistor
 -> FAN1 divisor : 8
 -> FAN2 divisor : 8
 -> FAN3 divisor : 8
 -> PWM 1 mode : Software controlled
 -> PWM 2 mode : Software controlled
 -> PWM 3 mode : Software controlled
 -> PWMOUT clock : 48M
 -> Temperature 1 offset : 0
 -> Temperature 2 offset : 0
 -> Temperature 3 offset : 0
 -> FAN1 mult : 1
 -> FAN1 div : 1
 -> FAN2 mult : 1
 -> FAN2 div : 1
 -> FAN3 mult : 1
 -> FAN3 div : 1
 -> Reverse PWM01 logic : OFF
 -> Reverse PWM02 logic : OFF
 -> Reverse PWM03 logic : OFF
HD1 (41.1GB) at $0000
 -> Temperature 1 offset : 0
HD0 (80.0GB) at $0001
 -> Temperature 1 offset : 0
ACPI at $0000
 -> Temperature 1 offset : 0
<-- End of CURRENT SENSORS' PROPERTIES

***************************** DMI SCAN

DMI structures from SMBIOS ver. 2.3
MBManufacturer : Hewlett-Packard
MBModel : HP System Board
MBVersion : HP P/N
BIOSVendor : Phoenix Technologies, LTD
BIOSVersion : Version 3.08
SysManufacturer : Compaq Presario 061
SysProductName : P8656E-ABA S4000V NA210
SysVersion : 0n31411RE101K2   10
SysSerialNumber : MXP33408QB
Structure   0 - 0000 - fixed len is 16 bytes -> BIOS information
  -> 01 02 00 E0 03 07 90 DE CB 7F 00 00 00 00 37 03
  -> 'Phoenix Technologies, LTD'
  -> ' Version 3.08'
  -> '07/16/2003'
Structure   1 - 0001 - fixed len is 21 bytes -> System information
  -> 01 02 03 04 C0 29 7F D7 C5 D4 D7 11 A2 B7 DD 5B 73 E6 F4 D9 06
  -> 'Compaq Presario 061'
  -> 'P8656E-ABA S4000V NA210'
  -> '0n31411RE101K2   10'
  -> 'MXP33408QB'
Structure   2 - 0002 - fixed len is 4 bytes -> Base board (or module) information
  -> 01 02 03 04
  -> 'Hewlett-Packard'
  -> 'HP System Board'
  -> 'HP P/N'
  -> ' '
Structure   3 - 0003 - fixed len is 13 bytes -> System enclosure or chassis
  -> 01 03 02 03 04 02 02 02 02 00 00 00 00
  -> 'Hewlett-Packard'
  -> ' '
  -> ' '
  -> ' '
Structure   4 - 0004 - fixed len is 31 bytes -> Processor information
  -> 01 03 B2 02 27 0F 00 00 FF FB EB BF 03 80 85 00 DC 05 FA 0B 41 04 0A 00 0B 00 FF FF 04 05 06
  -> 'Socket 478'
  -> 'Intel'
  -> 'Intel Pentium(R) 4'
  -> ' '
  -> ' '
  -> ' '
Structure   5 - 0005 - fixed len is 20 bytes -> Memory controller information
  -> 03 04 03 03 0A 01 00 00 05 02 04 06 00 07 00 08 00 09 00 04
Structure   6 - 0006 - fixed len is 8 bytes -> Memory module information
  -> 01 01 00 00 05 8A 8A 00
  -> 'A0'
Structure   6 - 0007 - fixed len is 8 bytes -> Memory module information
  -> 01 2F 00 00 05 09 09 00
  -> 'A1'
Structure   6 - 0008 - fixed len is 8 bytes -> Memory module information
  -> 01 FF 00 02 00 7F 7F 00
  -> 'A2'
Structure   6 - 0009 - fixed len is 8 bytes -> Memory module information
  -> 01 FF 00 02 00 7F 7F 00
  -> 'A3'
Structure   9 - 0015 - fixed len is 9 bytes -> System slots
  -> 01 06 05 03 04 01 00 02 01
  -> 'PCI0'
Structure   9 - 0016 - fixed len is 9 bytes -> System slots
  -> 01 06 05 04 04 02 00 02 01
  -> 'PCI1'
Structure   9 - 0017 - fixed len is 9 bytes -> System slots
  -> 01 06 05 03 04 03 00 02 01
  -> 'PCI2'
Structure   9 - 0018 - fixed len is 9 bytes -> System slots
  -> 01 06 05 03 04 04 00 02 01
  -> 'PCI3'
Structure   9 - 0019 - fixed len is 9 bytes -> System slots
  -> 01 0F 05 03 04 08 00 02 00
  -> 'AGP'
Structure  13 - 001A - fixed len is 18 bytes -> BIOS language information
  -> 03 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 01
  -> 'n|US|iso8859-1'
  -> 'n|US|iso8859-1'
  -> 'r|CA|iso8859-1'
  -> 'a|JP|unicode'
Structure  16 - 001B - fixed len is 11 bytes -> Physical memory array
  -> 03 03 03 00 00 40 00 FE FF 04 00
Structure  17 - 001C - fixed len is 23 bytes -> Memory device
  -> 1B 00 FE FF 40 00 40 00 00 04 09 00 01 02 0F 80 00 00 00 03 04 05 06
  -> 'A0'
  -> 'Bank0/1'
  -> 'None'
  -> 'None'
  -> 'None'
  -> 'None'
Structure  17 - 001D - fixed len is 23 bytes -> Memory device
  -> 1B 00 FE FF 40 00 40 00 00 02 09 00 01 02 0F 80 00 00 00 03 04 05 06
  -> 'A1'
  -> 'Bank2/3'
  -> 'None'
  -> 'None'
  -> 'None'
  -> 'None'
Structure  17 - 001E - fixed len is 23 bytes -> Memory device
  -> 1B 00 FE FF FF FF FF FF 00 00 09 00 01 02 02 04 00 00 00 03 04 05 06
  -> 'A2'
  -> 'Bank4/5'
  -> 'None'
  -> 'None'
  -> 'None'
  -> 'None'
Structure  17 - 001F - fixed len is 23 bytes -> Memory device
  -> 1B 00 FE FF FF FF FF FF 00 00 09 00 01 02 02 04 00 00 00 03 04 05 06
  -> 'A3'
  -> 'Bank6/7'
  -> 'None'
  -> 'None'
  -> 'None'
  -> 'None'
Structure  19 - 0020 - fixed len is 11 bytes -> Memory array mapped address
  -> 00 00 00 00 FF FF 17 00 1B 00 01
Structure  20 - 0021 - fixed len is 15 bytes -> Memory device mapped address
  -> 00 00 00 00 FF FF 0F 00 1C 00 20 00 01 00 00
Structure  20 - 0022 - fixed len is 15 bytes -> Memory device mapped address
  -> 00 00 10 00 FF FF 17 00 1D 00 20 00 01 00 00
Structure  20 - 0023 - fixed len is 15 bytes -> Memory device mapped address
  -> 00 00 00 00 00 00 00 00 1E 00 20 00 01 00 00
Structure  20 - 0024 - fixed len is 15 bytes -> Memory device mapped address
  -> 00 00 00 00 00 00 00 00 1F 00 20 00 01 00 00
Structure  32 - 0025 - fixed len is 7 bytes -> System boot information
  -> 00 00 00 00 00 00 00
Structure 144 - 0026 - fixed len is 8 bytes -> Unknown (144)
  -> FF FF FF FF FF FF 00 01
  -> 'SiS630E-MAC'
Structure 127 - 0027 - fixed len is 0 bytes -> End of table
  -> 

***************************** EVENTS

0 events defined

***************************** EXTRA UNCATEGORIZED INFO

Tray icon size : 16x16
UPTIME : 0 days 00:26:11
SpeedFan UPTIME : 0 days 00:04:01

***************************** MAIN WINDOW INFO

Win9x:NO  64Bit:NO  GiveIO:YES  SpeedFan:YES
I/O properly initialized
Linked ISA BUS at $0290
Linked SiS651 SMBUS at $1040
Scanning ISA BUS at $0290...
SuperIO Chip=IT8705F
IT8705F found on ISA at $290
Scanning SiSx30 SMBus at $1040...
Found Maxtor 2F040L0 on AdvSMART
Found ST380013A on AdvSMART
Found ACPI temperature
End of detection
Loaded 0 events

***************************** DEBUG INFO

FILE <C:\Program Files\SpeedFan\speedfan.exe> IS TRUSTED
SpeedFan executable is properly signed
CPU Thread Sync Cycles=1
Win9x:NO  64Bit:NO  GiveIO:YES  SpeedFan:YES
SpeedFan.sys ver. 2.000
  -> Can read memory
  -> Can read MSR
  -> Can map memory
  -> Can query thermal
  -> Can eval ACPI
About to do a test on INTEL MSRs...
Found <Intel(R) Pentium(R) 4 CPU 3.06GHz>
CURRENT AFFINITY=0003
CPU#00
  AFFINITY=0001
CPUID[1].EBX=00020809
  TSC=$000003B5CBBF888C
  MSR[$1B]=$00000000FEE00900
  MSR[$EE]=$FFFFFFFFFFFFFFFF
CPU#01
  AFFINITY=0002
CPUID[1].EBX=01020809
  TSC=$000003B5CBD45EE8
  MSR[$1B]=$00000000FEE00800
  MSR[$EE]=$FFFFFFFFFFFFFFFF
CPU#00 MSR[$1B]=$00000000FEE00900
CPU#01 MSR[$1B]=$00000000FEE00800
End of INTEL MSR test
FILE <C:\WINDOWS\System32\speedfan.sys> IS TRUSTED
SpeedFan driver is properly signed
I/O properly initialized
Linked ISA BUS at $0290
Linked PCI
Starting PCI scan...
Enabling SMBus...
SMBus I/O Base Address : $1040
Linked SiS651 SMBUS at $1040
FE01A3014A10C02F
PCI scan done!
Scanning ISA BUS at $0290...
About to check DELL support
PCI scanning is enabled
End of DELL support check
Second pass...
ITE r[$20]=$87 r[$21]=$05 r[$22]=$02 r[$07]=$00 
NEW --> SuperIO chip=ITE IT8705F ($002E)
Checking $002E for ITE (1)...
ITE Registers [$002E] : $87 $05 $02
SuperIO Chip=IT8705F
 --> [$25]=$00
 --> [$26]=$00
 --> [$27]=$00
 --> [$28]=$00
 --> [$29]=$00
 --> [$2A]=$04
 --> LDN0 [$60]=$03F0 [$62]=$0000 [$64]=$0000 (enabled)
 --> LDN1 [$60]=$03F8 [$62]=$0000 [$64]=$0000 (disabled)
 --> LDN2 [$60]=$0000 [$62]=$0000 [$64]=$0000 (disabled)
 --> LDN3 [$60]=$0378 [$62]=$0778 [$64]=$0080 (enabled)
 --> LDN4 [$60]=$0290 [$62]=$0000 [$64]=$0000 (enabled)
 --> LDN5 [$60]=$0800 [$62]=$0000 [$64]=$0000 (disabled)
 --> LDN6 [$60]=$0201 [$62]=$0000 [$64]=$0000 (disabled)
 --> LDN7 [$60]=$0310 [$62]=$0000 [$64]=$0000 (disabled)
 --> LDN8 [$60]=$0300 [$62]=$0000 [$64]=$0000 (disabled)
 --> LDN9 [$60]=$0000 [$62]=$0000 [$64]=$0000 (disabled)
 --> LDNA [$60]=$0000 [$62]=$0000 [$64]=$0000 (disabled)
 --> LDNB [$60]=$0000 [$62]=$0000 [$64]=$0000 (disabled)
IT8705F found on ISA at $290
 -> Temperature sensor diode 1 : Diode
 -> Temperature sensor diode 2 : Thermistor
 -> Temperature sensor diode 3 : Thermistor
 -> FAN1 divisor : 8
 -> FAN2 divisor : 8
 -> FAN3 divisor : 8
 -> PWM 1 mode : Software controlled
 -> PWM 2 mode : ON/OFF
 -> PWM 3 mode : ON/OFF
 -> PWMOUT clock : 48M
 -> Temperature 1 offset : 0
 -> Temperature 2 offset : 0
 -> Temperature 3 offset : 0
 -> FAN1 mult : 1
 -> FAN1 div : 1
 -> FAN2 mult : 1
 -> FAN2 div : 1
 -> FAN3 mult : 1
 -> FAN3 div : 1
 -> Reverse PWM01 logic : OFF
 -> Reverse PWM02 logic : OFF
 -> Reverse PWM03 logic : OFF
SiS5595 DAM Base Address : $8008
DAM Module is DISABLED
Scanning SiSx30 SMBus at $1040...
Something is at address $30
Something is at address $31
Something is at address $50
About to probe Intel QST...
End of Intel QST probing
About to probe Intel FB-DIMM support...
End of Intel FB-DIMM support probing
About to probe TOSHIBA SUPPORT...
End of TOSHIBA SUPPORT probing
About to probe Areca RAID support...
ARECA : interface properly linked
ARECA : 0 Areca RAID controller(s) found
End of Areca RAID probing
About to probe 3ware RAID support...
DLL properly linked
API version is <2.04.00.003>
3ware Controllers found : 0
End of 3ware RAID probing
About to probe SMART (Advanced Methods)...
AdvSMART debug messages start -->
WBEM Locator creation took 0 ms to execute
Server Connect took 16 ms to execute
Find USB Controllers took 108 ms to execute
DeviceID=PCI\VEN_1039&DEV_7001&SUBSYS_18141019&REV_0F\3&61AAA01&0&18
Name=SiS 7001 PCI to USB Open Host Controller
Find USB Controllers' Associators took 94 ms to execute
  DeviceID=USB\ROOT_HUB\4&2078F1EC&0
  Name=USB Root Hub
  DeviceID=USB\VID_046D&PID_C51B\5&13ABC9B4&0&2
  Name=USB Composite Device
  DeviceID=USB\VID_046D&PID_C51B&MI_00\6&2DCDCB66&0&0000
  Name=USB Human Interface Device
  DeviceID=HID\VID_046D&PID_C51B&MI_00\7&380F7688&0&0000
  Name=HID-compliant mouse
  DeviceID=USB\VID_046D&PID_C51B&MI_01\6&2DCDCB66&0&0001
  Name=USB Human Interface Device
  DeviceID=HID\VID_046D&PID_C51B&MI_01\7&204BEA43&0&0000
  Name=HID-compliant device
DeviceID=PCI\VEN_1039&DEV_7001&SUBSYS_18141019&REV_0F\3&61AAA01&0&19
Name=SiS 7001 PCI to USB Open Host Controller
Find USB Controllers' Associators took 61 ms to execute
  DeviceID=USB\ROOT_HUB\4&DBF4147&0
  Name=USB Root Hub
DeviceID=PCI\VEN_1039&DEV_7001&SUBSYS_18141019&REV_0F\3&61AAA01&0&1A
Name=SiS 7001 PCI to USB Open Host Controller
Find USB Controllers' Associators took 62 ms to execute
  DeviceID=USB\ROOT_HUB\4&10D8AFD3&0
  Name=USB Root Hub
DeviceID=PCI\VEN_1039&DEV_7002&SUBSYS_18141019&REV_00\3&61AAA01&0&1B
Name=SiS PCI to USB Enhanced Host Controller
Find USB Controllers' Associators took 62 ms to execute
  DeviceID=USB\ROOT_HUB20\4&5C0D9EF&0
  Name=USB Root Hub
USB Drive Search took 390 ms to execute
Find 1394 Controllers took 32 ms to execute
DeviceID=PCI\VEN_1039&DEV_7007&SUBSYS_18141019&REV_00\3&61AAA01&0&13
Name=OHCI Compliant IEEE 1394 Host Controller
Find 1394 Controllers' Associators took 45 ms to execute
Caption=1394 Net Adapter
ClassGuid={4D36E972-E325-11CE-BFC1-08002BE10318}
ConfigManagerErrorCode=0
ConfigManagerUserConfig=False
CreationClassName=Win32_PnPEntity
Description=1394 Net Adapter
DeviceID=V1394\NIC1394\FF0A1C9F0AE6
Manufacturer=Microsoft
Name=1394 Net Adapter
PNPDeviceID=V1394\NIC1394\FF0A1C9F0AE6
Service=NIC1394
Status=OK
SystemCreationClassName=Win32_ComputerSystem
SystemName=DANIEL-XI85763N
1394 Drive Search took 77 ms to execute
Find Disk Drives took 16 ms to execute
 
BytesPerSector=512
Caption=Maxtor 2F040L0
DeviceID=\\.\PHYSICALDRIVE1
InterfaceType=IDE
MediaLoaded=True
Model=Maxtor 2F040L0
Name=\\.\PHYSICALDRIVE1
Partitions=1
SCSIBus=0
SCSILogicalUnit=0
SCSIPort=0
SCSITargetId=1
Trying Physical access...
Using TSmartHardDiskPhysical
    Identify Sector -->
      000  40 00 FF 3F 37 C8 10 00 00 00 00 00 3F 00 00 00 00 00 00 00 46 31 43 37 57 45 47 45 20 20 20 20 @.ÿ?7È......?.......F1C7WEGE    
      020  20 20 20 20 20 20 20 20 03 00 00 10 39 00 56 41 4D 35 31 4A 4A 30 4D 61 78 74 6F 72 20 32 46 30         ....9.VAM51JJ0Maxtor 2F0
      040  34 30 4C 30 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 10 80 40L0                          .€
      060  00 00 00 2F 00 40 00 02 00 00 07 00 FF 3F 10 00 3F 00 10 FC FB 00 10 01 80 2D C9 04 00 00 07 00 .../.@......ÿ?..?..üû...€-É.....
      080  03 00 78 00 78 00 78 00 78 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ..x.x.x.x.......................
      0A0  FE 00 1E 00 6B 7C 09 7B 03 40 69 7C 01 3A 03 40 7F 20 00 00 00 00 00 00 FE FF 00 6B C0 C0 00 00 þ...k|.{.@i|.:.@ ......þÿ.kÀÀ..
      0C0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................................
      0E0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................................
      100  01 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................................
      120  00 00 00 00 00 00 00 00 00 00 00 00 01 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................................
      140  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................................
      160  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................................
      180  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................................
      1A0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................................
      1C0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................................
      1E0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 A5 72 ..............................¥r
      SMART checksum is $00
      000  10 00 03 27 00 E8 DF 71 17 00 00 00 00 00 04 32 00 FC FC C0 0D 00 00 00 00 00 05 33 00 FD FD 02
      020  00 00 00 00 00 00 06 01 00 FD FD 00 00 00 00 00 00 00 07 0A 00 FD 8B 00 00 00 00 00 00 00 08 27
      040  00 FC EE 44 98 00 00 00 00 00 09 32 00 A4 A4 D2 42 00 00 00 00 00 0A 2B 00 FC ED 01 00 00 00 00
      060  00 00 0B 2B 00 FD FC 00 00 00 00 00 00 00 0C 32 00 F5 F5 9C 0D 00 00 00 00 00 C0 32 00 FA FA E4
      080  0C 00 00 00 00 00 C1 32 00 FB FB D4 2C 00 00 00 00 00 C2 32 00 FD FD 32 00 00 00 00 00 00 C3 0A
      0A0  00 FD FC 10 69 00 00 00 00 00 C4 08 00 FD FD 00 00 00 00 00 00 00 C5 08 00 FB FB 02 00 00 00 00
      0C0  00 00 C6 08 00 FD FD 00 00 00 00 00 00 00 C7 08 00 C7 C7 00 00 00 00 00 00 00 C8 0A 00 FD FD 00
      0E0  00 00 00 00 00 00 C9 0A 00 FD FB 00 00 00 00 00 00 00 CA 0A 00 FD FD 00 00 00 00 00 00 00 CB 0B
      100  00 FD FD 00 00 00 00 00 00 00 CC 0A 00 FD FD 00 00 00 00 00 00 00 CD 0A 00 FD FD 00 00 00 00 00
      120  00 00 CF 2A 00 FC F7 01 00 00 00 00 00 00 D0 2A 00 FD F8 00 00 00 00 00 00 00 D1 24 00 FD FD 00
      140  00 00 00 00 00 00 63 04 00 FD FD 00 00 00 00 00 00 00 64 04 00 FD FD 00 00 00 00 00 00 00 65 04
      160  00 FD FD 00 00 00 00 00 00 00 80 00 ED 04 00 5B 03 00 01 00 02 15 00 00 00 00 00 00 00 00 00 00
      180  00 00 39 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      1A0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 01 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      1C0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      1E0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 05 00 48
  Error reading Smart Log Directory using TSmartHardDiskPhysical
  Reading Summary Smart Error Log because it seems to be supported
    - NOT Reading Summary Smart Error Log because disabled by flag
 
BytesPerSector=512
Caption=ST380013A
DeviceID=\\.\PHYSICALDRIVE0
InterfaceType=IDE
MediaLoaded=True
Model=ST380013A
Name=\\.\PHYSICALDRIVE0
Partitions=1
SCSIBus=0
SCSILogicalUnit=0
SCSIPort=0
SCSITargetId=0
Trying Physical access...
Using TSmartHardDiskPhysical
    Identify Sector -->
      000  5A 0C FF 3F 37 C8 10 00 00 00 00 00 3F 00 00 00 00 00 00 00 35 4A 56 57 54 48 48 38 20 20 20 20 Z.ÿ?7È......?.......5JVWTHH8    
      020  20 20 20 20 20 20 20 20 00 00 00 40 04 00 38 2E 30 31 20 20 20 20 53 54 33 38 30 30 31 33 41 20         ...@..8.01    ST380013A 
      040  20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 10 80                               .€
      060  00 00 00 2F 00 40 00 02 00 02 07 00 FF 3F 10 00 3F 00 10 FC FB 00 10 01 B0 F8 50 09 00 00 07 00 .../.@......ÿ?..?..üû...°øP.....
      080  03 00 78 00 78 00 F0 00 78 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ..x.x.ð.x.......................
      0A0  7E 00 1B 00 6B 34 01 7D 23 58 69 34 01 3C 23 40 3F 20 00 00 00 00 FE FE FE FF 7B 60 00 80 00 00 ~...k4.}#Xi4.<#@? ....þþþÿ{`.€..
      0C0  00 00 00 00 00 00 00 00 B0 F8 50 09 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ........°øP.....................
      0E0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................................
      100  01 00 B0 F8 50 09 B0 F8 50 09 20 20 02 00 B6 42 00 00 8A 00 06 3C 0A 3C 00 00 C6 07 00 01 00 08 ..°øP.°øP.  ..¶B..Š..<.<..Æ.....
      120  F0 10 00 10 02 00 30 00 00 00 00 00 00 00 06 FE 00 00 02 00 00 00 00 00 00 00 00 00 21 00 0B 00 ð.....0........þ............!...
      140  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................................
      160  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................................
      180  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................................
      1A0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................................
      1C0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ................................
      1E0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 A5 52 ..............................¥R
      SMART checksum is $00
      000  0A 00 01 0F 00 47 3F 20 6B F4 0D 00 00 00 03 03 00 63 61 00 00 00 00 00 00 00 04 32 00 64 64 45
      020  00 00 00 00 00 00 05 33 00 64 64 00 00 00 00 00 00 00 07 0F 00 57 3C DE 50 69 23 00 00 00 09 32
      040  00 3B 3B A9 8D 00 00 00 00 00 0A 13 00 64 64 00 00 00 00 00 00 00 0C 32 00 62 62 94 08 00 00 00
      060  00 00 C2 22 00 2B 35 2B 00 00 00 00 00 00 C3 1A 00 47 3E 20 6B F4 0D 00 00 00 C5 12 00 64 64 00
      080  00 00 00 00 00 00 C6 10 00 64 64 00 00 00 00 00 00 00 C7 3E 00 C8 C7 01 00 00 00 00 00 00 C8 00
      0A0  00 64 FD 00 00 00 00 00 00 00 CA 32 00 64 FD 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      0C0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      0E0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      100  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      120  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      140  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      160  00 00 00 00 00 00 00 00 00 00 82 00 AE 01 00 5B 03 00 01 00 01 3A 00 00 00 00 00 00 00 00 00 00
      180  00 00 D3 35 01 00 03 02 01 02 02 02 02 02 01 00 00 00 00 00 00 00 00 01 1C FA F1 02 00 00 00 00
      1A0  00 00 8E B1 59 0D E7 05 00 00 00 00 00 00 00 00 00 00 00 00 1C FA F1 02 00 00 FF FF 00 00 00 00
      1C0  00 00 01 00 00 00 01 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
      1E0  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 BC
  Error reading Smart Log Directory using TSmartHardDiskPhysical
  Reading Summary Smart Error Log because it seems to be supported
    - NOT Reading Summary Smart Error Log because disabled by flag
Disk Objects Creation took 203 ms to execute
AdvSMART debug messages end <--
SMART Hard disks found: 2
Found Maxtor 2F040L0 on AdvSMART
  HD00 -> <\\.\PHYSICALDRIVE1> (Physical) Model: <Maxtor 2F040L0> - Firmware: <VAM51JJ0> - Serial: <F1C7WEGE>
    ATA Revision=7
    AAM:supported (currently enabled)
    APM:supported (currently disabled)
    Power Management:supported (currently enabled)
    SMART:supported (currently enabled)
    48-bit Addressing:unsupported
    Max Queue Depth=0
    NCQ:unknown
    SMART Error Log Reporting:supported
    UDMA0:supported (currently disabled)
    UDMA1:supported (currently disabled)
    UDMA2:supported (currently disabled)
    UDMA3:supported (currently disabled)
    UDMA4:supported (currently disabled)
    UDMA5:supported (currently enabled)
    UDMA6:supported (currently disabled)
SMART Structure Revision : $0010
ID=$03  NAME=Spin Up Time  VALUE=$E8  WORST=$DF  RAW=$000000001771  THRSHLD=$3F  FLAGS=$0027
ID=$04  NAME=Start/Stop Count  VALUE=$FC  WORST=$FC  RAW=$000000000DC0  THRSHLD=$00  FLAGS=$0032
ID=$05  NAME=Reallocated Sector Count  VALUE=$FD  WORST=$FD  RAW=$000000000002  THRSHLD=$3F  FLAGS=$0033
ID=$06  NAME=Read Channel Margin  VALUE=$FD  WORST=$FD  RAW=$000000000000  THRSHLD=$64  FLAGS=$0001
ID=$07  NAME=Seek Error Rate  VALUE=$FD  WORST=$8B  RAW=$000000000000  THRSHLD=$00  FLAGS=$000A
ID=$08  NAME=Seek Time Performance  VALUE=$FC  WORST=$EE  RAW=$000000009844  THRSHLD=$BB  FLAGS=$0027
ID=$09  NAME=Power On Hours Count  VALUE=$A4  WORST=$A4  RAW=$0000000042D2  THRSHLD=$00  FLAGS=$0032
ID=$0A  NAME=Spin Retry Count  VALUE=$FC  WORST=$ED  RAW=$000000000001  THRSHLD=$9D  FLAGS=$002B
ID=$0B  NAME=Calibration Retry Count  VALUE=$FD  WORST=$FC  RAW=$000000000000  THRSHLD=$DF  FLAGS=$002B
ID=$0C  NAME=Power Cycle Count  VALUE=$F5  WORST=$F5  RAW=$000000000D9C  THRSHLD=$00  FLAGS=$0032
ID=$C0  NAME=Power Off Retract Count  VALUE=$FA  WORST=$FA  RAW=$000000000CE4  THRSHLD=$00  FLAGS=$0032
ID=$C1  NAME=Load Cycle Count  VALUE=$FB  WORST=$FB  RAW=$000000002CD4  THRSHLD=$00  FLAGS=$0032
ID=$C2  NAME=Temperature  VALUE=$FD  WORST=$FD  RAW=$000000000032  THRSHLD=$00  FLAGS=$0032
Current HD temperature is 50C
ID=$C3  NAME=Hardware ECC Recovered  VALUE=$FD  WORST=$FC  RAW=$000000006910  THRSHLD=$00  FLAGS=$000A
ID=$C4  NAME=Reallocated Event Count  VALUE=$FD  WORST=$FD  RAW=$000000000000  THRSHLD=$00  FLAGS=$0008
ID=$C5  NAME=Current Pending Sector Count  VALUE=$FB  WORST=$FB  RAW=$000000000002  THRSHLD=$00  FLAGS=$0008
ID=$C6  NAME=Uncorrectable Sector Count  VALUE=$FD  WORST=$FD  RAW=$000000000000  THRSHLD=$00  FLAGS=$0008
ID=$C7  NAME=UltraATA CRC Error Rate  VALUE=$C7  WORST=$C7  RAW=$000000000000  THRSHLD=$00  FLAGS=$0008
ID=$C8  NAME=Write Error Rate  VALUE=$FD  WORST=$FD  RAW=$000000000000  THRSHLD=$00  FLAGS=$000A
ID=$C9  NAME=Soft Read Error Rate  VALUE=$FD  WORST=$FB  RAW=$000000000000  THRSHLD=$00  FLAGS=$000A
ID=$CA  NAME=Data Address Mark Errors  VALUE=$FD  WORST=$FD  RAW=$000000000000  THRSHLD=$00  FLAGS=$000A
ID=$CB  NAME=Run Out Cancel  VALUE=$FD  WORST=$FD  RAW=$000000000000  THRSHLD=$B4  FLAGS=$000B
ID=$CC  NAME=Soft ECC Correction  VALUE=$FD  WORST=$FD  RAW=$000000000000  THRSHLD=$00  FLAGS=$000A
ID=$CD  NAME=Thermal Asperity Rate  VALUE=$FD  WORST=$FD  RAW=$000000000000  THRSHLD=$00  FLAGS=$000A
ID=$CF  NAME=Spin High Current  VALUE=$FC  WORST=$F7  RAW=$000000000001  THRSHLD=$00  FLAGS=$002A
ID=$D0  NAME=Spin Buzz  VALUE=$FD  WORST=$F8  RAW=$000000000000  THRSHLD=$00  FLAGS=$002A
ID=$D1  NAME=Offline Seek Performance  VALUE=$FD  WORST=$FD  RAW=$000000000000  THRSHLD=$00  FLAGS=$0024
ID=$63  NAME=(Unknown Attribute)  VALUE=$FD  WORST=$FD  RAW=$000000000000  THRSHLD=$00  FLAGS=$0004
ID=$64  NAME=(Unknown Attribute)  VALUE=$FD  WORST=$FD  RAW=$000000000000  THRSHLD=$00  FLAGS=$0004
ID=$65  NAME=(Unknown Attribute)  VALUE=$FD  WORST=$FD  RAW=$000000000000  THRSHLD=$00  FLAGS=$0004
Adding drive #0 (Maxtor 2F040L0) found on AdvSMART
Linked AdvSMART
 -> Temperature 1 offset : 0
Found ST380013A on AdvSMART
  HD01 -> <\\.\PHYSICALDRIVE0> (Physical) Model: <ST380013A> - Firmware: <8.01> - Serial: <5JVWTHH8>
    ATA Revision=6
    AAM:unsupported (currently disabled)
    APM:unsupported (currently disabled)
    Power Management:supported (currently enabled)
    SMART:supported (currently enabled)
    48-bit Addressing:supported
    Max Queue Depth=0
    NCQ:unknown
    SMART Error Log Reporting:supported
    UDMA0:supported (currently disabled)
    UDMA1:supported (currently disabled)
    UDMA2:supported (currently disabled)
    UDMA3:supported (currently disabled)
    UDMA4:supported (currently disabled)
    UDMA5:supported (currently enabled)
    UDMA6:unsupported (currently disabled)
SMART Structure Revision : $000A
ID=$01  NAME=Raw Read Error Rate  VALUE=$47  WORST=$3F  RAW=$00000DF46B20  THRSHLD=$06  FLAGS=$000F
ID=$03  NAME=Spin Up Time  VALUE=$63  WORST=$61  RAW=$000000000000  THRSHLD=$00  FLAGS=$0003
ID=$04  NAME=Start/Stop Count  VALUE=$64  WORST=$64  RAW=$000000000045  THRSHLD=$14  FLAGS=$0032
ID=$05  NAME=Reallocated Sector Count  VALUE=$64  WORST=$64  RAW=$000000000000  THRSHLD=$24  FLAGS=$0033
ID=$07  NAME=Seek Error Rate  VALUE=$57  WORST=$3C  RAW=$0000236950DE  THRSHLD=$1E  FLAGS=$000F
ID=$09  NAME=Power On Hours Count  VALUE=$3B  WORST=$3B  RAW=$000000008DA9  THRSHLD=$00  FLAGS=$0032
ID=$0A  NAME=Spin Retry Count  VALUE=$64  WORST=$64  RAW=$000000000000  THRSHLD=$61  FLAGS=$0013
ID=$0C  NAME=Power Cycle Count  VALUE=$62  WORST=$62  RAW=$000000000894  THRSHLD=$14  FLAGS=$0032
ID=$C2  NAME=Temperature  VALUE=$2B  WORST=$35  RAW=$00000000002B  THRSHLD=$00  FLAGS=$0022
Current HD temperature is 43C
ID=$C3  NAME=Hardware ECC Recovered  VALUE=$47  WORST=$3E  RAW=$00000DF46B20  THRSHLD=$00  FLAGS=$001A
ID=$C5  NAME=Current Pending Sector Count  VALUE=$64  WORST=$64  RAW=$000000000000  THRSHLD=$00  FLAGS=$0012
ID=$C6  NAME=Uncorrectable Sector Count  VALUE=$64  WORST=$64  RAW=$000000000000  THRSHLD=$00  FLAGS=$0010
ID=$C7  NAME=UltraATA CRC Error Rate  VALUE=$C8  WORST=$C7  RAW=$000000000001  THRSHLD=$00  FLAGS=$003E
ID=$C8  NAME=Write Error Rate  VALUE=$64  WORST=$FD  RAW=$000000000000  THRSHLD=$00  FLAGS=$0000
ID=$CA  NAME=Data Address Mark Errors  VALUE=$64  WORST=$FD  RAW=$000000000000  THRSHLD=$00  FLAGS=$0032
Adding drive #1 (ST380013A) found on AdvSMART
 -> Temperature 1 offset : 0
End of SMART (Advanced Methods) probing
Version 1.1 03 00000007
SMART Enabled for drive 0
 --> S.M.A.R.T. attributes properly read
 --> S.M.A.R.T. thresholds properly read
Start of DEBUG DATA for drive 0
--> cylinders : 9729
--> tracks per cilinder : 255
--> sectors per track : 63
--> bytes per sector : 512
--> disk size : 80.0
End of DEBUG DATA for drive 0
Found ST380013A Firmware revision <8.01> (80.0GB) Serial <5JVWTHH8>
 --> Drive already linked
Version 1.1 03 00000007
SMART Enabled for drive 1
 --> S.M.A.R.T. attributes properly read
 --> S.M.A.R.T. thresholds properly read
Start of DEBUG DATA for drive 1
--> cylinders : 4998
--> tracks per cilinder : 255
--> sectors per track : 63
--> bytes per sector : 512
--> disk size : 41.1
End of DEBUG DATA for drive 1
Found Maxtor 2F040L0 Firmware revision <VAM51JJ0> (41.1GB) Serial <F1C7WEGE>
 --> Drive already linked
18:50:50.445 About to probe SCSI...
18:50:50.445 ProbeSCSI: before first LogSense
18:50:50.445 ProbeSCSI: before first LogSense
18:50:50.461 End of SCSI probing
About to probe UGURU support...
Motherboard is Hewlett-Packard HP System Board
End of UGURU support probing
About to probe ACPI...
About to scan ACPI devices...
ACPI Devices -->
     ok    : \0000002a : ACPI_HAL\PNP0C08 - *PNP0C08 :  : Microsoft ACPI-Compliant System
     ok    : \00000032 : ACPI\FixedButton - *FixedButton :  : ACPI Fixed Feature Button
  00000001 : \0000002b : ACPI\GenuineIntel_-_x86_Family_15_Model_2 - *GenuineIntel_-_x86_Family_15_Model_2 - ACPI\GenuineIntel_-_x86_Family_15 - *GenuineIntel_-_x86_Family_15 - ACPI\GenuineIntel_-_x86 - *GenuineIntel_-_x86 : ACPI\Processor : Processor
  00000001 : \0000002c : ACPI\GenuineIntel_-_x86_Family_15_Model_2 - *GenuineIntel_-_x86_Family_15_Model_2 - ACPI\GenuineIntel_-_x86_Family_15 - *GenuineIntel_-_x86_Family_15 - ACPI\GenuineIntel_-_x86 - *GenuineIntel_-_x86 : ACPI\Processor : Processor
  00000002 : \00000034 : ACPI\PNP0000 - *PNP0000 :  : Programmable interrupt controller
  00000002 : \00000036 : ACPI\PNP0100 - *PNP0100 :  : System timer
  00000002 : \00000035 : ACPI\PNP0200 - *PNP0200 :  : Direct memory access controller
     ok    : \0000003d : ACPI\PNP0303 - *PNP0303 : *PNP030B : Standard 101/102-Key or Microsoft Natural PS/2 Keyboard
     ok    : \0000003c : ACPI\PNP0401 - *PNP0401 :  : ECP Printer Port
     ok    : \0000003b : ACPI\PNP0501 - *PNP0501 :  : Communications Port
     ok    : \0000003a : ACPI\PNP0700 - *PNP0700 :  : Standard floppy disk controller
  00000002 : \00000038 : ACPI\PNP0800 - *PNP0800 :  : System speaker
  00000001 : \00000030 : ACPI\PNP0A03 - *PNP0A03 :  : PCI bus
     ok    : \00000037 : ACPI\PNP0B00 - *PNP0B00 :  : System CMOS/real time clock
  00000002 : \0000002f : ACPI\PNP0C01 - *PNP0C01 :  : System board
  00000002 : \00000033 : ACPI\PNP0C02 - *PNP0C02 :  : Motherboard resources
  00000002 : \00000039 : ACPI\PNP0C04 - *PNP0C04 :  : Numeric data processor
     ok    : \0000002d : ACPI\PNP0C0C - *PNP0C0C :  : ACPI Power Button
     ok    : \0000002e : ACPI\PNP0C0E - *PNP0C0E :  : ACPI Sleep Button
     ok    : \00000031 : ACPI\ThermalZone - *ThermalZone :  : ACPI Thermal Zone
ACPI Devices <--
End of ACPI devices scanning
About to scan ACPI Thermal Zones...
End of ACPI Thermal Zones scanning
About to explore ACPI...
End of ACPI exploration
Found ACPI temperature
 -> Temperature 1 offset : 0
End of ACPI probing
About to probe ATK0110...
About to scan ACPI devices...
End of ACPI devices scanning
End of ATK0110 probing
About to probe AMD Internal Sensors...
End of AMD Internal Sensors probing
About to probe INTEL Internal Sensors...
End of INTEL Internal Sensors probing
About to probe NVIDIA ControlPanel Sensors...
End of NVIDIA ControlPanel Sensors probing
End of detection
LoadFineTunedAssociations: TempFileName=<C:\DOCUME~1\Daniel\LOCALS~1\Temp\SFC6A.tmp>
LoadFineTunedAssociations: CfgFileName=<Hewlett-Packard HP System Board HP P%2FN Compaq Presario 061 P8656E-ABA S4000V NA210>
LoadFineTunedAssociations: CFG <Hewlett-Packard HP System Board HP P%2FN Compaq Presario 061 P8656E-ABA S4000V NA210> not found in ZIP
LoadFineTunedAssociations: CfgFileName2=<Hewlett-Packard HP System Board  Compaq Presario 061 P8656E-ABA S4000V NA210>
LoadFineTunedAssociations: Error 3 while extracting CFG (Hewlett-Packard HP System Board  Compaq Presario 061 P8656E-ABA S4000V NA210) from ZIP
Loaded 0 events
Preparing report...